IRremoteESP8266

IRSanyoAc88 Member List

This is the complete list of members for IRSanyoAc88, including all inherited members.

_ | IRSanyoAc88 | private
_irsend | IRSanyoAc88 | private
begin(void) | IRSanyoAc88 |
calcChecksum(const uint8_t state[], const uint16_t length=kSanyoAcStateLength) | IRSanyoAc88 | privatestatic
calibrate(void) | IRSanyoAc88 | inline
checksum(void) | IRSanyoAc88 | private
convertFan(const stdAc::fanspeed_t speed) | IRSanyoAc88 | static
convertMode(const stdAc::opmode_t mode) | IRSanyoAc88 | static
getClock(void) const | IRSanyoAc88 |
getFan(void) const | IRSanyoAc88 |
getFilter(void) const | IRSanyoAc88 |
getMode(void) const | IRSanyoAc88 |
getPower(void) const | IRSanyoAc88 |
getRaw(void) | IRSanyoAc88 |
getSleep(void) const | IRSanyoAc88 |
getSwingV(void) const | IRSanyoAc88 |
getTemp(void) const | IRSanyoAc88 |
getTurbo(void) const | IRSanyoAc88 |
IRSanyoAc88(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRSanyoAc88 | explicit
off(void) | IRSanyoAc88 |
on(void) | IRSanyoAc88 |
send(const uint16_t repeat=kSanyoAc88MinRepeat) | IRSanyoAc88 |
setClock(const uint16_t mins_since_midnight) | IRSanyoAc88 |
setFan(const uint8_t speed) | IRSanyoAc88 |
setFilter(const bool on) | IRSanyoAc88 |
setMode(const uint8_t mode) | IRSanyoAc88 |
setPower(const bool on) | IRSanyoAc88 |
setRaw(const uint8_t newState[]) | IRSanyoAc88 |
setSleep(const bool on) | IRSanyoAc88 |
setSwingV(const bool on) | IRSanyoAc88 |
setTemp(const uint8_t degrees) | IRSanyoAc88 |
setTurbo(const bool on) | IRSanyoAc88 |
stateReset(void) | IRSanyoAc88 |
toCommon(void) const | IRSanyoAc88 |
toCommonFanSpeed(const uint8_t speed) | IRSanyoAc88 | static
toCommonMode(const uint8_t mode) | IRSanyoAc88 | static
toString(void) const | IRSanyoAc88 |