IRremoteESP8266

IRVoltas Member List

This is the complete list of members for IRVoltas, including all inherited members.

_ | IRVoltas | private
_irsend | IRVoltas | private
_model | IRVoltas | private
begin() | IRVoltas |
calcChecksum(const uint8_t state[], const uint16_t length=kVoltasStateLength) | IRVoltas | privatestatic
calibrate(void) | IRVoltas | inline
checksum(void) | IRVoltas | private
convertFan(const stdAc::fanspeed_t speed) | IRVoltas |
convertMode(const stdAc::opmode_t mode) | IRVoltas |
getEcono(void) const | IRVoltas |
getFan(void) | IRVoltas |
getLight(void) const | IRVoltas |
getMode(void) | IRVoltas |
getModel(const bool raw=false) const | IRVoltas |
getOffTime(void) const | IRVoltas |
getOnTime(void) const | IRVoltas |
getPower(void) const | IRVoltas |
getRaw(void) | IRVoltas |
getSleep(void) const | IRVoltas |
getSwingH(void) const | IRVoltas |
getSwingHChange(void) const | IRVoltas |
getSwingV(void) const | IRVoltas |
getTemp(void) | IRVoltas |
getTurbo(void) const | IRVoltas |
getWifi(void) const | IRVoltas |
IRVoltas(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRVoltas | explicit
off(void) | IRVoltas |
on(void) | IRVoltas |
send(const uint16_t repeat=kNoRepeat) | IRVoltas |
setEcono(const bool on) | IRVoltas |
setFan(const uint8_t speed) | IRVoltas |
setLight(const bool on) | IRVoltas |
setMode(const uint8_t mode) | IRVoltas |
setModel(const voltas_ac_remote_model_t model) | IRVoltas |
setOffTime(const uint16_t nr_of_mins) | IRVoltas |
setOnTime(const uint16_t nr_of_mins) | IRVoltas |
setPower(const bool on) | IRVoltas |
setRaw(const uint8_t new_code[]) | IRVoltas |
setSleep(const bool on) | IRVoltas |
setSwingH(const bool on) | IRVoltas |
setSwingHChange(const bool on) | IRVoltas |
setSwingV(const bool on) | IRVoltas |
setTemp(const uint8_t temp) | IRVoltas |
setTurbo(const bool on) | IRVoltas |
setWifi(const bool on) | IRVoltas |
stateReset() | IRVoltas |
toCommon(const stdAc::state_t *prev=NULL) | IRVoltas |
toCommonFanSpeed(const uint8_t speed) | IRVoltas | static
toCommonMode(const uint8_t mode) | IRVoltas | static
toString(void) | IRVoltas |
validChecksum(const uint8_t state[], const uint16_t length=kVoltasStateLength) | IRVoltas | static