IRremoteESP8266

Public Member Functions | Static Public Member Functions | Private Member Functions | Private Attributes | List of all members
IRTecoAc Class Reference

Class for handling detailed Teco A/C messages. More...

`#include <ir_Teco.h>`

Collaboration diagram for IRTecoAc:
[legend]

## Public Member Functions
| IRTecoAc (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | stateReset (void)
| Reset the internal state of the emulation. More...
void | send (const uint16_t repeat=kTecoDefaultRepeat)
| Send the current internal state as an IR message. More...
int8_t | calibrate (void)
| Run the calibration to calculate uSec timing offsets for this platform. More...
void | begin (void)
| Set up hardware to be able to send a message. More...
void | on (void)
| Set the requested power state of the A/C to on. More...
void | off (void)
| Set the requested power state of the A/C to off. More...
void | setPower (const bool on)
| Change the power setting. More...
bool | getPower (void) const
| Get the value of the current power setting. More...
void | setTemp (const uint8_t temp)
| Set the temperature. More...
uint8_t | getTemp (void) const
| Get the current temperature setting. More...
void | setFan (const uint8_t fan)
| Set the speed of the fan. More...
uint8_t | getFan (void) const
| Get the current fan speed setting. More...
void | setMode (const uint8_t mode)
| Set the operating mode of the A/C. More...
uint8_t | getMode (void) const
| Get the operating mode setting of the A/C. More...
void | setSwing (const bool on)
| Set the (vertical) swing setting of the A/C. More...
bool | getSwing (void) const
| Get the (vertical) swing setting of the A/C. More...
void | setSleep (const bool on)
| Set the Sleep setting of the A/C. More...
bool | getSleep (void) const
| Get the Sleep setting of the A/C. More...
void | setLight (const bool on)
| Set the Light (LED/Display) setting of the A/C. More...
bool | getLight (void) const
| Get the Light (LED/Display) setting of the A/C. More...
void | setHumid (const bool on)
| Set the Humid setting of the A/C. More...
bool | getHumid (void) const
| Get the Humid setting of the A/C. More...
void | setSave (const bool on)
| Set the Save setting of the A/C. More...
bool | getSave (void) const
| Get the Save setting of the A/C. More...
uint16_t | getTimer (void) const
| Get the timer time for when the A/C unit will switch power state. More...
void | setTimer (const uint16_t mins)
| Set the timer for when the A/C unit will switch power state. More...
uint64_t | getRaw (void) const
| Get a copy of the internal state/code for this protocol. More...
void | setRaw (const uint64_t new_code)
| Set the internal state from a valid code for this protocol. More...
stdAc::state_t | toCommon (void) const
| Convert the current internal state into its stdAc::state_t equivalent. More...
String | toString (void) const
| Convert the current internal state into a human readable string. More...

## Static Public Member Functions
static uint8_t | convertMode (const stdAc::opmode_t mode)
| Convert a stdAc::opmode_t enum into its native mode. More...
static uint8_t | convertFan (const stdAc::fanspeed_t speed)
| Convert a stdAc::fanspeed_t enum into it's native speed. More...
static stdAc::opmode_t | toCommonMode (const uint8_t mode)
| Convert a native mode into its stdAc equivalent. More...
static stdAc::fanspeed_t | toCommonFanSpeed (const uint8_t speed)
| Convert a native fan speed into its stdAc equivalent. More...

## Private Member Functions
bool | getTimerEnabled (void) const
| Is the timer function enabled? More...

## Private Attributes
IRsend | _irsend
| Instance of the IR send class. More...
TecoProtocol | _

## Detailed Description

Class for handling detailed Teco A/C messages.

## Constructor & Destructor Documentation

## ◆ IRTecoAc()

IRTecoAc::IRTecoAc | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |
| explicit

Class constructor.

Parameters

  [in] | pin | GPIO to be used when sending.
  [in] | inverted | Is the output signal to be inverted?
  [in] | use_modulation | Is frequency modulation to be used?

## Member Function Documentation

## ◆ begin()

void IRTecoAc::begin | ( | void |  | ) |

Set up hardware to be able to send a message.

## ◆ calibrate()

int8_t IRTecoAc::calibrate | ( | void |  | ) |
| inline

Run the calibration to calculate uSec timing offsets for this platform.

Returns
  The uSec timing offset needed per modulation of the IR Led.

Note
  This will produce a 65ms IR signal pulse at 38kHz. Only ever needs to be run once per object instantiation, if at all.

## ◆ convertFan()

uint8_t IRTecoAc::convertFan | ( | const stdAc::fanspeed_t | speed | ) |
| static

Convert a stdAc::fanspeed_t enum into it's native speed.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ convertMode()

uint8_t IRTecoAc::convertMode | ( | const stdAc::opmode_t | mode | ) |
| static

Convert a stdAc::opmode_t enum into its native mode.

Parameters

  [in] | mode | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ getFan()

uint8_t IRTecoAc::getFan | ( | void |  | ) | const

Get the current fan speed setting.

Returns
  The current fan speed/mode.

## ◆ getHumid()

bool IRTecoAc::getHumid | ( | void |  | ) | const

Get the Humid setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getLight()

bool IRTecoAc::getLight | ( | void |  | ) | const

Get the Light (LED/Display) setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getMode()

uint8_t IRTecoAc::getMode | ( | void |  | ) | const

Get the operating mode setting of the A/C.

Returns
  The current operating mode setting.

## ◆ getPower()

bool IRTecoAc::getPower | ( | void |  | ) | const

Get the value of the current power setting.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getRaw()

uint64_t IRTecoAc::getRaw | ( | void |  | ) | const

Get a copy of the internal state/code for this protocol.

Returns
  A code for this protocol based on the current internal state.

## ◆ getSave()

bool IRTecoAc::getSave | ( | void |  | ) | const

Get the Save setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getSleep()

bool IRTecoAc::getSleep | ( | void |  | ) | const

Get the Sleep setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getSwing()

bool IRTecoAc::getSwing | ( | void |  | ) | const

Get the (vertical) swing setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getTemp()

uint8_t IRTecoAc::getTemp | ( | void |  | ) | const

Get the current temperature setting.

Returns
  The current setting for temp. in degrees celsius.

## ◆ getTimer()

uint16_t IRTecoAc::getTimer | ( | void |  | ) | const

Get the timer time for when the A/C unit will switch power state.

Returns
  The number of minutes left on the timer. `0` means off.

## ◆ getTimerEnabled()

bool IRTecoAc::getTimerEnabled | ( | void |  | ) | const
| inlineprivate

Is the timer function enabled?

Returns
  true, the setting is on. false, the setting is off.

## ◆ off()

void IRTecoAc::off | ( | void |  | ) |

Set the requested power state of the A/C to off.

## ◆ on()

void IRTecoAc::on | ( | void |  | ) |

Set the requested power state of the A/C to on.

## ◆ send()

void IRTecoAc::send | ( | const uint16_t | repeat = `kTecoDefaultRepeat` | ) |

Send the current internal state as an IR message.

Parameters

  [in] | repeat | Nr. of times the message will be repeated.

## ◆ setFan()

void IRTecoAc::setFan | ( | const uint8_t | speed | ) |

Set the speed of the fan.

Parameters

  [in] | speed | The desired setting.

## ◆ setHumid()

void IRTecoAc::setHumid | ( | const bool | on | ) |

Set the Humid setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setLight()

void IRTecoAc::setLight | ( | const bool | on | ) |

Set the Light (LED/Display) setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setMode()

void IRTecoAc::setMode | ( | const uint8_t | mode | ) |

Set the operating mode of the A/C.

Parameters

  [in] | mode | The desired operating mode.

## ◆ setPower()

void IRTecoAc::setPower | ( | const bool | on | ) |

Change the power setting.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setRaw()

void IRTecoAc::setRaw | ( | const uint64_t | new_code | ) |

Set the internal state from a valid code for this protocol.

Parameters

  [in] | new_code | A valid code for this protocol.

## ◆ setSave()

void IRTecoAc::setSave | ( | const bool | on | ) |

Set the Save setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setSleep()

void IRTecoAc::setSleep | ( | const bool | on | ) |

Set the Sleep setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setSwing()

void IRTecoAc::setSwing | ( | const bool | on | ) |

Set the (vertical) swing setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setTemp()

void IRTecoAc::setTemp | ( | const uint8_t | temp | ) |

Set the temperature.

Parameters

  [in] | temp | The temperature in degrees celsius.

## ◆ setTimer()

void IRTecoAc::setTimer | ( | const uint16_t | nr_mins | ) |

Set the timer for when the A/C unit will switch power state.

Parameters

  [in] | nr_mins | Number of minutes before power state change. `0` will clear the timer. Max is 24 hrs.

Note
  Time is stored internally in increments of 30 mins.

## ◆ stateReset()

void IRTecoAc::stateReset | ( | void |  | ) |

Reset the internal state of the emulation.

Note
  Mode:auto, Power:Off, fan:auto, temp:16, swing:off, sleep:off

## ◆ toCommon()

stdAc::state_t IRTecoAc::toCommon | ( | void |  | ) | const

Convert the current internal state into its stdAc::state_t equivalent.

Returns
  The stdAc equivalent of the native settings.

## ◆ toCommonFanSpeed()

stdAc::fanspeed_t IRTecoAc::toCommonFanSpeed | ( | const uint8_t | speed | ) |
| static

Convert a native fan speed into its stdAc equivalent.

Parameters

  [in] | speed | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toCommonMode()

stdAc::opmode_t IRTecoAc::toCommonMode | ( | const uint8_t | mode | ) |
| static

Convert a native mode into its stdAc equivalent.

Parameters

  [in] | mode | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toString()

String IRTecoAc::toString | ( | void |  | ) | const

Convert the current internal state into a human readable string.

Returns
  A human readable string.

## Member Data Documentation

## ◆ _

TecoProtocol IRTecoAc::_
| private

## ◆ _irsend

IRsend IRTecoAc::_irsend
| private

Instance of the IR send class.

The documentation for this class was generated from the following files:

- src/ir_Teco.h
- src/ir_Teco.cpp