IRremoteESP8266

IRArgoAC Member List

This is the complete list of members for IRArgoAC, including all inherited members.

_ | IRArgoACBase< ArgoProtocol > | protected
_checksum(ArgoProtocol *state) | IRArgoACBase< ArgoProtocol > | protected
_checksum(ArgoProtocol *state) | IRArgoACBase< ArgoProtocol > | related
_checksum(ArgoProtocolWREM3 *state) | IRArgoACBase< ArgoProtocol > | related
_irsend | IRArgoACBase< ArgoProtocol > | protected
_length | IRArgoACBase< ArgoProtocol > | protected
_messageType | IRArgoACBase< ArgoProtocol > | protected
_stateReset(ArgoProtocol *state, argoIrMessageType_t messageType=argoIrMessageType_t::AC_CONTROL) | IRArgoACBase< ArgoProtocol > | protected
_stateReset(ArgoProtocol *state, argoIrMessageType_t) | IRArgoACBase< ArgoProtocol > | related
_stateReset(ArgoProtocolWREM3 *state, argoIrMessageType_t messageType) | IRArgoACBase< ArgoProtocol > | related
begin(void) | IRArgoACBase< ArgoProtocol > |
calcChecksum(const uint8_t state[], const uint16_t length) | IRArgoACBase< ArgoProtocol > | protectedstatic
calibrate(void) | IRArgoACBase< ArgoProtocol > | inline
checksum(void) | IRArgoACBase< ArgoProtocol > | protected
convertCommand(const stdAc::ac_command_t command) | IRArgoACBase< ArgoProtocol > | static
convertFan(const stdAc::fanspeed_t speed) | IRArgoACBase< ArgoProtocol > | static
convertMode(const stdAc::opmode_t mode) | IRArgoACBase< ArgoProtocol > | static
convertSwingV(const stdAc::swingv_t position) | IRArgoACBase< ArgoProtocol > | static
getChecksum(const uint8_t state[], const uint16_t length) | IRArgoACBase< ArgoProtocol > | protectedstatic
getFan(void) const | IRArgoAC |
getFanEx(void) const | IRArgoACBase< ArgoProtocol > |
getFlap(void) const | IRArgoAC |
getFlapEx(void) const | IRArgoACBase< ArgoProtocol > |
getiFeel(void) const | IRArgoACBase< ArgoProtocol > |
getMax(void) const | IRArgoACBase< ArgoProtocol > |
getMessageType(void) const | IRArgoACBase< ArgoProtocol > |
getMessageType(const uint8_t state[], const uint16_t length) | IRArgoACBase< ArgoProtocol > | static
getMode(void) const | IRArgoAC |
getModeEx(void) const | IRArgoACBase< ArgoProtocol > |
getNight(void) const | IRArgoACBase< ArgoProtocol > |
getPower(void) const | IRArgoACBase< ArgoProtocol > |
getRaw(void) | IRArgoACBase< ArgoProtocol > |
getRawByteLength() const | IRArgoACBase< ArgoProtocol > |
getRawByteLength(const ArgoProtocol &raw, argoIrMessageType_t messageTypeHint=argoIrMessageType_t::AC_CONTROL) | IRArgoACBase< ArgoProtocol > | protectedstatic
getRawByteLength(const ArgoProtocol &, argoIrMessageType_t messageType) | IRArgoACBase< ArgoProtocol > | related
getRawByteLength(const ArgoProtocolWREM3 &raw, argoIrMessageType_t) | IRArgoACBase< ArgoProtocol > | related
getSensorTemp(void) const | IRArgoACBase< ArgoProtocol > |
getStateLengthForIrMsgType(argoIrMessageType_t type) | IRArgoACBase< ArgoProtocol > | static
getTemp(void) const | IRArgoACBase< ArgoProtocol > |
IRArgoAC(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRArgoAC | explicit
IRArgoACBase(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRArgoACBase< ArgoProtocol > | explicit
off(void) | IRArgoACBase< ArgoProtocol > |
on(void) | IRArgoACBase< ArgoProtocol > |
send(const uint16_t repeat=kArgoDefaultRepeat) | IRArgoACBase< ArgoProtocol > |
sendSensorTemp(const uint8_t degrees, const uint16_t repeat=kArgoDefaultRepeat) | IRArgoAC |
setFan(const uint8_t fan) | IRArgoAC |
IRArgoACBase< ArgoProtocol >::setFan(const argoFan_t fan) | IRArgoACBase< ArgoProtocol > |
setFanEx(const argoFan_t fan) | IRArgoACBase< ArgoProtocol > | inline
setFlap(const uint8_t flap) | IRArgoAC |
IRArgoACBase< ArgoProtocol >::setFlap(const argoFlap_t flap) | IRArgoACBase< ArgoProtocol > |
setFlapEx(const argoFlap_t flap) | IRArgoACBase< ArgoProtocol > | inline
setiFeel(const bool on) | IRArgoACBase< ArgoProtocol > |
setMax(const bool on) | IRArgoACBase< ArgoProtocol > |
setMessageType(const argoIrMessageType_t msgType) | IRArgoACBase< ArgoProtocol > |
setMode(const uint8_t mode) | IRArgoAC |
IRArgoACBase< ArgoProtocol >::setMode(const argoMode_t mode) | IRArgoACBase< ArgoProtocol > |
setModeEx(const argoMode_t mode) | IRArgoACBase< ArgoProtocol > | inline
setNight(const bool on) | IRArgoACBase< ArgoProtocol > |
setPower(const bool on) | IRArgoACBase< ArgoProtocol > |
setRaw(const uint8_t state[], const uint16_t length) | IRArgoACBase< ArgoProtocol > |
setSensorTemp(const uint8_t degrees) | IRArgoACBase< ArgoProtocol > |
setTemp(const uint8_t degrees) | IRArgoACBase< ArgoProtocol > |
stateReset(argoIrMessageType_t messageType=argoIrMessageType_t::AC_CONTROL) | IRArgoACBase< ArgoProtocol > | protected
toCommon(void) const | IRArgoAC |
toCommonCommand(const argoIrMessageType_t command) | IRArgoACBase< ArgoProtocol > | protectedstatic
toCommonFanSpeed(const argoFan_t speed) | IRArgoACBase< ArgoProtocol > | protectedstatic
toCommonMode(const argoMode_t mode) | IRArgoACBase< ArgoProtocol > | protectedstatic
toCommonSwingV(const uint8_t position) | IRArgoACBase< ArgoProtocol > | protectedstatic
toString(void) const | IRArgoAC |
validChecksum(const uint8_t state[], const uint16_t length) | IRArgoACBase< ArgoProtocol > | static