IRremoteESP8266

IRGreeAC Member List

This is the complete list of members for IRGreeAC, including all inherited members.

_ | IRGreeAC | private
_irsend | IRGreeAC | private
_model | IRGreeAC | private
begin(void) | IRGreeAC |
calibrate(void) | IRGreeAC | inline
checksum(const uint16_t length=kGreeStateLength) | IRGreeAC | private
convertFan(const stdAc::fanspeed_t speed) | IRGreeAC | static
convertMode(const stdAc::opmode_t mode) | IRGreeAC | static
convertSwingH(const stdAc::swingh_t swingh) | IRGreeAC | static
convertSwingV(const stdAc::swingv_t swingv) | IRGreeAC | static
fixup(void) | IRGreeAC | private
getDisplayTempSource(void) const | IRGreeAC |
getEcono(void) const | IRGreeAC |
getFan(void) const | IRGreeAC |
getIFeel(void) const | IRGreeAC |
getLight(void) const | IRGreeAC |
getMode(void) const | IRGreeAC |
getModel(void) const | IRGreeAC |
getPower(void) const | IRGreeAC |
getRaw(void) | IRGreeAC |
getSleep(void) const | IRGreeAC |
getSwingHorizontal(void) const | IRGreeAC |
getSwingVerticalAuto(void) const | IRGreeAC |
getSwingVerticalPosition(void) const | IRGreeAC |
getTemp(void) const | IRGreeAC |
getTimer(void) const | IRGreeAC |
getTimerEnabled(void) const | IRGreeAC | private
getTurbo(void) const | IRGreeAC |
getUseFahrenheit(void) const | IRGreeAC |
getWiFi(void) const | IRGreeAC |
getXFan(void) const | IRGreeAC |
IRGreeAC(const uint16_t pin, const gree_ac_remote_model_t model=gree_ac_remote_model_t::YAW1F, const bool inverted=false, const bool use_modulation=true) | IRGreeAC | explicit
off(void) | IRGreeAC |
on(void) | IRGreeAC |
send(const uint16_t repeat=kGreeDefaultRepeat) | IRGreeAC |
setDisplayTempSource(const uint8_t mode) | IRGreeAC |
setEcono(const bool on) | IRGreeAC |
setFan(const uint8_t speed) | IRGreeAC |
setIFeel(const bool on) | IRGreeAC |
setLight(const bool on) | IRGreeAC |
setMode(const uint8_t new_mode) | IRGreeAC |
setModel(const gree_ac_remote_model_t model) | IRGreeAC |
setPower(const bool on) | IRGreeAC |
setRaw(const uint8_t new_code[]) | IRGreeAC |
setSleep(const bool on) | IRGreeAC |
setSwingHorizontal(const uint8_t position) | IRGreeAC |
setSwingVertical(const bool automatic, const uint8_t position) | IRGreeAC |
setTemp(const uint8_t temp, const bool fahrenheit=false) | IRGreeAC |
setTimer(const uint16_t minutes) | IRGreeAC |
setTimerEnabled(const bool on) | IRGreeAC | private
setTurbo(const bool on) | IRGreeAC |
setUseFahrenheit(const bool on) | IRGreeAC |
setWiFi(const bool on) | IRGreeAC |
setXFan(const bool on) | IRGreeAC |
stateReset(void) | IRGreeAC |
toCommon(void) | IRGreeAC |
toCommonFanSpeed(const uint8_t speed) | IRGreeAC | static
toCommonMode(const uint8_t mode) | IRGreeAC | static
toCommonSwingH(const uint8_t pos) | IRGreeAC | static
toCommonSwingV(const uint8_t pos) | IRGreeAC | static
toString(void) | IRGreeAC |
validChecksum(const uint8_t state[], const uint16_t length=kGreeStateLength) | IRGreeAC | static