IRremoteESP8266

IRMitsubishiHeavy88Ac Member List

This is the complete list of members for IRMitsubishiHeavy88Ac, including all inherited members.

_ | IRMitsubishiHeavy88Ac | private
_irsend | IRMitsubishiHeavy88Ac | private
begin(void) | IRMitsubishiHeavy88Ac |
calibrate(void) | IRMitsubishiHeavy88Ac | inline
checksum(void) | IRMitsubishiHeavy88Ac | private
checkZjsSig(const uint8_t *state) | IRMitsubishiHeavy88Ac | static
convertFan(const stdAc::fanspeed_t speed) | IRMitsubishiHeavy88Ac | static
convertMode(const stdAc::opmode_t mode) | IRMitsubishiHeavy88Ac | static
convertSwingH(const stdAc::swingh_t position) | IRMitsubishiHeavy88Ac | static
convertSwingV(const stdAc::swingv_t position) | IRMitsubishiHeavy88Ac | static
get3D(void) const | IRMitsubishiHeavy88Ac |
getClean(void) const | IRMitsubishiHeavy88Ac |
getEcono(void) const | IRMitsubishiHeavy88Ac |
getFan(void) const | IRMitsubishiHeavy88Ac |
getMode(void) const | IRMitsubishiHeavy88Ac |
getPower(void) const | IRMitsubishiHeavy88Ac |
getRaw(void) | IRMitsubishiHeavy88Ac |
getSwingHorizontal(void) const | IRMitsubishiHeavy88Ac |
getSwingVertical(void) const | IRMitsubishiHeavy88Ac |
getTemp(void) const | IRMitsubishiHeavy88Ac |
getTurbo(void) const | IRMitsubishiHeavy88Ac |
IRMitsubishiHeavy88Ac(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRMitsubishiHeavy88Ac | explicit
off(void) | IRMitsubishiHeavy88Ac |
on(void) | IRMitsubishiHeavy88Ac |
send(const uint16_t repeat=kMitsubishiHeavy88MinRepeat) | IRMitsubishiHeavy88Ac |
set3D(const bool on) | IRMitsubishiHeavy88Ac |
setClean(const bool on) | IRMitsubishiHeavy88Ac |
setEcono(const bool on) | IRMitsubishiHeavy88Ac |
setFan(const uint8_t fan) | IRMitsubishiHeavy88Ac |
setMode(const uint8_t mode) | IRMitsubishiHeavy88Ac |
setPower(const bool on) | IRMitsubishiHeavy88Ac |
setRaw(const uint8_t *data) | IRMitsubishiHeavy88Ac |
setSwingHorizontal(const uint8_t pos) | IRMitsubishiHeavy88Ac |
setSwingVertical(const uint8_t pos) | IRMitsubishiHeavy88Ac |
setTemp(const uint8_t temp) | IRMitsubishiHeavy88Ac |
setTurbo(const bool on) | IRMitsubishiHeavy88Ac |
stateReset(void) | IRMitsubishiHeavy88Ac |
toCommon(void) const | IRMitsubishiHeavy88Ac |
toCommonFanSpeed(const uint8_t speed) | IRMitsubishiHeavy88Ac | static
toCommonSwingH(const uint8_t pos) | IRMitsubishiHeavy88Ac | static
toCommonSwingV(const uint8_t pos) | IRMitsubishiHeavy88Ac | static
toString(void) const | IRMitsubishiHeavy88Ac |
validChecksum(const uint8_t *state, const uint16_t length=kMitsubishiHeavy88StateLength) | IRMitsubishiHeavy88Ac | static