IRremoteESP8266

Public Member Functions | Static Public Member Functions | Private Member Functions | Static Private Member Functions | Private Attributes | List of all members
IRDaikin128 Class Reference

Class for handling detailed Daikin 128-bit A/C messages. More...

`#include <ir_Daikin.h>`

Collaboration diagram for IRDaikin128:
[legend]

## Public Member Functions
| IRDaikin128 (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | send (const uint16_t repeat=kDaikin128DefaultRepeat)
| Send the current internal state as an IR message. More...
int8_t | calibrate (void)
| Run the calibration to calculate uSec timing offsets for this platform. More...
void | begin (void)
| Set up hardware to be able to send a message. More...
void | setPowerToggle (const bool toggle)
| Set the Power toggle setting of the A/C. More...
bool | getPowerToggle (void) const
| Get the Power toggle setting of the A/C. More...
void | setTemp (const uint8_t temp)
| Set the temperature. More...
uint8_t | getTemp (void) const
| Get the current temperature setting. More...
void | setFan (const uint8_t fan)
| Set the speed of the fan. More...
uint8_t | getFan (void) const
| Get the current fan speed setting. More...
uint8_t | getMode (void) const
| Get the operating mode setting of the A/C. More...
void | setMode (const uint8_t mode)
| Set the operating mode of the A/C. More...
void | setSwingVertical (const bool on)
| Set the Vertical Swing mode of the A/C. More...
bool | getSwingVertical (void) const
| Get the Vertical Swing mode of the A/C. More...
bool | getSleep (void) const
| Get the Sleep mode of the A/C. More...
void | setSleep (const bool on)
| Set the Sleep mode of the A/C. More...
bool | getQuiet (void) const
| Get the Quiet mode status of the A/C. More...
void | setQuiet (const bool on)
| Set the Quiet mode of the A/C. More...
bool | getPowerful (void) const
| Get the Powerful (Turbo) mode of the A/C. More...
void | setPowerful (const bool on)
| Set the Powerful (Turbo) mode of the A/C. More...
void | setEcono (const bool on)
| Set the Economy mode of the A/C. More...
bool | getEcono (void) const
| Get the Economical mode of the A/C. More...
void | setOnTimer (const uint16_t mins_since_midnight)
| Set the On Timer time for the A/C unit. More...
uint16_t | getOnTimer (void) const
| Get the On Timer time to be sent to the A/C unit. More...
bool | getOnTimerEnabled (void) const
| Get the enable status of the On Timer. More...
void | setOnTimerEnabled (const bool on)
| Set the enable status of the On Timer. More...
void | setOffTimer (const uint16_t mins_since_midnight)
| Set the Off Timer time for the A/C unit. More...
uint16_t | getOffTimer (void) const
| Get the Off Timer time to be sent to the A/C unit. More...
bool | getOffTimerEnabled (void) const
| Get the enable status of the Off Timer. More...
void | setOffTimerEnabled (const bool on)
| Set the enable status of the Off Timer. More...
void | setClock (const uint16_t mins_since_midnight)
| Set the clock on the A/C unit. More...
uint16_t | getClock (void) const
| Get the clock time to be sent to the A/C unit. More...
void | setLightToggle (const uint8_t unit_type)
| Set the Light toggle setting of the A/C. More...
uint8_t | getLightToggle (void) const
| Get the Light toggle setting of the A/C. More...
uint8_t * | getRaw (void)
| Get a PTR to the internal state/code for this protocol. More...
void | setRaw (const uint8_t new_code[])
| Set the internal state from a valid code for this protocol. More...
stdAc::state_t | toCommon (const stdAc::state_t *prev=NULL) const
| Convert the current internal state into its stdAc::state_t equivalent. More...
String | toString (void) const
| Convert the current internal state into a human readable string. More...

## Static Public Member Functions
static bool | validChecksum (uint8_t state[])
| Verify the checksum is valid for a given state. More...
static uint8_t | convertMode (const stdAc::opmode_t mode)
| Convert a stdAc::opmode_t enum into its native mode. More...
static uint8_t | convertFan (const stdAc::fanspeed_t speed)
| Convert a stdAc::fanspeed_t enum into it's native speed. More...
static stdAc::opmode_t | toCommonMode (const uint8_t mode)
| Convert a native mode into its stdAc equivalent. More...
static stdAc::fanspeed_t | toCommonFanSpeed (const uint8_t speed)
| Convert a native fan speed into its stdAc equivalent. More...

## Private Member Functions
void | stateReset (void)
| Reset the internal state to a fixed known good state. More...
void | checksum (void)
| Calculate and set the checksum values for the internal state. More...

## Static Private Member Functions
static uint8_t | calcFirstChecksum (const uint8_t state[])
static uint8_t | calcSecondChecksum (const uint8_t state[])

## Private Attributes
IRsend | _irsend
| instance of the IR send class More...
Daikin128Protocol | _

## Detailed Description

Class for handling detailed Daikin 128-bit A/C messages.

Note
  Code by crankyoldgit. Analysis by Daniel Vena

## Constructor & Destructor Documentation

## ◆ IRDaikin128()

IRDaikin128::IRDaikin128 | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |
| explicit

Class constructor.

Parameters

  [in] | pin | GPIO to be used when sending.
  [in] | inverted | Is the output signal to be inverted?
  [in] | use_modulation | Is frequency modulation to be used?

## Member Function Documentation

## ◆ begin()

void IRDaikin128::begin | ( | void |  | ) |

Set up hardware to be able to send a message.

## ◆ calcFirstChecksum()

uint8_t IRDaikin128::calcFirstChecksum | ( | const uint8_t | state[] | ) |
| static private

## ◆ calcSecondChecksum()

uint8_t IRDaikin128::calcSecondChecksum | ( | const uint8_t | state[] | ) |
| static private

## ◆ calibrate()

int8_t IRDaikin128::calibrate | ( | void |  | ) |
| inline

Run the calibration to calculate uSec timing offsets for this platform.

Returns
  The uSec timing offset needed per modulation of the IR Led.

Note
  This will produce a 65ms IR signal pulse at 38kHz. Only ever needs to be run once per object instantiation, if at all.

## ◆ checksum()

void IRDaikin128::checksum | ( | void |  | ) |
| private

Calculate and set the checksum values for the internal state.

## ◆ convertFan()

uint8_t IRDaikin128::convertFan | ( | const stdAc::fanspeed_t | speed | ) |
| static

Convert a stdAc::fanspeed_t enum into it's native speed.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ convertMode()

uint8_t IRDaikin128::convertMode | ( | const stdAc::opmode_t | mode | ) |
| static

Convert a stdAc::opmode_t enum into its native mode.

Parameters

  [in] | mode | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ getClock()

uint16_t IRDaikin128::getClock | ( | void |  | ) | const

Get the clock time to be sent to the A/C unit.

Returns
  The number of minutes past midnight.

## ◆ getEcono()

bool IRDaikin128::getEcono | ( | void |  | ) | const

Get the Economical mode of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getFan()

uint8_t IRDaikin128::getFan | ( | void |  | ) | const

Get the current fan speed setting.

Returns
  The current fan speed.

## ◆ getLightToggle()

uint8_t IRDaikin128::getLightToggle | ( | void |  | ) | const

Get the Light toggle setting of the A/C.

Returns
  The current operating mode setting.

## ◆ getMode()

uint8_t IRDaikin128::getMode | ( | void |  | ) | const

Get the operating mode setting of the A/C.

Returns
  The current operating mode setting.

## ◆ getOffTimer()

uint16_t IRDaikin128::getOffTimer | ( | void |  | ) | const

Get the Off Timer time to be sent to the A/C unit.

Returns
  The number of minutes past midnight.

## ◆ getOffTimerEnabled()

bool IRDaikin128::getOffTimerEnabled | ( | void |  | ) | const

Get the enable status of the Off Timer.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getOnTimer()

uint16_t IRDaikin128::getOnTimer | ( | void |  | ) | const

Get the On Timer time to be sent to the A/C unit.

Returns
  The number of minutes past midnight.

## ◆ getOnTimerEnabled()

bool IRDaikin128::getOnTimerEnabled | ( | void |  | ) | const

Get the enable status of the On Timer.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getPowerful()

bool IRDaikin128::getPowerful | ( | void |  | ) | const

Get the Powerful (Turbo) mode of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getPowerToggle()

bool IRDaikin128::getPowerToggle | ( | void |  | ) | const

Get the Power toggle setting of the A/C.

Returns
  The current operating mode setting.

## ◆ getQuiet()

bool IRDaikin128::getQuiet | ( | void |  | ) | const

Get the Quiet mode status of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getRaw()

uint8_t * IRDaikin128::getRaw | ( | void |  | ) |

Get a PTR to the internal state/code for this protocol.

Returns
  PTR to a code for this protocol based on the current internal state.

## ◆ getSleep()

bool IRDaikin128::getSleep | ( | void |  | ) | const

Get the Sleep mode of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getSwingVertical()

bool IRDaikin128::getSwingVertical | ( | void |  | ) | const

Get the Vertical Swing mode of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getTemp()

uint8_t IRDaikin128::getTemp | ( | void |  | ) | const

Get the current temperature setting.

Returns
  The current setting for temp. in degrees celsius.

## ◆ send()

void IRDaikin128::send | ( | const uint16_t | repeat = `kDaikin128DefaultRepeat` | ) |

Send the current internal state as an IR message.

Parameters

  [in] | repeat | Nr. of times the message will be repeated.

## ◆ setClock()

void IRDaikin128::setClock | ( | const uint16_t | mins_since_midnight | ) |

Set the clock on the A/C unit.

Parameters

  [in] | mins_since_midnight | Nr. of minutes past midnight.

## ◆ setEcono()

void IRDaikin128::setEcono | ( | const bool | on | ) |

Set the Economy mode of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setFan()

void IRDaikin128::setFan | ( | const uint8_t | speed | ) |

Set the speed of the fan.

Parameters

  [in] | speed | The desired setting.

## ◆ setLightToggle()

void IRDaikin128::setLightToggle | ( | const uint8_t | unit | ) |

Set the Light toggle setting of the A/C.

Parameters

  [in] | unit | Device to show the LED (Light) Display info about.

Note
  0 is off.

## ◆ setMode()

void IRDaikin128::setMode | ( | const uint8_t | mode | ) |

Set the operating mode of the A/C.

Parameters

  [in] | mode | The desired operating mode.

## ◆ setOffTimer()

void IRDaikin128::setOffTimer | ( | const uint16_t | mins_since_midnight | ) |

Set the Off Timer time for the A/C unit.

Parameters

  [in] | mins_since_midnight | Nr. of minutes past midnight.

## ◆ setOffTimerEnabled()

void IRDaikin128::setOffTimerEnabled | ( | const bool | on | ) |

Set the enable status of the Off Timer.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setOnTimer()

void IRDaikin128::setOnTimer | ( | const uint16_t | mins_since_midnight | ) |

Set the On Timer time for the A/C unit.

Parameters

  [in] | mins_since_midnight | Nr. of minutes past midnight.

## ◆ setOnTimerEnabled()

void IRDaikin128::setOnTimerEnabled | ( | const bool | on | ) |

Set the enable status of the On Timer.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setPowerful()

void IRDaikin128::setPowerful | ( | const bool | on | ) |

Set the Powerful (Turbo) mode of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setPowerToggle()

void IRDaikin128::setPowerToggle | ( | const bool | toggle | ) |

Set the Power toggle setting of the A/C.

Parameters

  [in] | toggle | true, the setting is on. false, the setting is off.

## ◆ setQuiet()

void IRDaikin128::setQuiet | ( | const bool | on | ) |

Set the Quiet mode of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setRaw()

void IRDaikin128::setRaw | ( | const uint8_t | new_code[] | ) |

Set the internal state from a valid code for this protocol.

Parameters

  [in] | new_code | A valid code for this protocol.

## ◆ setSleep()

void IRDaikin128::setSleep | ( | const bool | on | ) |

Set the Sleep mode of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setSwingVertical()

void IRDaikin128::setSwingVertical | ( | const bool | on | ) |

Set the Vertical Swing mode of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setTemp()

void IRDaikin128::setTemp | ( | const uint8_t | temp | ) |

Set the temperature.

Parameters

  [in] | temp | The temperature in degrees celsius.

## ◆ stateReset()

void IRDaikin128::stateReset | ( | void |  | ) |
| private

Reset the internal state to a fixed known good state.

## ◆ toCommon()

stdAc::state_t IRDaikin128::toCommon | ( | const stdAc::state_t * | prev = `NULL` | ) | const

Convert the current internal state into its stdAc::state_t equivalent.

Parameters

  [in] | prev | Ptr to a previous state.

Returns
  The stdAc equivalent of the native settings.

## ◆ toCommonFanSpeed()

stdAc::fanspeed_t IRDaikin128::toCommonFanSpeed | ( | const uint8_t | speed | ) |
| static

Convert a native fan speed into its stdAc equivalent.

Parameters

  [in] | speed | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toCommonMode()

stdAc::opmode_t IRDaikin128::toCommonMode | ( | const uint8_t | mode | ) |
| static

Convert a native mode into its stdAc equivalent.

Parameters

  [in] | mode | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toString()

String IRDaikin128::toString | ( | void |  | ) | const

Convert the current internal state into a human readable string.

Returns
  A human readable string.

## ◆ validChecksum()

bool IRDaikin128::validChecksum | ( | uint8_t | state[] | ) |
| static

Verify the checksum is valid for a given state.

Parameters

  [in] | state | The array to verify the checksum of.

Returns
  true, if the state has a valid checksum. Otherwise, false.

## Member Data Documentation

## ◆ _

Daikin128Protocol IRDaikin128::_
| private

## ◆ _irsend

IRsend IRDaikin128::_irsend
| private

instance of the IR send class

The documentation for this class was generated from the following files:

- src/ir_Daikin.h
- src/ir_Daikin.cpp