IRremoteESP8266

IRArgoAC_WREM3 Member List

This is the complete list of members for IRArgoAC_WREM3, including all inherited members.

_ | IRArgoACBase< ArgoProtocolWREM3 > | protected
_checksum(ArgoProtocolWREM3 *state) | IRArgoACBase< ArgoProtocolWREM3 > | protected
_checksum(ArgoProtocol *state) | IRArgoACBase< ArgoProtocolWREM3 > | related
_checksum(ArgoProtocolWREM3 *state) | IRArgoACBase< ArgoProtocolWREM3 > | related
_irsend | IRArgoACBase< ArgoProtocolWREM3 > | protected
_length | IRArgoACBase< ArgoProtocolWREM3 > | protected
_messageType | IRArgoACBase< ArgoProtocolWREM3 > | protected
_stateReset(ArgoProtocolWREM3 *state, argoIrMessageType_t messageType=argoIrMessageType_t::AC_CONTROL) | IRArgoACBase< ArgoProtocolWREM3 > | protected
_stateReset(ArgoProtocol *state, argoIrMessageType_t) | IRArgoACBase< ArgoProtocolWREM3 > | related
_stateReset(ArgoProtocolWREM3 *state, argoIrMessageType_t messageType) | IRArgoACBase< ArgoProtocolWREM3 > | related
begin(void) | IRArgoACBase< ArgoProtocolWREM3 > |
calcChecksum(const uint8_t state[], const uint16_t length) | IRArgoACBase< ArgoProtocolWREM3 > | protected static
calibrate(void) | IRArgoACBase< ArgoProtocolWREM3 > | inline
checksum(void) | IRArgoACBase< ArgoProtocolWREM3 > | protected
convertCommand(const stdAc::ac_command_t command) | IRArgoACBase< ArgoProtocolWREM3 > | static
convertFan(const stdAc::fanspeed_t speed) | IRArgoACBase< ArgoProtocolWREM3 > | static
convertMode(const stdAc::opmode_t mode) | IRArgoACBase< ArgoProtocolWREM3 > | static
convertSwingV(const stdAc::swingv_t position) | IRArgoACBase< ArgoProtocolWREM3 > | static
getChannel(void) const | IRArgoAC_WREM3 |
getChecksum(const uint8_t state[], const uint16_t length) | IRArgoACBase< ArgoProtocolWREM3 > | protected static
getConfigEntry(void) const | IRArgoAC_WREM3 |
getCurrentDayOfWeek(void) const | IRArgoAC_WREM3 |
getCurrentTimeMinutes(void) const | IRArgoAC_WREM3 |
getDelayTimerMinutes(void) const | IRArgoAC_WREM3 |
getEco(void) const | IRArgoAC_WREM3 |
getFan(void) const | IRArgoAC_WREM3 |
getFanEx(void) const | IRArgoACBase< ArgoProtocolWREM3 > |
getFilter(void) const | IRArgoAC_WREM3 |
getFlap(void) const | IRArgoAC_WREM3 |
getFlapEx(void) const | IRArgoACBase< ArgoProtocolWREM3 > |
getiFeel(void) const | IRArgoACBase< ArgoProtocolWREM3 > |
getLight(void) const | IRArgoAC_WREM3 |
getMax(void) const | IRArgoACBase< ArgoProtocolWREM3 > |
getMessageType(const ArgoProtocolWREM3 &raw) | IRArgoAC_WREM3 | static
IRArgoACBase< ArgoProtocolWREM3 >::getMessageType(void) const | IRArgoACBase< ArgoProtocolWREM3 > |
IRArgoACBase< ArgoProtocolWREM3 >::getMessageType(const uint8_t state[], const uint16_t length) | IRArgoACBase< ArgoProtocolWREM3 > | static
getMode(void) const | IRArgoAC_WREM3 |
getModeEx(void) const | IRArgoACBase< ArgoProtocolWREM3 > |
getModel(void) const | IRArgoAC_WREM3 |
getNight(void) const | IRArgoACBase< ArgoProtocolWREM3 > |
getPower(void) const | IRArgoACBase< ArgoProtocolWREM3 > |
getRaw(void) | IRArgoACBase< ArgoProtocolWREM3 > |
getRawByteLength() const | IRArgoACBase< ArgoProtocolWREM3 > |
getRawByteLength(const ArgoProtocolWREM3 &raw, argoIrMessageType_t messageTypeHint=argoIrMessageType_t::AC_CONTROL) | IRArgoACBase< ArgoProtocolWREM3 > | protected static
getRawByteLength(const ArgoProtocol &, argoIrMessageType_t messageType) | IRArgoACBase< ArgoProtocolWREM3 > | related
getRawByteLength(const ArgoProtocolWREM3 &raw, argoIrMessageType_t) | IRArgoACBase< ArgoProtocolWREM3 > | related
getScheduleTimerActiveDays(void) const | IRArgoAC_WREM3 |
getScheduleTimerStartMinutes(void) const | IRArgoAC_WREM3 |
getScheduleTimerStopMinutes(void) const | IRArgoAC_WREM3 |
getSensorTemp(void) const | IRArgoACBase< ArgoProtocolWREM3 > |
getStateLengthForIrMsgType(argoIrMessageType_t type) | IRArgoACBase< ArgoProtocolWREM3 > | static
getTemp(void) const | IRArgoACBase< ArgoProtocolWREM3 > |
getTimerActiveDaysBitmap(void) const | IRArgoAC_WREM3 |
getTimerType(void) const | IRArgoAC_WREM3 |
hasValidPreamble(const uint8_t state[], const uint16_t length) | IRArgoAC_WREM3 | static
IRArgoAC_WREM3(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRArgoAC_WREM3 | explicit
IRArgoACBase(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRArgoACBase< ArgoProtocolWREM3 > | explicit
isValidWrem3Message(const uint8_t state[], const uint16_t nbits, bool verifyChecksum=true) | IRArgoAC_WREM3 | static
off(void) | IRArgoACBase< ArgoProtocolWREM3 > |
on(void) | IRArgoACBase< ArgoProtocolWREM3 > |
send(const uint16_t repeat=kArgoDefaultRepeat) | IRArgoACBase< ArgoProtocolWREM3 > |
sendSensorTemp(const uint8_t degrees, const uint16_t repeat=kArgoDefaultRepeat) | IRArgoAC_WREM3 |
setChannel(const uint8_t channel) | IRArgoAC_WREM3 |
setConfigEntry(const uint8_t paramId, const uint8_t value) | IRArgoAC_WREM3 |
setCurrentDayOfWeek(argoWeekday dayOfWeek) | IRArgoAC_WREM3 |
setCurrentTimeMinutes(uint16_t currentTimeMinutes) | IRArgoAC_WREM3 |
setDelayTimerMinutes(const uint16_t delayMinutes) | IRArgoAC_WREM3 |
setEco(const bool on) | IRArgoAC_WREM3 |
setFan(const argoFan_t fan) | IRArgoACBase< ArgoProtocolWREM3 > |
setFanEx(const argoFan_t fan) | IRArgoACBase< ArgoProtocolWREM3 > | inline
setFilter(const bool on) | IRArgoAC_WREM3 |
setFlap(const argoFlap_t flap) | IRArgoACBase< ArgoProtocolWREM3 > |
setFlapEx(const argoFlap_t flap) | IRArgoACBase< ArgoProtocolWREM3 > | inline
setiFeel(const bool on) | IRArgoACBase< ArgoProtocolWREM3 > |
setLight(const bool on) | IRArgoAC_WREM3 |
setMax(const bool on) | IRArgoACBase< ArgoProtocolWREM3 > |
setMessageType(const argoIrMessageType_t msgType) | IRArgoACBase< ArgoProtocolWREM3 > |
setMode(const argoMode_t mode) | IRArgoACBase< ArgoProtocolWREM3 > |
setModeEx(const argoMode_t mode) | IRArgoACBase< ArgoProtocolWREM3 > | inline
setNight(const bool on) | IRArgoACBase< ArgoProtocolWREM3 > |
setPower(const bool on) | IRArgoACBase< ArgoProtocolWREM3 > |
setRaw(const uint8_t state[], const uint16_t length) | IRArgoACBase< ArgoProtocolWREM3 > |
setScheduleTimerActiveDays(const std::set< argoWeekday > &days) | IRArgoAC_WREM3 |
setScheduleTimerStartMinutes(const uint16_t startTimeMinutes) | IRArgoAC_WREM3 |
setScheduleTimerStopMinutes(const uint16_t stopTimeMinutes) | IRArgoAC_WREM3 |
setSensorTemp(const uint8_t degrees) | IRArgoACBase< ArgoProtocolWREM3 > |
setTemp(const uint8_t degrees) | IRArgoACBase< ArgoProtocolWREM3 > |
setTimerType(const argoTimerType_t timerType) | IRArgoAC_WREM3 |
stateReset(argoIrMessageType_t messageType=argoIrMessageType_t::AC_CONTROL) | IRArgoACBase< ArgoProtocolWREM3 > | protected
toCommon(void) const | IRArgoAC_WREM3 |
toCommonCommand(const argoIrMessageType_t command) | IRArgoACBase< ArgoProtocolWREM3 > | protected static
toCommonFanSpeed(const argoFan_t speed) | IRArgoACBase< ArgoProtocolWREM3 > | protected static
toCommonMode(const argoMode_t mode) | IRArgoACBase< ArgoProtocolWREM3 > | protected static
toCommonSwingV(const uint8_t position) | IRArgoACBase< ArgoProtocolWREM3 > | protected static
toString(void) const | IRArgoAC_WREM3 |
validChecksum(const uint8_t state[], const uint16_t length) | IRArgoACBase< ArgoProtocolWREM3 > | static