IRremoteESP8266

Classes | Variables
ir_York.h File Reference

Support for the York AC protocol (remote GRYLH2A) More...

Go to the source code of this file.

## Classes
union | YorkProtocol
| Native representation of a York A/C message. More...
class | IRYorkAc
| Class for handling detailed York A/C messages. More...

## Variables
const uint8_t | kYorkKnownGoodState [kYorkStateLength]
const uint8_t | kYorkMinTemp = 18
const uint8_t | kYorkMaxTemp = 32
const uint8_t | kYorkFanLow = 1
const uint8_t | kYorkFanMedium = 2
const uint8_t | kYorkFanHigh = 3
const uint8_t | kYorkFanAuto = 8
const uint8_t | kYorkHeat = 1
const uint8_t | kYorkCool = 2
const uint8_t | kYorkDry = 3
const uint8_t | kYorkFan = 4
const uint8_t | kYorkAuto = 8

## Detailed Description

Support for the York AC protocol (remote GRYLH2A)

## Variable Documentation

## ◆ kYorkAuto

const uint8_t kYorkAuto = 8

## ◆ kYorkCool

const uint8_t kYorkCool = 2

## ◆ kYorkDry

const uint8_t kYorkDry = 3

## ◆ kYorkFan

const uint8_t kYorkFan = 4

## ◆ kYorkFanAuto

const uint8_t kYorkFanAuto = 8

## ◆ kYorkFanHigh

const uint8_t kYorkFanHigh = 3

## ◆ kYorkFanLow

const uint8_t kYorkFanLow = 1

## ◆ kYorkFanMedium

const uint8_t kYorkFanMedium = 2

## ◆ kYorkHeat

const uint8_t kYorkHeat = 1

## ◆ kYorkKnownGoodState

const uint8_t kYorkKnownGoodState[kYorkStateLength]

Initial value:
= {
0x08, 0x10, 0x07, 0x02, 0x40, 0x08,
0x03, 0x18, 0x01, 0x60, 0x00, 0x00, 0x00, 0x00,
0xEC,
0xF5, 0xF2}

## ◆ kYorkMaxTemp

const uint8_t kYorkMaxTemp = 32

## ◆ kYorkMinTemp

const uint8_t kYorkMinTemp = 18