IRremoteESP8266

IRMitsubishiAC Member List

This is the complete list of members for IRMitsubishiAC, including all inherited members.

_ | IRMitsubishiAC | private
_irsend | IRMitsubishiAC | private
begin(void) | IRMitsubishiAC |
calculateChecksum(const uint8_t *data) | IRMitsubishiAC | private static
calibrate(void) | IRMitsubishiAC | inline
checksum(void) | IRMitsubishiAC | private
convertFan(const stdAc::fanspeed_t speed) | IRMitsubishiAC | static
convertMode(const stdAc::opmode_t mode) | IRMitsubishiAC | static
convertSwingH(const stdAc::swingh_t position) | IRMitsubishiAC | static
convertSwingV(const stdAc::swingv_t position) | IRMitsubishiAC | static
getAbsenseDetect(void) const | IRMitsubishiAC |
getClock(void) const | IRMitsubishiAC |
getDirectIndirect(void) const | IRMitsubishiAC |
getEcocool(void) const | IRMitsubishiAC |
getFan(void) const | IRMitsubishiAC |
getISave10C(void) const | IRMitsubishiAC |
getISee(void) const | IRMitsubishiAC |
getMode(void) const | IRMitsubishiAC |
getNaturalFlow(void) const | IRMitsubishiAC |
getPower(void) const | IRMitsubishiAC |
getRaw(void) | IRMitsubishiAC |
getStartClock(void) const | IRMitsubishiAC |
getStopClock(void) const | IRMitsubishiAC |
getTemp(void) const | IRMitsubishiAC |
getTimer(void) const | IRMitsubishiAC |
getVane(void) const | IRMitsubishiAC |
getVaneLeft(void) const | IRMitsubishiAC |
getWeeklyTimerEnabled(void) const | IRMitsubishiAC |
getWideVane(void) const | IRMitsubishiAC |
IRMitsubishiAC(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRMitsubishiAC | explicit
off(void) | IRMitsubishiAC |
on(void) | IRMitsubishiAC |
send(const uint16_t repeat=kMitsubishiACMinRepeat) | IRMitsubishiAC |
setAbsenseDetect(const bool state) | IRMitsubishiAC |
setClock(const uint8_t clock) | IRMitsubishiAC |
setDirectIndirect(const uint8_t position) | IRMitsubishiAC |
setEcocool(const bool state) | IRMitsubishiAC |
setFan(const uint8_t speed) | IRMitsubishiAC |
setISave10C(const bool state) | IRMitsubishiAC |
setISee(const bool state) | IRMitsubishiAC |
setMode(const uint8_t mode) | IRMitsubishiAC |
setNaturalFlow(const bool state) | IRMitsubishiAC |
setPower(const bool on) | IRMitsubishiAC |
setRaw(const uint8_t *data) | IRMitsubishiAC |
setStartClock(const uint8_t clock) | IRMitsubishiAC |
setStopClock(const uint8_t clock) | IRMitsubishiAC |
setTemp(const float degrees) | IRMitsubishiAC |
setTimer(const uint8_t timer) | IRMitsubishiAC |
setVane(const uint8_t position) | IRMitsubishiAC |
setVaneLeft(const uint8_t position) | IRMitsubishiAC |
setWeeklyTimerEnabled(const bool on) | IRMitsubishiAC |
setWideVane(const uint8_t position) | IRMitsubishiAC |
stateReset(void) | IRMitsubishiAC |
toCommon(void) const | IRMitsubishiAC |
toCommonFanSpeed(const uint8_t speed) | IRMitsubishiAC | static
toCommonMode(const uint8_t mode) | IRMitsubishiAC | static
toCommonSwingH(const uint8_t pos) | IRMitsubishiAC | static
toCommonSwingV(const uint8_t pos) | IRMitsubishiAC | static
toString(void) const | IRMitsubishiAC |
validChecksum(const uint8_t *data) | IRMitsubishiAC | static