IRremoteESP8266

Public Attributes | List of all members
TrotecProtocol Union Reference

Native representation of a Trotec A/C message. More...

`#include <ir_Trotec.h>`

## Public Attributes
uint8_t | raw [kTrotecStateLength]
| Remote state in IR code form. More...
struct {
uint8_t Intro1:8
uint8_t Intro2:8
uint8_t Mode:2
uint8_t __pad0__:1
uint8_t Power:1
uint8_t Fan:2
uint8_t __pad1__:2
uint8_t Temp:4
uint8_t __pad2__:3
uint8_t Sleep:1
uint8_t __pad3__:8
uint8_t __pad4__:6
uint8_t Timer:1
uint8_t __pad5__:1
uint8_t Hours:8
uint8_t __pad6__:8
uint8_t Sum:8
}; |

## Detailed Description

Native representation of a Trotec A/C message.

## Member Data Documentation

## ◆ @122

struct { ... }

## ◆ __pad0__

uint8_t TrotecProtocol::__pad0__

## ◆ __pad1__

uint8_t TrotecProtocol::__pad1__

## ◆ __pad2__

uint8_t TrotecProtocol::__pad2__

## ◆ __pad3__

uint8_t TrotecProtocol::__pad3__

## ◆ __pad4__

uint8_t TrotecProtocol::__pad4__

## ◆ __pad5__

uint8_t TrotecProtocol::__pad5__

## ◆ __pad6__

uint8_t TrotecProtocol::__pad6__

## ◆ Fan

uint8_t TrotecProtocol::Fan

## ◆ Hours

uint8_t TrotecProtocol::Hours

## ◆ Intro1

uint8_t TrotecProtocol::Intro1

## ◆ Intro2

uint8_t TrotecProtocol::Intro2

## ◆ Mode

uint8_t TrotecProtocol::Mode

## ◆ Power

uint8_t TrotecProtocol::Power

## ◆ raw

uint8_t TrotecProtocol::raw[kTrotecStateLength]

Remote state in IR code form.

## ◆ Sleep

uint8_t TrotecProtocol::Sleep

## ◆ Sum

uint8_t TrotecProtocol::Sum

## ◆ Temp

uint8_t TrotecProtocol::Temp

## ◆ Timer

uint8_t TrotecProtocol::Timer

The documentation for this union was generated from the following file:

- src/ir_Trotec.h