IRremoteESP8266

Variables
ir_Gree.cpp File Reference

Support for Gree A/C protocols. More...

## Variables
const uint16_t | kGreeHdrMark = 9000
const uint16_t | kGreeHdrSpace = 4500
| See #684 & real example in unit tests. More...
const uint16_t | kGreeBitMark = 620
const uint16_t | kGreeOneSpace = 1600
const uint16_t | kGreeZeroSpace = 540
const uint16_t | kGreeMsgSpace = 19980
| See #1508, #386, & Kelvinator. More...
const uint8_t | kGreeBlockFooter = 0b010
const uint8_t | kGreeBlockFooterBits = 3

## Detailed Description

Support for Gree A/C protocols.

See also
  https://github.com/ToniA/arduino-heatpumpir/blob/master/GreeHeatpumpIR.h
  https://github.com/crankyoldgit/IRremoteESP8266/issues/1508

## Variable Documentation

## ◆ kGreeBitMark

const uint16_t kGreeBitMark = 620

## ◆ kGreeBlockFooter

const uint8_t kGreeBlockFooter = 0b010

## ◆ kGreeBlockFooterBits

const uint8_t kGreeBlockFooterBits = 3

## ◆ kGreeHdrMark

const uint16_t kGreeHdrMark = 9000

## ◆ kGreeHdrSpace

const uint16_t kGreeHdrSpace = 4500

See #684 & real example in unit tests.

## ◆ kGreeMsgSpace

const uint16_t kGreeMsgSpace = 19980

See #1508, #386, & Kelvinator.

## ◆ kGreeOneSpace

const uint16_t kGreeOneSpace = 1600

## ◆ kGreeZeroSpace

const uint16_t kGreeZeroSpace = 540