IRremoteESP8266

IRArgoACBase< ARGO_PROTOCOL_T > Member List

This is the complete list of members for IRArgoACBase< ARGO_PROTOCOL_T >, including all inherited members.

_ | IRArgoACBase< ARGO_PROTOCOL_T > | protected
_checksum(ARGO_PROTOCOL_T *state) | IRArgoACBase< ARGO_PROTOCOL_T > | protected
_checksum(ArgoProtocol *state) | IRArgoACBase< ARGO_PROTOCOL_T > | related
_checksum(ArgoProtocolWREM3 *state) | IRArgoACBase< ARGO_PROTOCOL_T > | related
_irsend | IRArgoACBase< ARGO_PROTOCOL_T > | protected
_length | IRArgoACBase< ARGO_PROTOCOL_T > | protected
_messageType | IRArgoACBase< ARGO_PROTOCOL_T > | protected
_stateReset(ARGO_PROTOCOL_T *state, argoIrMessageType_t messageType=argoIrMessageType_t::AC_CONTROL) | IRArgoACBase< ARGO_PROTOCOL_T > | protected
_stateReset(ArgoProtocol *state, argoIrMessageType_t) | IRArgoACBase< ARGO_PROTOCOL_T > | related
_stateReset(ArgoProtocolWREM3 *state, argoIrMessageType_t messageType) | IRArgoACBase< ARGO_PROTOCOL_T > | related
begin(void) | IRArgoACBase< ARGO_PROTOCOL_T > |
calcChecksum(const uint8_t state[], const uint16_t length) | IRArgoACBase< ARGO_PROTOCOL_T > | protected static
calibrate(void) | IRArgoACBase< ARGO_PROTOCOL_T > | inline
checksum(void) | IRArgoACBase< ARGO_PROTOCOL_T > | protected
convertCommand(const stdAc::ac_command_t command) | IRArgoACBase< ARGO_PROTOCOL_T > | static
convertFan(const stdAc::fanspeed_t speed) | IRArgoACBase< ARGO_PROTOCOL_T > | static
convertMode(const stdAc::opmode_t mode) | IRArgoACBase< ARGO_PROTOCOL_T > | static
convertSwingV(const stdAc::swingv_t position) | IRArgoACBase< ARGO_PROTOCOL_T > | static
getChecksum(const uint8_t state[], const uint16_t length) | IRArgoACBase< ARGO_PROTOCOL_T > | protected static
getFanEx(void) const | IRArgoACBase< ARGO_PROTOCOL_T > |
getFlapEx(void) const | IRArgoACBase< ARGO_PROTOCOL_T > |
getiFeel(void) const | IRArgoACBase< ARGO_PROTOCOL_T > |
getMax(void) const | IRArgoACBase< ARGO_PROTOCOL_T > |
getMessageType(void) const | IRArgoACBase< ARGO_PROTOCOL_T > |
getMessageType(const uint8_t state[], const uint16_t length) | IRArgoACBase< ARGO_PROTOCOL_T > | static
getModeEx(void) const | IRArgoACBase< ARGO_PROTOCOL_T > |
getNight(void) const | IRArgoACBase< ARGO_PROTOCOL_T > |
getPower(void) const | IRArgoACBase< ARGO_PROTOCOL_T > |
getRaw(void) | IRArgoACBase< ARGO_PROTOCOL_T > |
getRawByteLength() const | IRArgoACBase< ARGO_PROTOCOL_T > |
getRawByteLength(const ARGO_PROTOCOL_T &raw, argoIrMessageType_t messageTypeHint=argoIrMessageType_t::AC_CONTROL) | IRArgoACBase< ARGO_PROTOCOL_T > | protected static
getRawByteLength(const ArgoProtocol &, argoIrMessageType_t messageType) | IRArgoACBase< ARGO_PROTOCOL_T > | related
getRawByteLength(const ArgoProtocolWREM3 &raw, argoIrMessageType_t) | IRArgoACBase< ARGO_PROTOCOL_T > | related
getSensorTemp(void) const | IRArgoACBase< ARGO_PROTOCOL_T > |
getStateLengthForIrMsgType(argoIrMessageType_t type) | IRArgoACBase< ARGO_PROTOCOL_T > | static
getTemp(void) const | IRArgoACBase< ARGO_PROTOCOL_T > |
IRArgoACBase(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRArgoACBase< ARGO_PROTOCOL_T > | explicit
off(void) | IRArgoACBase< ARGO_PROTOCOL_T > |
on(void) | IRArgoACBase< ARGO_PROTOCOL_T > |
send(const uint16_t repeat=kArgoDefaultRepeat) | IRArgoACBase< ARGO_PROTOCOL_T > |
setFan(const argoFan_t fan) | IRArgoACBase< ARGO_PROTOCOL_T > |
setFanEx(const argoFan_t fan) | IRArgoACBase< ARGO_PROTOCOL_T > | inline
setFlap(const argoFlap_t flap) | IRArgoACBase< ARGO_PROTOCOL_T > |
setFlapEx(const argoFlap_t flap) | IRArgoACBase< ARGO_PROTOCOL_T > | inline
setiFeel(const bool on) | IRArgoACBase< ARGO_PROTOCOL_T > |
setMax(const bool on) | IRArgoACBase< ARGO_PROTOCOL_T > |
setMessageType(const argoIrMessageType_t msgType) | IRArgoACBase< ARGO_PROTOCOL_T > |
setMode(const argoMode_t mode) | IRArgoACBase< ARGO_PROTOCOL_T > |
setModeEx(const argoMode_t mode) | IRArgoACBase< ARGO_PROTOCOL_T > | inline
setNight(const bool on) | IRArgoACBase< ARGO_PROTOCOL_T > |
setPower(const bool on) | IRArgoACBase< ARGO_PROTOCOL_T > |
setRaw(const uint8_t state[], const uint16_t length) | IRArgoACBase< ARGO_PROTOCOL_T > |
setSensorTemp(const uint8_t degrees) | IRArgoACBase< ARGO_PROTOCOL_T > |
setTemp(const uint8_t degrees) | IRArgoACBase< ARGO_PROTOCOL_T > |
stateReset(argoIrMessageType_t messageType=argoIrMessageType_t::AC_CONTROL) | IRArgoACBase< ARGO_PROTOCOL_T > | protected
toCommonCommand(const argoIrMessageType_t command) | IRArgoACBase< ARGO_PROTOCOL_T > | protected static
toCommonFanSpeed(const argoFan_t speed) | IRArgoACBase< ARGO_PROTOCOL_T > | protected static
toCommonMode(const argoMode_t mode) | IRArgoACBase< ARGO_PROTOCOL_T > | protected static
toCommonSwingV(const uint8_t position) | IRArgoACBase< ARGO_PROTOCOL_T > | protected static
validChecksum(const uint8_t state[], const uint16_t length) | IRArgoACBase< ARGO_PROTOCOL_T > | static