IRremoteESP8266

IRFujitsuAC Member List

This is the complete list of members for IRFujitsuAC, including all inherited members.

_ | IRFujitsuAC | private
_cmd | IRFujitsuAC | private
_irsend | IRFujitsuAC | private
_model | IRFujitsuAC | private
_rawstatemodified | IRFujitsuAC | private
_state_length | IRFujitsuAC | private
_state_length_short | IRFujitsuAC | private
begin(void) | IRFujitsuAC |
buildFromState(const uint16_t length) | IRFujitsuAC | private
calibrate(void) | IRFujitsuAC | inline
checkSum(void) | IRFujitsuAC | private
convertFan(stdAc::fanspeed_t speed) | IRFujitsuAC | static
convertMode(const stdAc::opmode_t mode) | IRFujitsuAC | static
get10CHeat(void) const | IRFujitsuAC |
getCelsius(void) const | IRFujitsuAC |
getClean(void) const | IRFujitsuAC |
getCmd(void) const | IRFujitsuAC |
getFanSpeed(void) const | IRFujitsuAC |
getFilter(void) const | IRFujitsuAC |
getId(void) const | IRFujitsuAC |
getMode(void) const | IRFujitsuAC |
getModel(void) const | IRFujitsuAC |
getOffSleepTimer(void) const | IRFujitsuAC |
getOnTimer(void) const | IRFujitsuAC |
getOutsideQuiet(void) const | IRFujitsuAC |
getPower(void) const | IRFujitsuAC |
getRaw(void) | IRFujitsuAC |
getStateLength(void) | IRFujitsuAC |
getSwing(void) const | IRFujitsuAC |
getTemp(void) const | IRFujitsuAC |
getTimerType(void) const | IRFujitsuAC |
IRFujitsuAC(const uint16_t pin, const fujitsu_ac_remote_model_t model=ARRAH2E, const bool inverted=false, const bool use_modulation=true) | IRFujitsuAC | explicit
isLongCode(void) const | IRFujitsuAC |
off(void) | IRFujitsuAC |
on(void) | IRFujitsuAC |
send(const uint16_t repeat=kFujitsuAcMinRepeat) | IRFujitsuAC |
set10CHeat(const bool on) | IRFujitsuAC |
setCelsius(const bool on) | IRFujitsuAC |
setClean(const bool on) | IRFujitsuAC |
setCmd(const uint8_t cmd) | IRFujitsuAC |
setFanSpeed(const uint8_t fan) | IRFujitsuAC |
setFilter(const bool on) | IRFujitsuAC |
setId(const uint8_t num) | IRFujitsuAC |
setMode(const uint8_t mode) | IRFujitsuAC |
setModel(const fujitsu_ac_remote_model_t model) | IRFujitsuAC |
setOffSleepTimer(const uint16_t nr_mins) | IRFujitsuAC | inline private
setOffTimer(const uint16_t nr_mins) | IRFujitsuAC |
setOnTimer(const uint16_t nr_mins) | IRFujitsuAC |
setOutsideQuiet(const bool on) | IRFujitsuAC |
setPower(const bool on) | IRFujitsuAC |
setRaw(const uint8_t newState[], const uint16_t length) | IRFujitsuAC |
setSleepTimer(const uint16_t nr_mins) | IRFujitsuAC |
setSwing(const uint8_t mode) | IRFujitsuAC |
setTemp(const float temp, const bool useCelsius=true) | IRFujitsuAC |
setTimerType(const uint8_t timertype) | IRFujitsuAC |
stateReset(void) | IRFujitsuAC |
stepHoriz(void) | IRFujitsuAC |
stepVert(void) | IRFujitsuAC |
toCommon(const stdAc::state_t *prev=NULL) | IRFujitsuAC |
toCommonFanSpeed(const uint8_t speed) | IRFujitsuAC | static
toCommonMode(const uint8_t mode) | IRFujitsuAC | static
toggleSwingHoriz(const bool update=true) | IRFujitsuAC |
toggleSwingVert(const bool update=true) | IRFujitsuAC |
toString(void) const | IRFujitsuAC |
updateUseLongOrShort(void) | IRFujitsuAC | private
validChecksum(uint8_t *state, const uint16_t length) | IRFujitsuAC | static