IRremoteESP8266

Public Attributes | List of all members
Trotec3550Protocol Union Reference

Native representation of a Trotec 3550 A/C message. More...

`#include <ir_Trotec.h>`

## Public Attributes
uint8_t | raw [kTrotecStateLength]
| Remote state in IR code form. More...
struct {
uint8_t Intro: 8
uint8_t SwingV:1
uint8_t Power:1
uint8_t __pad0__:1
uint8_t TimerSet:1
uint8_t TempC:4
uint8_t TimerHrs:4
uint8_t __pad1__:4
uint8_t TempF:5
uint8_t __pad2__:3
uint8_t __pad3__:8
uint8_t __pad4__:8
uint8_t Mode:2
uint8_t __pad5__:2
uint8_t Fan:2
uint8_t __pad6__:2
uint8_t __pad7__:7
uint8_t Celsius:1
uint8_t Sum:8
}; |

## Detailed Description

Native representation of a Trotec 3550 A/C message.

## Member Data Documentation

## ◆ @124

struct { ... }

## ◆ __pad0__

uint8_t Trotec3550Protocol::__pad0__

## ◆ __pad1__

uint8_t Trotec3550Protocol::__pad1__

## ◆ __pad2__

uint8_t Trotec3550Protocol::__pad2__

## ◆ __pad3__

uint8_t Trotec3550Protocol::__pad3__

## ◆ __pad4__

uint8_t Trotec3550Protocol::__pad4__

## ◆ __pad5__

uint8_t Trotec3550Protocol::__pad5__

## ◆ __pad6__

uint8_t Trotec3550Protocol::__pad6__

## ◆ __pad7__

uint8_t Trotec3550Protocol::__pad7__

## ◆ Celsius

uint8_t Trotec3550Protocol::Celsius

## ◆ Fan

uint8_t Trotec3550Protocol::Fan

## ◆ Intro

uint8_t Trotec3550Protocol::Intro

## ◆ Mode

uint8_t Trotec3550Protocol::Mode

## ◆ Power

uint8_t Trotec3550Protocol::Power

## ◆ raw

uint8_t Trotec3550Protocol::raw[kTrotecStateLength]

Remote state in IR code form.

## ◆ Sum

uint8_t Trotec3550Protocol::Sum

## ◆ SwingV

uint8_t Trotec3550Protocol::SwingV

## ◆ TempC

uint8_t Trotec3550Protocol::TempC

## ◆ TempF

uint8_t Trotec3550Protocol::TempF

## ◆ TimerHrs

uint8_t Trotec3550Protocol::TimerHrs

## ◆ TimerSet

uint8_t Trotec3550Protocol::TimerSet

The documentation for this union was generated from the following file:

- src/ir_Trotec.h