IRremoteESP8266

IRMirageAc Member List

This is the complete list of members for IRMirageAc, including all inherited members.

_ | IRMirageAc | private
_irsend | IRMirageAc | private
_model | IRMirageAc | private
begin(void) | IRMirageAc |
calculateChecksum(const uint8_t *data) | IRMirageAc | static
calibrate(void) | IRMirageAc | inline
checksum(void) | IRMirageAc | private
convertFan(const stdAc::fanspeed_t speed, const mirage_ac_remote_model_t model=mirage_ac_remote_model_t::KKG9AC1) | IRMirageAc | static
convertMode(const stdAc::opmode_t mode) | IRMirageAc | static
convertSwingV(const stdAc::swingv_t position) | IRMirageAc | static
fromCommon(const stdAc::state_t state) | IRMirageAc |
getCleanToggle(void) const | IRMirageAc |
getClock(void) const | IRMirageAc |
getFan(void) const | IRMirageAc |
getFilter(void) const | IRMirageAc |
getIFeel(void) const | IRMirageAc |
getLight(void) const | IRMirageAc |
getMode(void) const | IRMirageAc |
getModel(const bool useRaw=false) const | IRMirageAc |
getModel(const uint8_t *state) | IRMirageAc | static
getOffTimer(void) const | IRMirageAc |
getOnTimer(void) const | IRMirageAc |
getPower(void) const | IRMirageAc |
getQuiet(void) const | IRMirageAc |
getRaw(void) | IRMirageAc |
getSensorTemp(void) const | IRMirageAc |
getSleep(void) const | IRMirageAc |
getSwingH(void) const | IRMirageAc |
getSwingV(void) const | IRMirageAc |
getTemp(void) const | IRMirageAc |
getTurbo(void) const | IRMirageAc |
IRMirageAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRMirageAc | explicit
off(void) | IRMirageAc |
on(void) | IRMirageAc |
send(const uint16_t repeat=kMirageMinRepeat) | IRMirageAc |
setCleanToggle(const bool on) | IRMirageAc |
setClock(const uint32_t nr_of_seconds) | IRMirageAc |
setFan(const uint8_t speed) | IRMirageAc |
setFilter(const bool on) | IRMirageAc |
setIFeel(const bool on) | IRMirageAc |
setLight(const bool on) | IRMirageAc |
setMode(const uint8_t mode) | IRMirageAc |
setModel(const mirage_ac_remote_model_t model) | IRMirageAc |
setOffTimer(const uint16_t nr_of_mins) | IRMirageAc |
setOnTimer(const uint16_t nr_of_mins) | IRMirageAc |
setPower(const bool on) | IRMirageAc |
setQuiet(const bool on) | IRMirageAc |
setRaw(const uint8_t *data) | IRMirageAc |
setSensorTemp(const uint8_t degrees) | IRMirageAc |
setSleep(const bool on) | IRMirageAc |
setSwingH(const bool on) | IRMirageAc |
setSwingV(const uint8_t position) | IRMirageAc |
setTemp(const uint8_t degrees) | IRMirageAc |
setTurbo(const bool on) | IRMirageAc |
stateReset(void) | IRMirageAc |
toCommon(void) const | IRMirageAc |
toCommonFanSpeed(const uint8_t speed, const mirage_ac_remote_model_t model=mirage_ac_remote_model_t::KKG9AC1) | IRMirageAc | static
toCommonMode(const uint8_t mode) | IRMirageAc | static
toCommonSwingV(const uint8_t pos) | IRMirageAc | static
toString(void) const | IRMirageAc |
validChecksum(const uint8_t *data) | IRMirageAc | static