IRremoteESP8266

IRac Member List

This is the complete list of members for IRac, including all inherited members.

_inverted | IRac | private
_modulation | IRac | private
_pin | IRac | private
_prev | IRac | private
airton(IRAirtonAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool light, const bool econo, const bool filter, const int16_t sleep=-1) | IRac | private
airwell(IRAirwellAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan) | IRac | private
amcor(IRAmcorAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan) | IRac | private
argo(IRArgoAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool iFeel, const bool turbo, const int16_t sleep=-1) | IRac | private
argoWrem3_ACCommand(IRArgoAC_WREM3 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool iFeel, const bool night, const bool econo, const bool turbo, const bool filter, const bool light) | IRac | private
argoWrem3_ConfigSet(IRArgoAC_WREM3 *ac, const uint8_t param, const uint8_t value, bool safe=true) | IRac | private
argoWrem3_iFeelReport(IRArgoAC_WREM3 *ac, const float sensorTemp) | IRac | private
argoWrem3_SetTimer(IRArgoAC_WREM3 *ac, bool on, const uint16_t currentTime, const uint16_t delayMinutes) | IRac | private
boolToString(const bool value) | IRac | static
bosch144(IRBosch144AC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const bool quiet) | IRac | private
carrier64(IRCarrierAc64 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const int16_t sleep=-1) | IRac | private
cleanState(const stdAc::state_t state) | IRac | private static
cmpStates(const stdAc::state_t a, const stdAc::state_t b) | IRac | static
commandTypeToString(const stdAc::ac_command_t cmdType) | IRac | static
coolix(IRCoolixAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool iFeel, const bool turbo, const bool light, const bool clean, const int16_t sleep=-1) | IRac | private
corona(IRCoronaAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool econo) | IRac | private
daikin(IRDaikinESP *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool clean) | IRac | private
daikin128(IRDaikin128 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet, const bool turbo, const bool light, const bool econo, const int16_t sleep=-1, const int16_t clock=-1) | IRac | private
daikin152(IRDaikin152 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet, const bool turbo, const bool econo) | IRac | private
daikin160(IRDaikin160 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv) | IRac | private
daikin176(IRDaikin176 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingh_t swingh) | IRac | private
daikin2(IRDaikin2 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool light, const bool econo, const bool filter, const bool clean, const bool beep, const int16_t sleep=-1, const int16_t clock=-1) | IRac | private
daikin216(IRDaikin216 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo) | IRac | private
daikin64(IRDaikin64 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet, const bool turbo, const int16_t sleep=-1, const int16_t clock=-1) | IRac | private
delonghiac(IRDelonghiAc *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const bool turbo, const int16_t sleep=-1) | IRac | private
ecoclim(IREcoclimAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const int16_t sleep=-1, const int16_t clock=-1) | IRac | private
electra(IRElectraAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool iFeel, const bool turbo, const bool lighttoggle, const bool clean) | IRac | private
fanspeedToString(const stdAc::fanspeed_t speed) | IRac | static
fujitsu(IRFujitsuAC *ac, const fujitsu_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool filter, const bool clean, const int16_t sleep=-1) | IRac | private
getState(void) | IRac |
getStatePrev(void) | IRac |
goodweather(IRGoodweatherAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool light, const int16_t sleep=-1) | IRac | private
gree(IRGreeAC *ac, const gree_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool iFeel, const bool turbo, const bool econo, const bool light, const bool clean, const int16_t sleep=-1) | IRac | private
haier(IRHaierAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool filter, const int16_t sleep=-1, const int16_t clock=-1) | IRac | private
haier160(IRHaierAC160 *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool quiet, const bool filter, const bool clean, const bool light, const bool prevlight, const int16_t sleep=-1) | IRac | private
haier176(IRHaierAC176 *ac, const haier_ac176_remote_model_t model, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool quiet, const bool filter, const int16_t sleep=-1) | IRac | private
haierYrwo2(IRHaierACYRW02 *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool quiet, const bool filter, const int16_t sleep=-1) | IRac | private
handleToggles(const stdAc::state_t desired, const stdAc::state_t *prev=NULL) | IRac | private static
hasStateChanged(void) | IRac |
hitachi(IRHitachiAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh) | IRac | private
hitachi1(IRHitachiAc1 *ac, const hitachi_ac1_remote_model_t model, const bool on, const bool power_toggle, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool swing_toggle, const int16_t sleep=-1) | IRac | private
hitachi264(IRHitachiAc264 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan) | IRac | private
hitachi296(IRHitachiAc296 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan) | IRac | private
hitachi344(IRHitachiAc344 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh) | IRac | private
hitachi424(IRHitachiAc424 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv) | IRac | private
initState(stdAc::state_t *state, const decode_type_t vendor, const int16_t model, const bool power, const stdAc::opmode_t mode, const float degrees, const bool celsius, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool light, const bool filter, const bool clean, const bool beep, const int16_t sleep, const int16_t clock) | IRac | static
initState(stdAc::state_t *state) | IRac | static
IRac(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRac | explicit
isProtocolSupported(const decode_type_t protocol) | IRac | static
kelon(IRKelonAc *ac, const bool togglePower, const stdAc::opmode_t mode, const int8_t dryGrade, const float degrees, const stdAc::fanspeed_t fan, const bool toggleSwing, const bool superCool, const int16_t sleep) | IRac | private
kelvinator(IRKelvinatorAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool light, const bool filter, const bool clean) | IRac | private
lg(IRLgAc *ac, const lg_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingv_t swingv_prev, const stdAc::swingh_t swingh, const bool light) | IRac | private
markAsSent(void) | IRac |
midea(IRMideaAC *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool iFeel, const bool quiet, const bool quiet_prev, const bool turbo, const bool econo, const bool light, const bool clean, const int16_t sleep=-1) | IRac | private
mirage(IRMirageAc *ac, const stdAc::state_t state) | IRac | private
mitsubishi(IRMitsubishiAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const int16_t clock=-1) | IRac | private
mitsubishi112(IRMitsubishi112 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet) | IRac | private
mitsubishi136(IRMitsubishi136 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet) | IRac | private
mitsubishiHeavy152(IRMitsubishiHeavy152Ac *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool filter, const bool clean, const int16_t sleep=-1) | IRac | private
mitsubishiHeavy88(IRMitsubishiHeavy88Ac *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool econo, const bool clean) | IRac | private
neoclima(IRNeoclimaAc *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool econo, const bool light, const bool filter, const int16_t sleep=-1) | IRac | private
next | IRac |
opmodeToString(const stdAc::opmode_t mode, const bool ha=false) | IRac | static
panasonic(IRPanasonicAc *ac, const panasonic_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool filter, const int16_t clock=-1) | IRac | private
panasonic32(IRPanasonicAc32 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh) | IRac | private
rhoss(IRRhossAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swing) | IRac | private
samsung(IRSamsungAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool light, const bool filter, const bool clean, const bool beep, const int16_t sleep=-1, const bool prevpower=true, const int16_t prevsleep=-1, const bool forceextended=true) | IRac | private
sanyo(IRSanyoAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool iFeel, const bool beep, const int16_t sleep=-1) | IRac | private
sanyo88(IRSanyoAc88 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool filter, const int16_t sleep=-1, const int16_t clock=-1) | IRac | private
sendAc(void) | IRac |
sendAc(const stdAc::state_t desired, const stdAc::state_t *prev=NULL) | IRac |
sendAc(const decode_type_t vendor, const int16_t model, const bool power, const stdAc::opmode_t mode, const float degrees, const bool celsius, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool light, const bool filter, const bool clean, const bool beep, const int16_t sleep=-1, const int16_t clock=-1) | IRac |
sharp(IRSharpAc *ac, const sharp_ac_remote_model_t model, const bool on, const bool prev_power, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingv_t swingv_prev, const bool turbo, const bool light, const bool filter, const bool clean) | IRac | private
strToBool(const char *str, const bool def=false) | IRac | static
strToCommandType(const char *str, const stdAc::ac_command_t def=stdAc::ac_command_t::kControlCommand) | IRac | static
strToFanspeed(const char *str, const stdAc::fanspeed_t def=stdAc::fanspeed_t::kAuto) | IRac | static
strToModel(const char *str, const int16_t def=-1) | IRac | static
strToOpmode(const char *str, const stdAc::opmode_t def=stdAc::opmode_t::kAuto) | IRac | static
strToSwingH(const char *str, const stdAc::swingh_t def=stdAc::swingh_t::kOff) | IRac | static
strToSwingV(const char *str, const stdAc::swingv_t def=stdAc::swingv_t::kOff) | IRac | static
swinghToString(const stdAc::swingh_t swingh) | IRac | static
swingvToString(const stdAc::swingv_t swingv) | IRac | static
tcl112(IRTcl112Ac *ac, const tcl_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool light, const bool econo, const bool filter) | IRac | private
technibel(IRTechnibelAc *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const int16_t sleep=-1) | IRac | private
teco(IRTecoAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool light, const int16_t sleep=-1) | IRac | private
toshiba(IRToshibaAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool econo, const bool filter) | IRac | private
transcold(IRTranscoldAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh) | IRac | private
trotec(IRTrotecESP *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const int16_t sleep=-1) | IRac | private
trotec3550(IRTrotec3550 *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv) | IRac | private
truma(IRTrumaAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const bool quiet) | IRac | private
vestel(IRVestelAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool filter, const int16_t sleep=-1, const int16_t clock=-1, const bool sendNormal=true) | IRac | private
voltas(IRVoltas *ac, const voltas_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool econo, const bool light, const int16_t sleep=-1) | IRac | private
whirlpool(IRWhirlpoolAc *ac, const whirlpool_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool light, const int16_t sleep=-1, const int16_t clock=-1) | IRac | private