IRremoteESP8266

IRLgAc Member List

This is the complete list of members for IRLgAc, including all inherited members.

_ | IRLgAc | private
_irsend | IRLgAc | private
_isAKB73757604(void) const | IRLgAc | private
_isAKB74955603(void) const | IRLgAc | private
_isLG6711A20083V(void) const | IRLgAc | private
_isNormal(void) const | IRLgAc | private
_light | IRLgAc | private
_model | IRLgAc | private
_protocol | IRLgAc | private
_setTemp(const uint8_t value) | IRLgAc | inline private
_swingh | IRLgAc | private
_swingh_prev | IRLgAc | private
_swingv | IRLgAc | private
_swingv_prev | IRLgAc | private
_temp | IRLgAc | private
_vaneswingv | IRLgAc | private
_vaneswingv_prev | IRLgAc | private
begin(void) | IRLgAc |
calcChecksum(const uint32_t state) | IRLgAc | static
calcVaneSwingV(const uint8_t vane, const uint8_t position) | IRLgAc | static
calibrate(void) | IRLgAc | inline
checksum(void) | IRLgAc | private
convertFan(const stdAc::fanspeed_t speed) | IRLgAc | static
convertMode(const stdAc::opmode_t mode) | IRLgAc | static
convertSwingV(const stdAc::swingv_t swingv) | IRLgAc | static
convertVaneSwingV(const stdAc::swingv_t swingv) | IRLgAc | static
getFan(void) const | IRLgAc |
getLight(void) const | IRLgAc |
getMode(void) const | IRLgAc |
getModel(void) const | IRLgAc |
getPower(void) const | IRLgAc |
getRaw(void) | IRLgAc |
getSwingH(void) const | IRLgAc |
getSwingV(void) const | IRLgAc |
getTemp(void) const | IRLgAc |
getVaneCode(const uint32_t raw) | IRLgAc | static
getVaneSwingV(const uint8_t vane) const | IRLgAc |
IRLgAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRLgAc | explicit
isLightToggle(void) const | IRLgAc |
isOffCommand(void) const | IRLgAc |
isSwing(void) const | IRLgAc |
isSwingH(void) const | IRLgAc |
isSwingV(void) const | IRLgAc |
isSwingVToggle(void) const | IRLgAc |
isValidLgAc(void) const | IRLgAc |
isVaneSwingV(void) const | IRLgAc |
off(void) | IRLgAc |
on(void) | IRLgAc |
send(const uint16_t repeat=kLgDefaultRepeat) | IRLgAc |
setFan(const uint8_t speed) | IRLgAc |
setLight(const bool on) | IRLgAc |
setMode(const uint8_t mode) | IRLgAc |
setModel(const lg_ac_remote_model_t model) | IRLgAc |
setPower(const bool on) | IRLgAc |
setRaw(const uint32_t new_code, const decode_type_t protocol=decode_type_t::UNKNOWN) | IRLgAc |
setSwingH(const bool on) | IRLgAc |
setSwingV(const uint32_t position) | IRLgAc |
setTemp(const uint8_t degrees) | IRLgAc |
setVaneSwingV(const uint8_t vane, const uint8_t position) | IRLgAc |
stateReset(void) | IRLgAc |
toCommon(const stdAc::state_t *prev=NULL) const | IRLgAc |
toCommonFanSpeed(const uint8_t speed) | IRLgAc | static
toCommonMode(const uint8_t mode) | IRLgAc | static
toCommonSwingV(const uint32_t code) | IRLgAc | static
toCommonVaneSwingV(const uint8_t pos) | IRLgAc | static
toString(void) const | IRLgAc |
updateSwingPrev(void) | IRLgAc |
validChecksum(const uint32_t state) | IRLgAc | static