IRremoteESP8266

Public Member Functions | Static Public Member Functions | Private Member Functions | Static Private Member Functions | Private Attributes | List of all members
IRSharpAc Class Reference

Class for handling detailed Sharp A/C messages. More...

`#include <ir_Sharp.h>`

Collaboration diagram for IRSharpAc:
[legend]

## Public Member Functions
| IRSharpAc (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | send (const uint16_t repeat=kSharpAcDefaultRepeat)
| Send the current internal state as an IR message. More...
int8_t | calibrate (void)
| Run the calibration to calculate uSec timing offsets for this platform. More...
void | begin (void)
| Set up hardware to be able to send a message. More...
void | setModel (const sharp_ac_remote_model_t model)
| Set the model of the A/C to emulate. More...
sharp_ac_remote_model_t | getModel (const bool raw=false) const
| Get/Detect the model of the A/C. More...
void | on (void)
| Set the requested power state of the A/C to on. More...
void | off (void)
| Set the requested power state of the A/C to off. More...
void | setPower (const bool on, const bool prev_on=true)
| Change the power setting, including the previous power state. More...
bool | getPower (void) const
| Get the value of the current power setting. More...
bool | isPowerSpecial (void) const
| Is one of the special power states in use? More...
void | setTemp (const uint8_t temp, const bool save=true)
| Set the temperature. More...
uint8_t | getTemp (void) const
| Get the current temperature setting. More...
void | setFan (const uint8_t fan, const bool save=true)
| Set the speed of the fan. More...
uint8_t | getFan (void) const
| Get the current fan speed setting. More...
void | setMode (const uint8_t mode, const bool save=true)
| Set the operating mode of the A/C. More...
uint8_t | getMode (void) const
| Get the operating mode setting of the A/C. More...
void | setSpecial (const uint8_t mode)
| Set the value of the Special (button/command?) setting. More...
uint8_t | getSpecial (void) const
| Get the value of the Special (button/command?) setting. More...
bool | getTurbo (void) const
| Get the Turbo setting of the A/C. More...
void | setTurbo (const bool on)
| Set the Turbo setting of the A/C. More...
bool | getSwingToggle (void) const
| Get the (vertical) Swing Toggle setting of the A/C. More...
void | setSwingToggle (const bool on)
| Set the (vertical) Swing Toggle setting of the A/C. More...
uint8_t | getSwingV (void) const
| Get the Vertical Swing setting of the A/C. More...
void | setSwingV (const uint8_t position, const bool force=false)
| Set the Vertical Swing setting of the A/C. More...
bool | getIon (void) const
| Get the Ion (Filter) setting of the A/C. More...
void | setIon (const bool on)
| Set the Ion (Filter) setting of the A/C. More...
bool | getEconoToggle (void) const
| Get the Economical mode toggle setting of the A/C. More...
void | setEconoToggle (const bool on)
| Set the Economical mode toggle setting of the A/C. More...
bool | getLightToggle (void) const
| Get the Light toggle setting of the A/C. More...
void | setLightToggle (const bool on)
| Set the Light mode toggle setting of the A/C. More...
uint16_t | getTimerTime (void) const
| Get how long the timer is set for, in minutes. More...
bool | getTimerEnabled (void) const
| Is the Timer enabled? More...
bool | getTimerType (void) const
| Get the current timer type. More...
void | setTimer (bool enable, bool timer_type, uint16_t mins)
| Set or cancel the timer function. More...
bool | getClean (void) const
| Get the Clean setting of the A/C. More...
void | setClean (const bool on)
| Set the Economical mode toggle setting of the A/C. More...
uint8_t * | getRaw (void)
| Get a PTR to the internal state/code for this protocol. More...
void | setRaw (const uint8_t new_code[], const uint16_t length=kSharpAcStateLength)
| Set the internal state from a valid code for this protocol. More...
stdAc::opmode_t | toCommonMode (const uint8_t mode) const
| Convert a native mode into its stdAc equivalent. More...
stdAc::fanspeed_t | toCommonFanSpeed (const uint8_t speed) const
| Convert a native fan speed into its stdAc equivalent. More...
stdAc::swingv_t | toCommonSwingV (const uint8_t pos, const stdAc::opmode_t mode=stdAc::opmode_t::kHeat) const
| Convert a native vertical swing postion to it's common equivalent. More...
stdAc::state_t | toCommon (const stdAc::state_t *prev=NULL) const
| Convert the current internal state into its stdAc::state_t equivalent. More...
String | toString (void) const
| Convert the current internal state into a human readable string. More...

## Static Public Member Functions
static bool | validChecksum (uint8_t state[], const uint16_t length=kSharpAcStateLength)
| Verify the checksum is valid for a given state. More...
static uint8_t | convertMode (const stdAc::opmode_t mode)
| Convert a stdAc::opmode_t enum into its native mode. More...
static uint8_t | convertFan (const stdAc::fanspeed_t speed, const sharp_ac_remote_model_t model=sharp_ac_remote_model_t::A907)
| Convert a stdAc::fanspeed_t enum into it's native speed. More...
static uint8_t | convertSwingV (const stdAc::swingv_t position)
| Convert a standard A/C vertical swing into its native setting. More...

## Private Member Functions
void | stateReset (void)
| Reset the state of the remote to a known good state/sequence. More...
void | checksum (void)
| Calculate and set the checksum values for the internal state. More...
void | setPowerSpecial (const uint8_t value)
| Set the value of the Power Special setting without any checks. More...
uint8_t | getPowerSpecial (void) const
| Get the value of the Power Special setting. More...
void | clearPowerSpecial (void)
| Clear the "special"/non-normal bits in the power section. e.g. for normal/common command modes. More...
bool | _getEconoToggle (void) const
| Get the Economical mode toggle setting of the A/C. More...
void | _setEconoToggle (const bool on)
| Set the Economical mode toggle setting of the A/C. More...

## Static Private Member Functions
static uint8_t | calcChecksum (uint8_t state[], const uint16_t length=kSharpAcStateLength)
| Calculate the checksum for a given state. More...

## Private Attributes
IRsend | _irsend
| Instance of the IR send class. More...
SharpProtocol | _
uint8_t | _temp
| Saved copy of the desired temp. More...
uint8_t | _mode
| Saved copy of the desired mode. More...
uint8_t | _fan
| Saved copy of the desired fan speed. More...
sharp_ac_remote_model_t | _model
| Saved copy of the model. More...

## Detailed Description

Class for handling detailed Sharp A/C messages.

## Constructor & Destructor Documentation

## ◆ IRSharpAc()

IRSharpAc::IRSharpAc | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |
| explicit

Class constructor.

Parameters

  [in] | pin | GPIO to be used when sending.
  [in] | inverted | Is the output signal to be inverted?
  [in] | use_modulation | Is frequency modulation to be used?

## Member Function Documentation

## ◆ _getEconoToggle()

bool IRSharpAc::_getEconoToggle | ( | void |  | ) | const
| private

Get the Economical mode toggle setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

Note
  Shares the same location as the Light setting on A705.

## ◆ _setEconoToggle()

void IRSharpAc::_setEconoToggle | ( | const bool | on | ) |
| private

Set the Economical mode toggle setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

Warning
  Probably incompatible with `setTurbo()`

Note
  Shares the same location as the Light setting on A705.

## ◆ begin()

void IRSharpAc::begin | ( | void |  | ) |

Set up hardware to be able to send a message.

## ◆ calcChecksum()

uint8_t IRSharpAc::calcChecksum | ( | uint8_t | state[],
|  | const uint16_t | length = `kSharpAcStateLength`
| ) |  |
| static private

Calculate the checksum for a given state.

Parameters

  [in] | state | The array to calc the checksum of.
  [in] | length | The length/size of the array.

Returns
  The calculated 4-bit checksum value.

## ◆ calibrate()

int8_t IRSharpAc::calibrate | ( | void |  | ) |
| inline

Run the calibration to calculate uSec timing offsets for this platform.

Returns
  The uSec timing offset needed per modulation of the IR Led.

Note
  This will produce a 65ms IR signal pulse at 38kHz. Only ever needs to be run once per object instantiation, if at all.

## ◆ checksum()

void IRSharpAc::checksum | ( | void |  | ) |
| private

Calculate and set the checksum values for the internal state.

## ◆ clearPowerSpecial()

void IRSharpAc::clearPowerSpecial | ( | void |  | ) |
| private

Clear the "special"/non-normal bits in the power section. e.g. for normal/common command modes.

## ◆ convertFan()

uint8_t IRSharpAc::convertFan | ( | const stdAc::fanspeed_t | speed,
|  | const sharp_ac_remote_model_t | model = `sharp_ac_remote_model_t::A907`
| ) |  |
| static

Convert a stdAc::fanspeed_t enum into it's native speed.

Parameters

  [in] | speed | The enum to be converted.
  [in] | model | The enum of the appropriate model.

Returns
  The native equivalent of the enum.

## ◆ convertMode()

uint8_t IRSharpAc::convertMode | ( | const stdAc::opmode_t | mode | ) |
| static

Convert a stdAc::opmode_t enum into its native mode.

Parameters

  [in] | mode | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ convertSwingV()

uint8_t IRSharpAc::convertSwingV | ( | const stdAc::swingv_t | position | ) |
| static

Convert a standard A/C vertical swing into its native setting.

Parameters

  [in] | position | A stdAc::swingv_t position to convert.

Returns
  The equivalent native horizontal swing position.

## ◆ getClean()

bool IRSharpAc::getClean | ( | void |  | ) | const

Get the Clean setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getEconoToggle()

bool IRSharpAc::getEconoToggle | ( | void |  | ) | const

Get the Economical mode toggle setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

Note
  Available on the A907 models.

## ◆ getFan()

uint8_t IRSharpAc::getFan | ( | void |  | ) | const

Get the current fan speed setting.

Returns
  The current fan speed/mode.

## ◆ getIon()

bool IRSharpAc::getIon | ( | void |  | ) | const

Get the Ion (Filter) setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getLightToggle()

bool IRSharpAc::getLightToggle | ( | void |  | ) | const

Get the Light toggle setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

Note
  Not available on the A907 model.

## ◆ getMode()

uint8_t IRSharpAc::getMode | ( | void |  | ) | const

Get the operating mode setting of the A/C.

Returns
  The current operating mode setting.

## ◆ getModel()

sharp_ac_remote_model_t IRSharpAc::getModel | ( | const bool | raw = `false` | ) | const

Get/Detect the model of the A/C.

Parameters

  [in] | raw | Try to determine the model from the raw code only.

Returns
  The enum of the compatible model.

## ◆ getPower()

bool IRSharpAc::getPower | ( | void |  | ) | const

Get the value of the current power setting.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getPowerSpecial()

uint8_t IRSharpAc::getPowerSpecial | ( | void |  | ) | const
| private

Get the value of the Power Special setting.

Returns
  The setting's value.

## ◆ getRaw()

uint8_t * IRSharpAc::getRaw | ( | void |  | ) |

Get a PTR to the internal state/code for this protocol.

Returns
  PTR to a code for this protocol based on the current internal state.

## ◆ getSpecial()

uint8_t IRSharpAc::getSpecial | ( | void |  | ) | const

Get the value of the Special (button/command?) setting.

Returns
  The setting's value.

## ◆ getSwingToggle()

bool IRSharpAc::getSwingToggle | ( | void |  | ) | const

Get the (vertical) Swing Toggle setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getSwingV()

uint8_t IRSharpAc::getSwingV | ( | void |  | ) | const

Get the Vertical Swing setting of the A/C.

Returns
  The position of the Vertical Swing setting.

## ◆ getTemp()

uint8_t IRSharpAc::getTemp | ( | void |  | ) | const

Get the current temperature setting.

Returns
  The current setting for temp. in degrees celsius.

## ◆ getTimerEnabled()

bool IRSharpAc::getTimerEnabled | ( | void |  | ) | const

Is the Timer enabled?

Returns
  true, the setting is on. false, the setting is off.

## ◆ getTimerTime()

uint16_t IRSharpAc::getTimerTime | ( | void |  | ) | const

Get how long the timer is set for, in minutes.

Returns
  The time in nr of minutes.

## ◆ getTimerType()

bool IRSharpAc::getTimerType | ( | void |  | ) | const

Get the current timer type.

Returns
  true, It's an "On" timer. false, It's an "Off" timer.

## ◆ getTurbo()

bool IRSharpAc::getTurbo | ( | void |  | ) | const

Get the Turbo setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ isPowerSpecial()

bool IRSharpAc::isPowerSpecial | ( | void |  | ) | const

Is one of the special power states in use?

Returns
  true, it is. false, it isn't.

## ◆ off()

void IRSharpAc::off | ( | void |  | ) |

Set the requested power state of the A/C to off.

## ◆ on()

void IRSharpAc::on | ( | void |  | ) |

Set the requested power state of the A/C to on.

## ◆ send()

void IRSharpAc::send | ( | const uint16_t | repeat = `kSharpAcDefaultRepeat` | ) |

Send the current internal state as an IR message.

Parameters

  [in] | repeat | Nr. of times the message will be repeated.

## ◆ setClean()

void IRSharpAc::setClean | ( | const bool | on | ) |

Set the Economical mode toggle setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

Note
  Officially A/C unit needs to be "Off" before clean mode can be entered

## ◆ setEconoToggle()

void IRSharpAc::setEconoToggle | ( | const bool | on | ) |

Set the Economical mode toggle setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

Warning
  Probably incompatible with `setTurbo()`

Note
  Available on the A907 models.

## ◆ setFan()

void IRSharpAc::setFan | ( | const uint8_t | speed,
|  | const bool | save = `true`
| ) |  |

Set the speed of the fan.

Parameters

  [in] | speed | The desired setting.
  [in] | save | Do we save this setting as a user set one?

## ◆ setIon()

void IRSharpAc::setIon | ( | const bool | on | ) |

Set the Ion (Filter) setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setLightToggle()

void IRSharpAc::setLightToggle | ( | const bool | on | ) |

Set the Light mode toggle setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

Warning
  Probably incompatible with `setTurbo()`

Note
  Not available on the A907 model.

## ◆ setMode()

void IRSharpAc::setMode | ( | const uint8_t | mode,
|  | const bool | save = `true`
| ) |  |

Set the operating mode of the A/C.

Parameters

  [in] | mode | The desired operating mode.
  [in] | save | Do we save this setting as a user set one?

## ◆ setModel()

void IRSharpAc::setModel | ( | const sharp_ac_remote_model_t | model | ) |

Set the model of the A/C to emulate.

Parameters

  [in] | model | The enum of the appropriate model.

## ◆ setPower()

void IRSharpAc::setPower | ( | const bool | on,
|  | const bool | prev_on = `true`
| ) |  |

Change the power setting, including the previous power state.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.
  [in] | prev_on | true, the setting is on. false, the setting is off.

## ◆ setPowerSpecial()

void IRSharpAc::setPowerSpecial | ( | const uint8_t | value | ) |
| inline private

Set the value of the Power Special setting without any checks.

Parameters

  [in] | value | The value to set Power Special to.

## ◆ setRaw()

void IRSharpAc::setRaw | ( | const uint8_t | new_code[],
|  | const uint16_t | length = `kSharpAcStateLength`
| ) |  |

Set the internal state from a valid code for this protocol.

Parameters

  [in] | new_code | A valid code for this protocol.
  [in] | length | The length/size of the new_code array.

## ◆ setSpecial()

void IRSharpAc::setSpecial | ( | const uint8_t | mode | ) |

Set the value of the Special (button/command?) setting.

Parameters

  [in] | mode | The value to set Special to.

## ◆ setSwingToggle()

void IRSharpAc::setSwingToggle | ( | const bool | on | ) |

Set the (vertical) Swing Toggle setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setSwingV()

void IRSharpAc::setSwingV | ( | const uint8_t | position,
|  | const bool | force = `false`
| ) |  |

Set the Vertical Swing setting of the A/C.

Note
  Some positions may not work on all models.

Parameters

  [in] | position | The desired position/setting.

Note
  `setSwingV(kSharpAcSwingVLowest)` will only allow the Lowest setting in Heat mode, it will default to `kSharpAcSwingVLow` otherwise. If you want to set this value in other modes e.g. Cool, you must use `setSwingV`s optional `force` parameter.

Parameters

  [in] | force | Do we override the safety checks and just do it?

## ◆ setTemp()

void IRSharpAc::setTemp | ( | const uint8_t | temp,
|  | const bool | save = `true`
| ) |  |

Set the temperature.

Parameters

  [in] | temp | The temperature in degrees celsius.
  [in] | save | Do we save this setting as a user set one?

## ◆ setTimer()

void IRSharpAc::setTimer | ( | bool | enable,
|  | bool | timer_type,
|  | uint16_t | mins
| ) |  |

Set or cancel the timer function.

Parameters

  [in] | enable | Is the timer to be enabled (true) or canceled(false)?
  [in] | timer_type | An On (true) or an Off (false). Ignored if canceled.
  [in] | mins | Nr. of minutes the timer is to be set to.

Note
  Rounds down to 30 min increments. (max: 720 mins (12h), 0 is Off)

## ◆ setTurbo()

void IRSharpAc::setTurbo | ( | const bool | on | ) |

Set the Turbo setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

Note
  If you use this method, you will need to send it before making other changes to the settings, as they may overwrite some of the bits used by this setting.

## ◆ stateReset()

void IRSharpAc::stateReset | ( | void |  | ) |
| private

Reset the state of the remote to a known good state/sequence.

## ◆ toCommon()

stdAc::state_t IRSharpAc::toCommon | ( | const stdAc::state_t * | prev = `NULL` | ) | const

Convert the current internal state into its stdAc::state_t equivalent.

Parameters

  [in] | prev | Ptr to the previous state if required.

Returns
  The stdAc equivalent of the native settings.

## ◆ toCommonFanSpeed()

stdAc::fanspeed_t IRSharpAc::toCommonFanSpeed | ( | const uint8_t | speed | ) | const

Convert a native fan speed into its stdAc equivalent.

Parameters

  [in] | speed | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toCommonMode()

stdAc::opmode_t IRSharpAc::toCommonMode | ( | const uint8_t | mode | ) | const

Convert a native mode into its stdAc equivalent.

Parameters

  [in] | mode | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toCommonSwingV()

stdAc::swingv_t IRSharpAc::toCommonSwingV | ( | const uint8_t | pos,
|  | const stdAc::opmode_t | mode = `stdAc::opmode_t::kHeat`
| ) |  | const

Convert a native vertical swing postion to it's common equivalent.

Parameters

  [in] | pos | A native position to convert.
  [in] | mode | What operating mode are we in?

Returns
  The common vertical swing position.

## ◆ toString()

String IRSharpAc::toString | ( | void |  | ) | const

Convert the current internal state into a human readable string.

Returns
  A human readable string.

## ◆ validChecksum()

bool IRSharpAc::validChecksum | ( | uint8_t | state[],
|  | const uint16_t | length = `kSharpAcStateLength`
| ) |  |
| static

Verify the checksum is valid for a given state.

Parameters

  [in] | state | The array to verify the checksum of.
  [in] | length | The length/size of the array.

Returns
  true, if the state has a valid checksum. Otherwise, false.

## Member Data Documentation

## ◆ _

SharpProtocol IRSharpAc::_
| private

## ◆ _fan

uint8_t IRSharpAc::_fan
| private

Saved copy of the desired fan speed.

## ◆ _irsend

IRsend IRSharpAc::_irsend
| private

Instance of the IR send class.

## ◆ _mode

uint8_t IRSharpAc::_mode
| private

Saved copy of the desired mode.

## ◆ _model

sharp_ac_remote_model_t IRSharpAc::_model
| private

Saved copy of the model.

## ◆ _temp

uint8_t IRSharpAc::_temp
| private

Saved copy of the desired temp.

The documentation for this class was generated from the following files:

- src/ir_Sharp.h
- src/ir_Sharp.cpp