IRremoteESP8266

Public Attributes | List of all members
RhossProtocol Union Reference

Native representation of a Rhoss A/C message. More...

`#include <ir_Rhoss.h>`

## Public Attributes
uint8_t | raw [kRhossStateLength]
struct {
uint8_t __pad0__:8
uint8_t Temp:4
uint8_t __pad1__:4
uint8_t __pad2__:8
uint8_t __pad3__:8
uint8_t Fan:2
uint8_t __pad4__:2
uint8_t Mode:4
uint8_t Swing:1
uint8_t __pad5__:5
uint8_t Power:2
uint8_t __pad6__:8
uint8_t __pad7__:8
uint8_t __pad8__:8
uint8_t __pad9__:8
uint8_t __pad10__:8
uint8_t Sum:8
}; |

## Detailed Description

Native representation of a Rhoss A/C message.

## Member Data Documentation

## ◆ @100

struct { ... }

## ◆ __pad0__

uint8_t RhossProtocol::__pad0__

## ◆ __pad10__

uint8_t RhossProtocol::__pad10__

## ◆ __pad1__

uint8_t RhossProtocol::__pad1__

## ◆ __pad2__

uint8_t RhossProtocol::__pad2__

## ◆ __pad3__

uint8_t RhossProtocol::__pad3__

## ◆ __pad4__

uint8_t RhossProtocol::__pad4__

## ◆ __pad5__

uint8_t RhossProtocol::__pad5__

## ◆ __pad6__

uint8_t RhossProtocol::__pad6__

## ◆ __pad7__

uint8_t RhossProtocol::__pad7__

## ◆ __pad8__

uint8_t RhossProtocol::__pad8__

## ◆ __pad9__

uint8_t RhossProtocol::__pad9__

## ◆ Fan

uint8_t RhossProtocol::Fan

## ◆ Mode

uint8_t RhossProtocol::Mode

## ◆ Power

uint8_t RhossProtocol::Power

## ◆ raw

uint8_t RhossProtocol::raw[kRhossStateLength]

## ◆ Sum

uint8_t RhossProtocol::Sum

## ◆ Swing

uint8_t RhossProtocol::Swing

## ◆ Temp

uint8_t RhossProtocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Rhoss.h