IRremoteESP8266

Public Member Functions | Static Public Member Functions | Private Member Functions | Private Attributes | List of all members
IRWhirlpoolAc Class Reference

Class for handling detailed Whirlpool A/C messages. More...

`#include <ir_Whirlpool.h>`

Collaboration diagram for IRWhirlpoolAc:
[legend]

## Public Member Functions
| IRWhirlpoolAc (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | stateReset (void)
| Reset the state of the remote to a known good state/sequence. More...
void | send (const uint16_t repeat=kWhirlpoolAcDefaultRepeat, const bool calcchecksum=true)
| Send the current internal state as an IR message. More...
int8_t | calibrate (void)
| Run the calibration to calculate uSec timing offsets for this platform. More...
void | begin (void)
| Set up hardware to be able to send a message. More...
void | setPowerToggle (const bool on)
| Change the power toggle setting. More...
bool | getPowerToggle (void) const
| Get the value of the current power toggle setting. More...
void | setSleep (const bool on)
| Set the Sleep setting of the A/C. More...
bool | getSleep (void) const
| Get the Sleep setting of the A/C. More...
void | setSuper (const bool on)
| Set the Super (Turbo/Jet) setting of the A/C. More...
bool | getSuper (void) const
| Get the Super (Turbo/Jet) setting of the A/C. More...
void | setTemp (const uint8_t temp)
| Set the temperature. More...
uint8_t | getTemp (void) const
| Get the current temperature setting. More...
void | setFan (const uint8_t speed)
| Set the speed of the fan. More...
uint8_t | getFan (void) const
| Get the current fan speed setting. More...
void | setMode (const uint8_t mode)
| Set the operating mode of the A/C. More...
uint8_t | getMode (void) const
| Get the operating mode setting of the A/C. More...
void | setSwing (const bool on)
| Set the (vertical) swing setting of the A/C. More...
bool | getSwing (void) const
| Get the (vertical) swing setting of the A/C. More...
void | setLight (const bool on)
| Set the Light (Display/LED) setting of the A/C. More...
bool | getLight (void) const
| Get the Light (Display/LED) setting of the A/C. More...
uint16_t | getClock (void) const
| Get the clock time in nr. of minutes past midnight. More...
void | setClock (const uint16_t minspastmidnight)
| Set the clock time in nr. of minutes past midnight. More...
uint16_t | getOnTimer (void) const
| Get the On Timer time.. More...
void | setOnTimer (const uint16_t minspastmidnight)
| Set the On Timer time. More...
void | enableOnTimer (const bool on)
| Enable the On Timer. More...
bool | isOnTimerEnabled (void) const
| Is the On timer enabled? More...
uint16_t | getOffTimer (void) const
| Get the Off Timer time.. More...
void | setOffTimer (const uint16_t minspastmidnight)
| Set the Off Timer time. More...
void | enableOffTimer (const bool on)
| Enable the Off Timer. More...
bool | isOffTimerEnabled (void) const
| Is the Off timer enabled? More...
void | setCommand (const uint8_t code)
| Set the Command (Button) setting of the A/C. More...
uint8_t | getCommand (void) const
| Get the Command (Button) setting of the A/C. More...
whirlpool_ac_remote_model_t | getModel (void) const
| Get/Detect the model of the A/C. More...
void | setModel (const whirlpool_ac_remote_model_t model)
| Set the model of the A/C to emulate. More...
uint8_t * | getRaw (const bool calcchecksum=true)
| Get a copy of the internal state/code for this protocol. More...
void | setRaw (const uint8_t new_code[], const uint16_t length=kWhirlpoolAcStateLength)
| Set the internal state from a valid code for this protocol. More...
stdAc::state_t | toCommon (const stdAc::state_t *prev=NULL) const
| Convert the current internal state into its stdAc::state_t equivalent. More...
String | toString (void) const
| Convert the current internal state into a human readable string. More...

## Static Public Member Functions
static bool | validChecksum (const uint8_t state[], const uint16_t length=kWhirlpoolAcStateLength)
| Verify the checksum is valid for a given state. More...
static uint8_t | convertMode (const stdAc::opmode_t mode)
| Convert a stdAc::opmode_t enum into its native mode. More...
static uint8_t | convertFan (const stdAc::fanspeed_t speed)
| Convert a stdAc::fanspeed_t enum into it's native speed. More...
static stdAc::opmode_t | toCommonMode (const uint8_t mode)
| Convert a native mode into its stdAc equivalent. More...
static stdAc::fanspeed_t | toCommonFanSpeed (const uint8_t speed)
| Convert a native fan speed into its stdAc equivalent. More...

## Private Member Functions
void | checksum (const uint16_t length=kWhirlpoolAcStateLength)
| Calculate & set the checksum for the current internal state of the remote. More...
void | _setTemp (const uint8_t temp, const bool remember=true)
| Set the temperature. More...
void | _setMode (const uint8_t mode)
| Set the operating mode of the A/C. More...
int8_t | getTempOffset (void) const
| Calculate the temp. offset in deg C for the current model. More...

## Private Attributes
IRsend | _irsend
| Instance of the IR send class. More...
WhirlpoolProtocol | _
uint8_t | _desiredtemp
| The last user explicitly set temperature. More...

## Detailed Description

Class for handling detailed Whirlpool A/C messages.

## Constructor & Destructor Documentation

## ◆ IRWhirlpoolAc()

IRWhirlpoolAc::IRWhirlpoolAc | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |
| explicit

Class constructor.

Parameters

  [in] | pin | GPIO to be used when sending.
  [in] | inverted | Is the output signal to be inverted?
  [in] | use_modulation | Is frequency modulation to be used?

## Member Function Documentation

## ◆ _setMode()

void IRWhirlpoolAc::_setMode | ( | const uint8_t | mode | ) |
| private

Set the operating mode of the A/C.

Parameters

  [in] | mode | The desired operating mode.

Note
  Internal use only.

## ◆ _setTemp()

void IRWhirlpoolAc::_setTemp | ( | const uint8_t | temp,
|  | const bool | remember = `true`
| ) |  |
| private

Set the temperature.

Parameters

  [in] | temp | The temperature in degrees celsius.
  [in] | remember | Do we save this temperature?

Note
  Internal use only.

## ◆ begin()

void IRWhirlpoolAc::begin | ( | void |  | ) |

Set up hardware to be able to send a message.

## ◆ calibrate()

int8_t IRWhirlpoolAc::calibrate | ( | void |  | ) |
| inline

Run the calibration to calculate uSec timing offsets for this platform.

Returns
  The uSec timing offset needed per modulation of the IR Led.

Note
  This will produce a 65ms IR signal pulse at 38kHz. Only ever needs to be run once per object instantiation, if at all.

## ◆ checksum()

void IRWhirlpoolAc::checksum | ( | const uint16_t | length = `kWhirlpoolAcStateLength` | ) |
| private

Calculate & set the checksum for the current internal state of the remote.

Parameters

  [in] | length | The length/size of the internal state array.

## ◆ convertFan()

uint8_t IRWhirlpoolAc::convertFan | ( | const stdAc::fanspeed_t | speed | ) |
| static

Convert a stdAc::fanspeed_t enum into it's native speed.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ convertMode()

uint8_t IRWhirlpoolAc::convertMode | ( | const stdAc::opmode_t | mode | ) |
| static

Convert a stdAc::opmode_t enum into its native mode.

Parameters

  [in] | mode | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ enableOffTimer()

void IRWhirlpoolAc::enableOffTimer | ( | const bool | on | ) |

Enable the Off Timer.

Parameters

  [in] | on | true, the timer is enabled. false, the timer is disabled.

## ◆ enableOnTimer()

void IRWhirlpoolAc::enableOnTimer | ( | const bool | on | ) |

Enable the On Timer.

Parameters

  [in] | on | true, the timer is enabled. false, the timer is disabled.

## ◆ getClock()

uint16_t IRWhirlpoolAc::getClock | ( | void |  | ) | const

Get the clock time in nr. of minutes past midnight.

Returns
  The time expressed as the Nr. of minutes past midnight.

## ◆ getCommand()

uint8_t IRWhirlpoolAc::getCommand | ( | void |  | ) | const

Get the Command (Button) setting of the A/C.

Returns
  The current Command (Button) of the A/C.

## ◆ getFan()

uint8_t IRWhirlpoolAc::getFan | ( | void |  | ) | const

Get the current fan speed setting.

Returns
  The current fan speed/mode.

## ◆ getLight()

bool IRWhirlpoolAc::getLight | ( | void |  | ) | const

Get the Light (Display/LED) setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getMode()

uint8_t IRWhirlpoolAc::getMode | ( | void |  | ) | const

Get the operating mode setting of the A/C.

Returns
  The current operating mode setting.

## ◆ getModel()

whirlpool_ac_remote_model_t IRWhirlpoolAc::getModel | ( | void |  | ) | const

Get/Detect the model of the A/C.

Returns
  The enum of the compatible model.

## ◆ getOffTimer()

uint16_t IRWhirlpoolAc::getOffTimer | ( | void |  | ) | const

Get the Off Timer time..

Returns
  The time expressed as the Nr. of minutes past midnight.

## ◆ getOnTimer()

uint16_t IRWhirlpoolAc::getOnTimer | ( | void |  | ) | const

Get the On Timer time..

Returns
  The time expressed as the Nr. of minutes past midnight.

## ◆ getPowerToggle()

bool IRWhirlpoolAc::getPowerToggle | ( | void |  | ) | const

Get the value of the current power toggle setting.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getRaw()

uint8_t * IRWhirlpoolAc::getRaw | ( | const bool | calcchecksum = `true` | ) |

Get a copy of the internal state/code for this protocol.

Parameters

  [in] | calcchecksum | Do we need to calculate the checksum?.

Returns
  A code for this protocol based on the current internal state.

## ◆ getSleep()

bool IRWhirlpoolAc::getSleep | ( | void |  | ) | const

Get the Sleep setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getSuper()

bool IRWhirlpoolAc::getSuper | ( | void |  | ) | const

Get the Super (Turbo/Jet) setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getSwing()

bool IRWhirlpoolAc::getSwing | ( | void |  | ) | const

Get the (vertical) swing setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getTemp()

uint8_t IRWhirlpoolAc::getTemp | ( | void |  | ) | const

Get the current temperature setting.

Returns
  The current setting for temp. in degrees celsius.

## ◆ getTempOffset()

int8_t IRWhirlpoolAc::getTempOffset | ( | void |  | ) | const
| private

Calculate the temp. offset in deg C for the current model.

Returns
  The temperature offset.

## ◆ isOffTimerEnabled()

bool IRWhirlpoolAc::isOffTimerEnabled | ( | void |  | ) | const

Is the Off timer enabled?

Returns
  true, the Timer is enabled. false, the Timer is disabled.

## ◆ isOnTimerEnabled()

bool IRWhirlpoolAc::isOnTimerEnabled | ( | void |  | ) | const

Is the On timer enabled?

Returns
  true, the Timer is enabled. false, the Timer is disabled.

## ◆ send()

void IRWhirlpoolAc::send | ( | const uint16_t | repeat = `kWhirlpoolAcDefaultRepeat`,
|  | const bool | calcchecksum = `true`
| ) |  |

Send the current internal state as an IR message.

Parameters

  [in] | repeat | Nr. of times the message will be repeated.
  [in] | calcchecksum | Do we need to calculate the checksum?.

## ◆ setClock()

void IRWhirlpoolAc::setClock | ( | const uint16_t | minspastmidnight | ) |

Set the clock time in nr. of minutes past midnight.

Parameters

  [in] | minspastmidnight | The time expressed as minutes past midnight.

## ◆ setCommand()

void IRWhirlpoolAc::setCommand | ( | const uint8_t | code | ) |

Set the Command (Button) setting of the A/C.

Parameters

  [in] | code | The current Command (Button) of the A/C.

## ◆ setFan()

void IRWhirlpoolAc::setFan | ( | const uint8_t | speed | ) |

Set the speed of the fan.

Parameters

  [in] | speed | The desired setting.

## ◆ setLight()

void IRWhirlpoolAc::setLight | ( | const bool | on | ) |

Set the Light (Display/LED) setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setMode()

void IRWhirlpoolAc::setMode | ( | const uint8_t | mode | ) |

Set the operating mode of the A/C.

Parameters

  [in] | mode | The desired operating mode.

## ◆ setModel()

void IRWhirlpoolAc::setModel | ( | const whirlpool_ac_remote_model_t | model | ) |

Set the model of the A/C to emulate.

Parameters

  [in] | model | The enum of the appropriate model.

## ◆ setOffTimer()

void IRWhirlpoolAc::setOffTimer | ( | const uint16_t | minspastmidnight | ) |

Set the Off Timer time.

Parameters

  [in] | minspastmidnight | The time expressed as minutes past midnight.

## ◆ setOnTimer()

void IRWhirlpoolAc::setOnTimer | ( | const uint16_t | minspastmidnight | ) |

Set the On Timer time.

Parameters

  [in] | minspastmidnight | The time expressed as minutes past midnight.

## ◆ setPowerToggle()

void IRWhirlpoolAc::setPowerToggle | ( | const bool | on | ) |

Change the power toggle setting.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setRaw()

void IRWhirlpoolAc::setRaw | ( | const uint8_t | new_code[],
|  | const uint16_t | length = `kWhirlpoolAcStateLength`
| ) |  |

Set the internal state from a valid code for this protocol.

Parameters

  [in] | new_code | A valid code for this protocol.
  [in] | length | The length/size of the new_code array.

## ◆ setSleep()

void IRWhirlpoolAc::setSleep | ( | const bool | on | ) |

Set the Sleep setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setSuper()

void IRWhirlpoolAc::setSuper | ( | const bool | on | ) |

Set the Super (Turbo/Jet) setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setSwing()

void IRWhirlpoolAc::setSwing | ( | const bool | on | ) |

Set the (vertical) swing setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setTemp()

void IRWhirlpoolAc::setTemp | ( | const uint8_t | temp | ) |

Set the temperature.

Parameters

  [in] | temp | The temperature in degrees celsius.

## ◆ stateReset()

void IRWhirlpoolAc::stateReset | ( | void |  | ) |

Reset the state of the remote to a known good state/sequence.

## ◆ toCommon()

stdAc::state_t IRWhirlpoolAc::toCommon | ( | const stdAc::state_t * | prev = `NULL` | ) | const

Convert the current internal state into its stdAc::state_t equivalent.

Parameters

  [in] | prev | Ptr to the previous state if required.

Returns
  The stdAc equivalent of the native settings.

## ◆ toCommonFanSpeed()

stdAc::fanspeed_t IRWhirlpoolAc::toCommonFanSpeed | ( | const uint8_t | speed | ) |
| static

Convert a native fan speed into its stdAc equivalent.

Parameters

  [in] | speed | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toCommonMode()

stdAc::opmode_t IRWhirlpoolAc::toCommonMode | ( | const uint8_t | mode | ) |
| static

Convert a native mode into its stdAc equivalent.

Parameters

  [in] | mode | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toString()

String IRWhirlpoolAc::toString | ( | void |  | ) | const

Convert the current internal state into a human readable string.

Returns
  A human readable string.

## ◆ validChecksum()

bool IRWhirlpoolAc::validChecksum | ( | const uint8_t | state[],
|  | const uint16_t | length = `kWhirlpoolAcStateLength`
| ) |  |
| static

Verify the checksum is valid for a given state.

Parameters

  [in] | state | The array to verify the checksum of.
  [in] | length | The length/size of the array.

Returns
  true, if the state has a valid checksum. Otherwise, false.

## Member Data Documentation

## ◆ _

WhirlpoolProtocol IRWhirlpoolAc::_
| private

## ◆ _desiredtemp

uint8_t IRWhirlpoolAc::_desiredtemp
| private

The last user explicitly set temperature.

## ◆ _irsend

IRsend IRWhirlpoolAc::_irsend
| private

Instance of the IR send class.

The documentation for this class was generated from the following files:

- src/ir_Whirlpool.h
- src/ir_Whirlpool.cpp