IRremoteESP8266

Public Member Functions | Static Public Member Functions | Private Member Functions | Private Attributes | List of all members
IRTranscoldAc Class Reference

Class for handling detailed Transcold A/C messages. More...

`#include <ir_Transcold.h>`

Collaboration diagram for IRTranscoldAc:
[legend]

## Public Member Functions
| IRTranscoldAc (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | stateReset (void)
| Reset the internal state to a fixed known good state. More...
void | send (const uint16_t repeat=kTranscoldDefaultRepeat)
| Send the current internal state as an IR message. More...
int8_t | calibrate (void)
| Run the calibration to calculate uSec timing offsets for this platform. More...
void | begin (void)
| Set up hardware to be able to send a message. More...
void | on (void)
| Change the power setting to On. More...
void | off (void)
| Change the power setting to Off. More...
void | setPower (const bool state)
| Change the power setting. More...
bool | getPower (void) const
| Get the value of the current power setting. More...
void | setTemp (const uint8_t temp)
| Set the temperature. More...
uint8_t | getTemp (void) const
| Get the current temperature setting. More...
void | setFan (const uint8_t speed, const bool modecheck=true)
| Set the speed of the fan. More...
uint8_t | getFan (void) const
| Get the current fan speed setting. More...
void | setMode (const uint8_t mode)
| Set the operating mode of the A/C. More...
uint8_t | getMode (void) const
| Get the operating mode setting of the A/C. More...
void | setSwing (void)
| Toggle the Swing mode of the A/C. More...
bool | getSwing (void) const
| Get the Swing setting of the A/C. More...
uint32_t | getRaw (void) const
| Get a copy of the internal state as a valid code for this protocol. More...
void | setRaw (const uint32_t new_code)
| Set the internal state from a valid code for this protocol. More...
stdAc::state_t | toCommon (const stdAc::state_t *prev=NULL) const
| Convert the A/C state to it's common stdAc::state_t equivalent. More...
String | toString (void) const
| Convert the internal state into a human readable string. More...

## Static Public Member Functions
static uint8_t | convertMode (const stdAc::opmode_t mode)
| Convert a standard A/C mode into its native mode. More...
static uint8_t | convertFan (const stdAc::fanspeed_t speed)
| Convert a stdAc::fanspeed_t enum into it's native speed. More...
static stdAc::opmode_t | toCommonMode (const uint8_t mode)
| Convert a native mode to it's common stdAc::opmode_t equivalent. More...
static stdAc::fanspeed_t | toCommonFanSpeed (const uint8_t speed)
| Convert a native fan speed into its stdAc equivalent. More...

## Private Member Functions
bool | isSpecialState (void) const
| Is the current state is a special state? More...
bool | handleSpecialState (const uint32_t data)
| Adjust any internal settings based on the type of special state we are supplied. Does nothing if it isn't a special state. More...

## Private Attributes
IRsend | _irsend
| Instance of the IR send class. More...
bool | swingFlag
bool | swingHFlag
bool | swingVFlag
TranscoldProtocol | _
uint32_t | special_state
| special mode. More...

## Detailed Description

Class for handling detailed Transcold A/C messages.

## Constructor & Destructor Documentation

## ◆ IRTranscoldAc()

IRTranscoldAc::IRTranscoldAc | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |
| explicit

Class constructor.

Parameters

  [in] | pin | GPIO to be used when sending.
  [in] | inverted | Is the output signal to be inverted?
  [in] | use_modulation | Is frequency modulation to be used?

## Member Function Documentation

## ◆ begin()

void IRTranscoldAc::begin | ( | void |  | ) |

Set up hardware to be able to send a message.

## ◆ calibrate()

int8_t IRTranscoldAc::calibrate | ( | void |  | ) |
| inline

Run the calibration to calculate uSec timing offsets for this platform.

Returns
  The uSec timing offset needed per modulation of the IR Led.

Note
  This will produce a 65ms IR signal pulse at 38kHz. Only ever needs to be run once per object instantiation, if at all.

## ◆ convertFan()

uint8_t IRTranscoldAc::convertFan | ( | const stdAc::fanspeed_t | speed | ) |
| static

Convert a stdAc::fanspeed_t enum into it's native speed.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ convertMode()

uint8_t IRTranscoldAc::convertMode | ( | const stdAc::opmode_t | mode | ) |
| static

Convert a standard A/C mode into its native mode.

Parameters

  [in] | mode | A stdAc::opmode_t to be converted to it's native equivalent.

Returns
  The corresponding native mode.

## ◆ getFan()

uint8_t IRTranscoldAc::getFan | ( | void |  | ) | const

Get the current fan speed setting.

Returns
  The current fan speed.

## ◆ getMode()

uint8_t IRTranscoldAc::getMode | ( | void |  | ) | const

Get the operating mode setting of the A/C.

Returns
  The current operating mode setting.

## ◆ getPower()

bool IRTranscoldAc::getPower | ( | void |  | ) | const

Get the value of the current power setting.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getRaw()

uint32_t IRTranscoldAc::getRaw | ( | void |  | ) | const

Get a copy of the internal state as a valid code for this protocol.

Returns
  A valid code for this protocol based on the current internal state.

## ◆ getSwing()

bool IRTranscoldAc::getSwing | ( | void |  | ) | const

Get the Swing setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getTemp()

uint8_t IRTranscoldAc::getTemp | ( | void |  | ) | const

Get the current temperature setting.

Returns
  The current setting for temp. in degrees celsius.

## ◆ handleSpecialState()

bool IRTranscoldAc::handleSpecialState | ( | const uint32_t | data | ) |
| private

Adjust any internal settings based on the type of special state we are supplied. Does nothing if it isn't a special state.

Parameters

  [in] | data | The state we need to act upon.

Note
  Special state means commands that are not affecting Temperature/Mode/Fan

Returns
  true, if it is a special state. false if it isn't.

## ◆ isSpecialState()

bool IRTranscoldAc::isSpecialState | ( | void |  | ) | const
| private

Is the current state is a special state?

Returns
  true, if it is. false if it isn't.

## ◆ off()

void IRTranscoldAc::off | ( | void |  | ) |

Change the power setting to Off.

## ◆ on()

void IRTranscoldAc::on | ( | void |  | ) |

Change the power setting to On.

## ◆ send()

void IRTranscoldAc::send | ( | const uint16_t | repeat = `kTranscoldDefaultRepeat` | ) |

Send the current internal state as an IR message.

Parameters

  [in] | repeat | Nr. of times the message will be repeated.

## ◆ setFan()

void IRTranscoldAc::setFan | ( | const uint8_t | speed,
|  | const bool | modecheck = `true`
| ) |  |

Set the speed of the fan.

Parameters

  [in] | speed | The desired setting.
  [in] | modecheck | Do we enforce any mode limitations before setting?

## ◆ setMode()

void IRTranscoldAc::setMode | ( | const uint8_t | mode | ) |

Set the operating mode of the A/C.

Parameters

  [in] | mode | The desired operating mode.

## ◆ setPower()

void IRTranscoldAc::setPower | ( | const bool | on | ) |

Change the power setting.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setRaw()

void IRTranscoldAc::setRaw | ( | const uint32_t | new_code | ) |

Set the internal state from a valid code for this protocol.

Parameters

  [in] | new_code | A valid code for this protocol.

## ◆ setSwing()

void IRTranscoldAc::setSwing | ( | void |  | ) |

Toggle the Swing mode of the A/C.

## ◆ setTemp()

void IRTranscoldAc::setTemp | ( | const uint8_t | desired | ) |

Set the temperature.

Parameters

  [in] | desired | The temperature in degrees celsius.

## ◆ stateReset()

void IRTranscoldAc::stateReset | ( | void |  | ) |

Reset the internal state to a fixed known good state.

## ◆ toCommon()

stdAc::state_t IRTranscoldAc::toCommon | ( | const stdAc::state_t * | prev = `NULL` | ) | const

Convert the A/C state to it's common stdAc::state_t equivalent.

Parameters

  [in] | prev | Ptr to the previous state if required.

Returns
  A stdAc::state_t state.

## ◆ toCommonFanSpeed()

stdAc::fanspeed_t IRTranscoldAc::toCommonFanSpeed | ( | const uint8_t | speed | ) |
| static

Convert a native fan speed into its stdAc equivalent.

Parameters

  [in] | speed | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toCommonMode()

stdAc::opmode_t IRTranscoldAc::toCommonMode | ( | const uint8_t | mode | ) |
| static

Convert a native mode to it's common stdAc::opmode_t equivalent.

Parameters

  [in] | mode | A native operation mode to be converted.

Returns
  The corresponding common stdAc::opmode_t mode.

## ◆ toString()

String IRTranscoldAc::toString | ( | void |  | ) | const

Convert the internal state into a human readable string.

Returns
  The current internal state expressed as a human readable String.

## Member Data Documentation

## ◆ _

TranscoldProtocol IRTranscoldAc::_
| private

## ◆ _irsend

IRsend IRTranscoldAc::_irsend
| private

Instance of the IR send class.

## ◆ special_state

uint32_t IRTranscoldAc::special_state
| private

special mode.

## ◆ swingFlag

bool IRTranscoldAc::swingFlag
| private

## ◆ swingHFlag

bool IRTranscoldAc::swingHFlag
| private

## ◆ swingVFlag

bool IRTranscoldAc::swingVFlag
| private

The documentation for this class was generated from the following files:

- src/ir_Transcold.h
- src/ir_Transcold.cpp