IRremoteESP8266

Public Member Functions | Static Public Member Functions | Private Member Functions | Static Private Member Functions | Private Attributes | List of all members
IRMideaAC Class Reference

Class for handling detailed Midea A/C messages. More...

`#include <ir_Midea.h>`

Collaboration diagram for IRMideaAC:
[legend]

## Public Member Functions
| IRMideaAC (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | stateReset (void)
| Reset the state of the remote to a known good state/sequence. More...
void | send (const uint16_t repeat=kMideaMinRepeat)
| Send the current internal state as an IR message. More...
int8_t | calibrate (void)
| Run the calibration to calculate uSec timing offsets for this platform. More...
void | begin (void)
| Set up hardware to be able to send a message. More...
void | on (void)
| Set the requested power state of the A/C to on. More...
void | off (void)
| Set the requested power state of the A/C to off. More...
void | setPower (const bool on)
| Change the power setting. More...
bool | getPower (void) const
| Get the value of the current power setting. More...
bool | getUseCelsius (void) const
| Is the device currently using Celsius or the Fahrenheit temp scale? More...
void | setUseCelsius (const bool celsius)
| Set the A/C unit to use Celsius natively. More...
void | setTemp (const uint8_t temp, const bool useCelsius=false)
| Set the temperature. More...
uint8_t | getTemp (const bool useCelsius=false) const
| Get the current temperature setting. More...
void | setSensorTemp (const uint8_t temp, const bool useCelsius=false)
| Set the Sensor temperature. More...
uint8_t | getSensorTemp (const bool useCelsius=false) const
| Get the current Sensor temperature setting. More...
void | setEnableSensorTemp (const bool on)
| Enable the remote's Sensor temperature. More...
bool | getEnableSensorTemp (void) const
| Is the remote temperature sensor enabled? More...
void | setFan (const uint8_t fan)
| Set the speed of the fan. More...
uint8_t | getFan (void) const
| Get the current fan speed setting. More...
void | setMode (const uint8_t mode)
| Set the operating mode of the A/C. More...
uint8_t | getMode (void) const
| Get the operating mode setting of the A/C. More...
void | setRaw (const uint64_t newState)
| Set the internal state from a valid code for this protocol. More...
uint64_t | getRaw (void)
| Get a copy of the internal state/code for this protocol. More...
void | setSleep (const bool on)
| Set the Sleep setting of the A/C. More...
bool | getSleep (void) const
| Get the Sleep setting of the A/C. More...
bool | isSwingVToggle (void) const
| Is the current state a vertical swing toggle message? More...
void | setSwingVToggle (const bool on)
| Set the A/C to toggle the vertical swing toggle for the next send. More...
bool | getSwingVToggle (void)
bool | isSwingVStep (void) const
| Is the current state a step vertical swing message? More...
void | setSwingVStep (const bool on)
| Set the A/C to step the vertical swing for the next send. More...
bool | getSwingVStep (void)
bool | isEconoToggle (void) const
| Is the current state an Econo (energy saver) toggle message? More...
void | setEconoToggle (const bool on)
| Set the A/C to toggle the Econo (energy saver) mode for the next send. More...
bool | getEconoToggle (void)
bool | isTurboToggle (void) const
| Is the current state a Turbo toggle message? More...
void | setTurboToggle (const bool on)
| Set the A/C to toggle the Turbo mode for the next send. More...
bool | getTurboToggle (void)
bool | isLightToggle (void) const
| Is the current state a Light (LED) toggle message? More...
void | setLightToggle (const bool on)
| Set the A/C to toggle the Light (LED) mode for the next send. More...
bool | getLightToggle (void)
bool | isCleanToggle (void) const
| Is the current state a Self-Clean toggle message? More...
void | setCleanToggle (const bool on)
| Set the A/C to toggle the Self Clean mode for the next send. More...
bool | getCleanToggle (void)
bool | is8CHeatToggle (void) const
| Is the current state a 8C Heat (Freeze Protect) toggle message? More...
void | set8CHeatToggle (const bool on)
| Set the A/C to toggle the 8C Heat (Freeze Protect) mode for the next send. More...
bool | get8CHeatToggle (void)
bool | isQuiet (void) const
| Is the current state a Quiet(Silent) message? More...
void | setQuiet (const bool on)
| Set the Quiet (Silent) mode for the next send. More...
void | setQuiet (const bool on, const bool prev)
| Set the Quiet (Silent) mode for the next send. More...
bool | getQuiet (void) const
uint8_t | getType (void) const
| Get the message type setting of the A/C message. More...
bool | isOnTimerEnabled (void) const
| Is the OnTimer enabled? More...
uint16_t | getOnTimer (void) const
| Get the value of the OnTimer is currently set to. More...
void | setOnTimer (const uint16_t mins)
| Set the value of the On Timer. More...
bool | isOffTimerEnabled (void) const
| Is the OffTimer enabled? More...
uint16_t | getOffTimer (void) const
| Get the value of the OffTimer is currently set to. More...
void | setOffTimer (const uint16_t mins)
| Set the value of the Off Timer. More...
stdAc::state_t | toCommon (const stdAc::state_t *prev=NULL)
| Convert the current internal state into its stdAc::state_t equivalent. More...
String | toString (void)
| Convert the current internal state into a human readable string. More...

## Static Public Member Functions
static bool | validChecksum (const uint64_t state)
| Verify the checksum is valid for a given state. More...
static uint8_t | convertMode (const stdAc::opmode_t mode)
| Convert a stdAc::opmode_t enum into its native mode. More...
static uint8_t | convertFan (const stdAc::fanspeed_t speed)
| Convert a stdAc::fanspeed_t enum into it's native speed. More...
static stdAc::opmode_t | toCommonMode (const uint8_t mode)
| Convert a native mode into its stdAc equivalent. More...
static stdAc::fanspeed_t | toCommonFanSpeed (const uint8_t speed)
| Convert a native fan speed into its stdAc equivalent. More...

## Private Member Functions
void | checksum (void)
| Calculate & set the checksum for the current internal state of the remote. More...
void | setType (const uint8_t type)
| Set the message type setting of the A/C message. More...

## Static Private Member Functions
static uint8_t | calcChecksum (const uint64_t state)
| Calculate the checksum for a given state. More...

## Private Attributes
IRsend | _irsend
| Instance of the IR send class. More...
MideaProtocol | _
bool | _CleanToggle
bool | _EconoToggle
bool | _8CHeatToggle
bool | _LightToggle
bool | _Quiet
bool | _Quiet_prev
bool | _SwingVToggle
bool | _SwingVStep
bool | _TurboToggle

## Detailed Description

Class for handling detailed Midea A/C messages.

Warning
  Consider this very alpha code.

## Constructor & Destructor Documentation

## ◆ IRMideaAC()

IRMideaAC::IRMideaAC | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |
| explicit

Class constructor.

Parameters

  [in] | pin | GPIO to be used when sending.
  [in] | inverted | Is the output signal to be inverted?
  [in] | use_modulation | Is frequency modulation to be used?

## Member Function Documentation

## ◆ begin()

void IRMideaAC::begin | ( | void |  | ) |

Set up hardware to be able to send a message.

## ◆ calcChecksum()

uint8_t IRMideaAC::calcChecksum | ( | const uint64_t | state | ) |
| static private

Calculate the checksum for a given state.

Parameters

  [in] | state | The value to calc the checksum of.

Returns
  The calculated checksum value.

## ◆ calibrate()

int8_t IRMideaAC::calibrate | ( | void |  | ) |
| inline

Run the calibration to calculate uSec timing offsets for this platform.

Returns
  The uSec timing offset needed per modulation of the IR Led.

Note
  This will produce a 65ms IR signal pulse at 38kHz. Only ever needs to be run once per object instantiation, if at all.

## ◆ checksum()

void IRMideaAC::checksum | ( | void |  | ) |
| private

Calculate & set the checksum for the current internal state of the remote.

## ◆ convertFan()

uint8_t IRMideaAC::convertFan | ( | const stdAc::fanspeed_t | speed | ) |
| static

Convert a stdAc::fanspeed_t enum into it's native speed.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ convertMode()

uint8_t IRMideaAC::convertMode | ( | const stdAc::opmode_t | mode | ) |
| static

Convert a stdAc::opmode_t enum into its native mode.

Parameters

  [in] | mode | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ get8CHeatToggle()

bool IRMideaAC::get8CHeatToggle | ( | void |  | ) |

Returns
  true, the setting is on. false, the setting is off.

## ◆ getCleanToggle()

bool IRMideaAC::getCleanToggle | ( | void |  | ) |

Returns
  true, the setting is on. false, the setting is off.

## ◆ getEconoToggle()

bool IRMideaAC::getEconoToggle | ( | void |  | ) |

Returns
  true, the setting is on. false, the setting is off.

## ◆ getEnableSensorTemp()

bool IRMideaAC::getEnableSensorTemp | ( | void |  | ) | const

Is the remote temperature sensor enabled?

Returns
  A boolean indicating if it is enabled or not.

Note
  Also known as FollowMe

## ◆ getFan()

uint8_t IRMideaAC::getFan | ( | void |  | ) | const

Get the current fan speed setting.

Returns
  The current fan speed.

## ◆ getLightToggle()

bool IRMideaAC::getLightToggle | ( | void |  | ) |

Returns
  true, the setting is on. false, the setting is off.

## ◆ getMode()

uint8_t IRMideaAC::getMode | ( | void |  | ) | const

Get the operating mode setting of the A/C.

Returns
  The current operating mode setting.

## ◆ getOffTimer()

uint16_t IRMideaAC::getOffTimer | ( | void |  | ) | const

Get the value of the OffTimer is currently set to.

Returns
  The number of minutes.

## ◆ getOnTimer()

uint16_t IRMideaAC::getOnTimer | ( | void |  | ) | const

Get the value of the OnTimer is currently set to.

Returns
  The number of minutes.

## ◆ getPower()

bool IRMideaAC::getPower | ( | void |  | ) | const

Get the value of the current power setting.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getQuiet()

bool IRMideaAC::getQuiet | ( | void |  | ) | const

Returns
  true, the setting is on. false, the setting is off.

## ◆ getRaw()

uint64_t IRMideaAC::getRaw | ( | void |  | ) |

Get a copy of the internal state/code for this protocol.

Returns
  The code for this protocol based on the current internal state.

## ◆ getSensorTemp()

uint8_t IRMideaAC::getSensorTemp | ( | const bool | celsius = `false` | ) | const

Get the current Sensor temperature setting.

Parameters

  [in] | celsius | true, the results are in Celsius. false, in Fahrenheit.

Returns
  The current setting for temp. in the requested units/scale.

Note
  Also known as FollowMe

## ◆ getSleep()

bool IRMideaAC::getSleep | ( | void |  | ) | const

Get the Sleep setting of the A/C.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getSwingVStep()

bool IRMideaAC::getSwingVStep | ( | void |  | ) |

Returns
  true, the setting is on. false, the setting is off.

## ◆ getSwingVToggle()

bool IRMideaAC::getSwingVToggle | ( | void |  | ) |

Note
  On Danby A/C units, this is associated with the Ion Filter instead.

Returns
  true, the setting is on. false, the setting is off.

## ◆ getTemp()

uint8_t IRMideaAC::getTemp | ( | const bool | celsius = `false` | ) | const

Get the current temperature setting.

Parameters

  [in] | celsius | true, the results are in Celsius. false, in Fahrenheit.

Returns
  The current setting for temp. in the requested units/scale.

## ◆ getTurboToggle()

bool IRMideaAC::getTurboToggle | ( | void |  | ) |

Returns
  true, the setting is on. false, the setting is off.

## ◆ getType()

uint8_t IRMideaAC::getType | ( | void |  | ) | const

Get the message type setting of the A/C message.

Returns
  The message type setting.

## ◆ getUseCelsius()

bool IRMideaAC::getUseCelsius | ( | void |  | ) | const

Is the device currently using Celsius or the Fahrenheit temp scale?

Returns
  true, the A/C unit uses Celsius natively, false, is Fahrenheit.

## ◆ is8CHeatToggle()

bool IRMideaAC::is8CHeatToggle | ( | void |  | ) | const

Is the current state a 8C Heat (Freeze Protect) toggle message?

Note
  Only works in Heat mode.

Returns
  true, it is. false, it isn't.

## ◆ isCleanToggle()

bool IRMideaAC::isCleanToggle | ( | void |  | ) | const

Is the current state a Self-Clean toggle message?

Returns
  true, it is. false, it isn't.

## ◆ isEconoToggle()

bool IRMideaAC::isEconoToggle | ( | void |  | ) | const

Is the current state an Econo (energy saver) toggle message?

Returns
  true, it is. false, it isn't.

## ◆ isLightToggle()

bool IRMideaAC::isLightToggle | ( | void |  | ) | const

Is the current state a Light (LED) toggle message?

Returns
  true, it is. false, it isn't.

## ◆ isOffTimerEnabled()

bool IRMideaAC::isOffTimerEnabled | ( | void |  | ) | const

Is the OffTimer enabled?

Returns
  true for yes, false for no.

## ◆ isOnTimerEnabled()

bool IRMideaAC::isOnTimerEnabled | ( | void |  | ) | const

Is the OnTimer enabled?

Returns
  true for yes, false for no.

## ◆ isQuiet()

bool IRMideaAC::isQuiet | ( | void |  | ) | const

Is the current state a Quiet(Silent) message?

Returns
  true, it is. false, it isn't.

## ◆ isSwingVStep()

bool IRMideaAC::isSwingVStep | ( | void |  | ) | const

Is the current state a step vertical swing message?

Returns
  true, it is. false, it isn't.

## ◆ isSwingVToggle()

bool IRMideaAC::isSwingVToggle | ( | void |  | ) | const

Is the current state a vertical swing toggle message?

Note
  On Danby A/C units, this is associated with the Ion Filter instead.

Returns
  true, it is. false, it isn't.

## ◆ isTurboToggle()

bool IRMideaAC::isTurboToggle | ( | void |  | ) | const

Is the current state a Turbo toggle message?

Returns
  true, it is. false, it isn't.

## ◆ off()

void IRMideaAC::off | ( | void |  | ) |

Set the requested power state of the A/C to off.

## ◆ on()

void IRMideaAC::on | ( | void |  | ) |

Set the requested power state of the A/C to on.

## ◆ send()

void IRMideaAC::send | ( | const uint16_t | repeat = `kMideaMinRepeat` | ) |

Send the current internal state as an IR message.

Parameters

  [in] | repeat | Nr. of times the message will be repeated.

## ◆ set8CHeatToggle()

void IRMideaAC::set8CHeatToggle | ( | const bool | on | ) |

Set the A/C to toggle the 8C Heat (Freeze Protect) mode for the next send.

Note
  Only works in Heat mode.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setCleanToggle()

void IRMideaAC::setCleanToggle | ( | const bool | on | ) |

Set the A/C to toggle the Self Clean mode for the next send.

Note
  Only works in Cool, Dry, or Auto modes.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setEconoToggle()

void IRMideaAC::setEconoToggle | ( | const bool | on | ) |

Set the A/C to toggle the Econo (energy saver) mode for the next send.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setEnableSensorTemp()

void IRMideaAC::setEnableSensorTemp | ( | const bool | on | ) |

Enable the remote's Sensor temperature.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

Note
  Also known as FollowMe

## ◆ setFan()

void IRMideaAC::setFan | ( | const uint8_t | fan | ) |

Set the speed of the fan.

Parameters

  [in] | fan | The desired setting. 1-3 set the speed, 0 for auto.

## ◆ setLightToggle()

void IRMideaAC::setLightToggle | ( | const bool | on | ) |

Set the A/C to toggle the Light (LED) mode for the next send.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setMode()

void IRMideaAC::setMode | ( | const uint8_t | mode | ) |

Set the operating mode of the A/C.

Parameters

  [in] | mode | The desired operating mode.

## ◆ setOffTimer()

void IRMideaAC::setOffTimer | ( | const uint16_t | mins | ) |

Set the value of the Off Timer.

Parameters

  [in] | mins | The number of minutes for the timer.

Note
  Time will be rounded down to nearest 30 min as that is the resolution of the actual device/protocol.
  A value of less than 30 will disable the Timer.

## ◆ setOnTimer()

void IRMideaAC::setOnTimer | ( | const uint16_t | mins | ) |

Set the value of the On Timer.

Parameters

  [in] | mins | The number of minutes for the timer.

Note
  Time will be rounded down to nearest 30 min as that is the resolution of the actual device/protocol.
  A value of less than 30 will disable the Timer.

Warning
  On Timer is incompatible with Sensor Temp/Follow Me messages. Setting it will disable that mode/settings.

## ◆ setPower()

void IRMideaAC::setPower | ( | const bool | on | ) |

Change the power setting.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setQuiet() [1/2]

void IRMideaAC::setQuiet | ( | const bool | on | ) |

Set the Quiet (Silent) mode for the next send.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setQuiet() [2/2]

void IRMideaAC::setQuiet | ( | const bool | on,
|  | const bool | prev
| ) |  |

Set the Quiet (Silent) mode for the next send.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.
  [in] | prev | true, previously the setting was on. false, setting was off.

## ◆ setRaw()

void IRMideaAC::setRaw | ( | const uint64_t | newState | ) |

Set the internal state from a valid code for this protocol.

Parameters

  [in] | newState | A valid code for this protocol.

## ◆ setSensorTemp()

void IRMideaAC::setSensorTemp | ( | const uint8_t | temp,
|  | const bool | useCelsius = `false`
| ) |  |

Set the Sensor temperature.

Parameters

  [in] | temp | The temperature in degrees celsius.
  [in] | useCelsius | true, use the Celsius temp scale. false, is Fahrenheit

Note
  Also known as FollowMe

## ◆ setSleep()

void IRMideaAC::setSleep | ( | const bool | on | ) |

Set the Sleep setting of the A/C.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setSwingVStep()

void IRMideaAC::setSwingVStep | ( | const bool | on | ) |

Set the A/C to step the vertical swing for the next send.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setSwingVToggle()

void IRMideaAC::setSwingVToggle | ( | const bool | on | ) |

Set the A/C to toggle the vertical swing toggle for the next send.

Note
  On Danby A/C units, this is associated with the Ion Filter instead.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setTemp()

void IRMideaAC::setTemp | ( | const uint8_t | temp,
|  | const bool | useCelsius = `false`
| ) |  |

Set the temperature.

Parameters

  [in] | temp | The temperature in degrees celsius.
  [in] | useCelsius | true, use the Celsius temp scale. false, is Fahrenheit

## ◆ setTurboToggle()

void IRMideaAC::setTurboToggle | ( | const bool | on | ) |

Set the A/C to toggle the Turbo mode for the next send.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ setType()

void IRMideaAC::setType | ( | const uint8_t | setting | ) |
| private

Set the message type setting of the A/C message.

Parameters

  [in] | setting | The desired message type setting.

## ◆ setUseCelsius()

void IRMideaAC::setUseCelsius | ( | const bool | on | ) |

Set the A/C unit to use Celsius natively.

Parameters

  [in] | on | true, the setting is on. false, the setting is off.

## ◆ stateReset()

void IRMideaAC::stateReset | ( | void |  | ) |

Reset the state of the remote to a known good state/sequence.

## ◆ toCommon()

stdAc::state_t IRMideaAC::toCommon | ( | const stdAc::state_t * | prev = `NULL` | ) |

Convert the current internal state into its stdAc::state_t equivalent.

Parameters

  [in] | prev | A Ptr to the previous state.

Returns
  The stdAc equivalent of the native settings.

## ◆ toCommonFanSpeed()

stdAc::fanspeed_t IRMideaAC::toCommonFanSpeed | ( | const uint8_t | speed | ) |
| static

Convert a native fan speed into its stdAc equivalent.

Parameters

  [in] | speed | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toCommonMode()

stdAc::opmode_t IRMideaAC::toCommonMode | ( | const uint8_t | mode | ) |
| static

Convert a native mode into its stdAc equivalent.

Parameters

  [in] | mode | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toString()

String IRMideaAC::toString | ( | void |  | ) |

Convert the current internal state into a human readable string.

Returns
  A human readable string.

## ◆ validChecksum()

bool IRMideaAC::validChecksum | ( | const uint64_t | state | ) |
| static

Verify the checksum is valid for a given state.

Parameters

  [in] | state | The state to verify the checksum of.

Returns
  true, if the state has a valid checksum. Otherwise, false.

## Member Data Documentation

## ◆ _

MideaProtocol IRMideaAC::_
| private

## ◆ _8CHeatToggle

bool IRMideaAC::_8CHeatToggle
| private

## ◆ _CleanToggle

bool IRMideaAC::_CleanToggle
| private

## ◆ _EconoToggle

bool IRMideaAC::_EconoToggle
| private

## ◆ _irsend

IRsend IRMideaAC::_irsend
| private

Instance of the IR send class.

## ◆ _LightToggle

bool IRMideaAC::_LightToggle
| private

## ◆ _Quiet

bool IRMideaAC::_Quiet
| private

## ◆ _Quiet_prev

bool IRMideaAC::_Quiet_prev
| private

## ◆ _SwingVStep

bool IRMideaAC::_SwingVStep
| private

## ◆ _SwingVToggle

bool IRMideaAC::_SwingVToggle
| private

## ◆ _TurboToggle

bool IRMideaAC::_TurboToggle
| private

The documentation for this class was generated from the following files:

- src/ir_Midea.h
- src/ir_Midea.cpp