IRremoteESP8266

Public Attributes | List of all members
AmcorProtocol Union Reference

Native representation of a Amcor A/C message. More...

`#include <ir_Amcor.h>`

## Public Attributes
uint8_t | raw [kAmcorStateLength]
struct {
uint8_t __pad0__:8
uint8_t Mode:3
uint8_t __pad1__:1
uint8_t Fan:3
uint8_t __pad2__:1
uint8_t __pad3__:1
uint8_t Temp:6
uint8_t __pad4__:1
uint8_t __pad5__:8
uint8_t __pad6__:8
uint8_t __pad7__:4
uint8_t Power:4
uint8_t Max:2
uint8_t __pad8__:4
uint8_t Vent:2
uint8_t Sum:8
}; |

## Detailed Description

Native representation of a Amcor A/C message.

## Member Data Documentation

## ◆ @5

struct { ... }

## ◆ __pad0__

uint8_t AmcorProtocol::__pad0__

## ◆ __pad1__

uint8_t AmcorProtocol::__pad1__

## ◆ __pad2__

uint8_t AmcorProtocol::__pad2__

## ◆ __pad3__

uint8_t AmcorProtocol::__pad3__

## ◆ __pad4__

uint8_t AmcorProtocol::__pad4__

## ◆ __pad5__

uint8_t AmcorProtocol::__pad5__

## ◆ __pad6__

uint8_t AmcorProtocol::__pad6__

## ◆ __pad7__

uint8_t AmcorProtocol::__pad7__

## ◆ __pad8__

uint8_t AmcorProtocol::__pad8__

## ◆ Fan

uint8_t AmcorProtocol::Fan

## ◆ Max

uint8_t AmcorProtocol::Max

## ◆ Mode

uint8_t AmcorProtocol::Mode

## ◆ Power

uint8_t AmcorProtocol::Power

## ◆ raw

uint8_t AmcorProtocol::raw[kAmcorStateLength]

## ◆ Sum

uint8_t AmcorProtocol::Sum

## ◆ Temp

uint8_t AmcorProtocol::Temp

## ◆ Vent

uint8_t AmcorProtocol::Vent

The documentation for this union was generated from the following file:

- src/ir_Amcor.h