IRremoteESP8266

Public Attributes | List of all members
HaierAc176Protocol Union Reference

Native representation of a Haier 176 bit A/C message. More...

`#include <ir_Haier.h>`

## Public Attributes
uint8_t | raw [kHaierAC176StateLength]
| The state in native form. More...
struct {
uint8_t Model:8
uint8_t SwingV:4
uint8_t Temp:4
uint8_t __pad0__:5
uint8_t SwingH:3
uint8_t __pad1__:1
uint8_t Health:1
uint8_t __pad2__:3
uint8_t TimerMode:3
uint8_t __pad3__:6
uint8_t Power:1
uint8_t __pad4__:1
uint8_t OffTimerHrs:5
uint8_t Fan:3
uint8_t OffTimerMins:6
uint8_t Turbo:1
uint8_t Quiet:1
uint8_t OnTimerHrs:5
uint8_t Mode:3
uint8_t OnTimerMins:6
uint8_t __pad5__:1
uint8_t Sleep:1
uint8_t __pad6__:8
uint8_t ExtraDegreeF:1
uint8_t __pad7__:4
uint8_t UseFahrenheit:1
uint8_t __pad8__:2
uint8_t __pad9__:8
uint8_t Button:5
uint8_t Lock:1
uint8_t __pad10__:2
uint8_t Sum:8
uint8_t Prefix2:8
uint8_t __pad11__:8
uint8_t __pad12__:6
uint8_t Fan2:2
uint8_t __pad13__:8
uint8_t __pad14__:8
uint8_t __pad15__:8
uint8_t __pad16__:8
uint8_t Sum2:8
}; |

## Detailed Description

Native representation of a Haier 176 bit A/C message.

## Member Data Documentation

## ◆ @57

struct { ... }

## ◆ __pad0__

uint8_t HaierAc176Protocol::__pad0__

## ◆ __pad10__

uint8_t HaierAc176Protocol::__pad10__

## ◆ __pad11__

uint8_t HaierAc176Protocol::__pad11__

## ◆ __pad12__

uint8_t HaierAc176Protocol::__pad12__

## ◆ __pad13__

uint8_t HaierAc176Protocol::__pad13__

## ◆ __pad14__

uint8_t HaierAc176Protocol::__pad14__

## ◆ __pad15__

uint8_t HaierAc176Protocol::__pad15__

## ◆ __pad16__

uint8_t HaierAc176Protocol::__pad16__

## ◆ __pad1__

uint8_t HaierAc176Protocol::__pad1__

## ◆ __pad2__

uint8_t HaierAc176Protocol::__pad2__

## ◆ __pad3__

uint8_t HaierAc176Protocol::__pad3__

## ◆ __pad4__

uint8_t HaierAc176Protocol::__pad4__

## ◆ __pad5__

uint8_t HaierAc176Protocol::__pad5__

## ◆ __pad6__

uint8_t HaierAc176Protocol::__pad6__

## ◆ __pad7__

uint8_t HaierAc176Protocol::__pad7__

## ◆ __pad8__

uint8_t HaierAc176Protocol::__pad8__

## ◆ __pad9__

uint8_t HaierAc176Protocol::__pad9__

## ◆ Button

uint8_t HaierAc176Protocol::Button

## ◆ ExtraDegreeF

uint8_t HaierAc176Protocol::ExtraDegreeF

## ◆ Fan

uint8_t HaierAc176Protocol::Fan

## ◆ Fan2

uint8_t HaierAc176Protocol::Fan2

## ◆ Health

uint8_t HaierAc176Protocol::Health

## ◆ Lock

uint8_t HaierAc176Protocol::Lock

## ◆ Mode

uint8_t HaierAc176Protocol::Mode

## ◆ Model

uint8_t HaierAc176Protocol::Model

## ◆ OffTimerHrs

uint8_t HaierAc176Protocol::OffTimerHrs

## ◆ OffTimerMins

uint8_t HaierAc176Protocol::OffTimerMins

## ◆ OnTimerHrs

uint8_t HaierAc176Protocol::OnTimerHrs

## ◆ OnTimerMins

uint8_t HaierAc176Protocol::OnTimerMins

## ◆ Power

uint8_t HaierAc176Protocol::Power

## ◆ Prefix2

uint8_t HaierAc176Protocol::Prefix2

## ◆ Quiet

uint8_t HaierAc176Protocol::Quiet

## ◆ raw

uint8_t HaierAc176Protocol::raw[kHaierAC176StateLength]

The state in native form.

## ◆ Sleep

uint8_t HaierAc176Protocol::Sleep

## ◆ Sum

uint8_t HaierAc176Protocol::Sum

## ◆ Sum2

uint8_t HaierAc176Protocol::Sum2

## ◆ SwingH

uint8_t HaierAc176Protocol::SwingH

## ◆ SwingV

uint8_t HaierAc176Protocol::SwingV

## ◆ Temp

uint8_t HaierAc176Protocol::Temp

## ◆ TimerMode

uint8_t HaierAc176Protocol::TimerMode

## ◆ Turbo

uint8_t HaierAc176Protocol::Turbo

## ◆ UseFahrenheit

uint8_t HaierAc176Protocol::UseFahrenheit

The documentation for this union was generated from the following file:

- src/ir_Haier.h