IRremoteESP8266

IRrecv Member List

This is the complete list of members for IRrecv, including all inherited members.

_getParamsPtr(void) | IRrecv | private
_matchGeneric(volatile uint16_t *data_ptr, uint64_t *result_bits_ptr, uint8_t *result_ptr, const bool use_bits, const uint16_t remaining, const uint16_t required, const uint16_t hdrmark, const uint32_t hdrspace, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint16_t footermark, const uint32_t footerspace, const bool atleast=false, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true) | IRrecv | private
_timer_num | IRrecv | private
_tolerance | IRrecv | private
_unknown_threshold | IRrecv | private
_validTolerance(const uint8_t percentage) | IRrecv | private
compare(const uint16_t oldval, const uint16_t newval) | IRrecv | private
copyIrParams(volatile irparams_t *src, irparams_t *dst) | IRrecv | private
crudeNoiseFilter(decode_results *results, const uint16_t floor=0) | IRrecv | private
decode(decode_results *results, irparams_t *save=NULL, uint8_t max_skip=0, uint16_t noise_floor=0) | IRrecv |
decodeAirton(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kAirtonBits, const bool strict=true) | IRrecv | private
decodeAirwell(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kAirwellBits, const bool strict=true) | IRrecv | private
decodeAiwaRCT501(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kAiwaRcT501Bits, const bool strict=true) | IRrecv | private
decodeAmcor(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kAmcorBits, const bool strict=true) | IRrecv | private
decodeArgo(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kArgoBits, const bool strict=true) | IRrecv | private
decodeArgoWREM3(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kArgo3AcControlStateLength *8, const bool strict=true) | IRrecv | private
decodeArris(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kArrisBits, const bool strict=true) | IRrecv | private
decodeBosch144(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kBosch144Bits, const bool strict=true) | IRrecv | private
decodeBose(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kBoseBits, const bool strict=true) | IRrecv | private
decodeCarrierAC(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCarrierAcBits, const bool strict=true) | IRrecv | private
decodeCarrierAC128(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCarrierAc128Bits, const bool strict=true) | IRrecv | private
decodeCarrierAC40(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCarrierAc40Bits, const bool strict=true) | IRrecv | private
decodeCarrierAC64(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCarrierAc64Bits, const bool strict=true) | IRrecv | private
decodeCarrierAC84(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCarrierAc84Bits, const bool strict=true) | IRrecv | private
decodeClimaButler(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kClimaButlerBits, const bool strict=true) | IRrecv | private
decodeCOOLIX(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCoolixBits, const bool strict=true) | IRrecv | private
decodeCoolix48(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCoolix48Bits, const bool strict=true) | IRrecv | private
decodeCoronaAc(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kCoronaAcBitsShort, const bool strict=true) | IRrecv | private
decodeDaikin(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikinBits, const bool strict=true) | IRrecv | private
decodeDaikin128(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin128Bits, const bool strict=true) | IRrecv | private
decodeDaikin152(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin152Bits, const bool strict=true) | IRrecv | private
decodeDaikin160(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin160Bits, const bool strict=true) | IRrecv | private
decodeDaikin176(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin176Bits, const bool strict=true) | IRrecv | private
decodeDaikin2(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin2Bits, const bool strict=true) | IRrecv | private
decodeDaikin200(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin200Bits, const bool strict=true) | IRrecv | private
decodeDaikin216(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin216Bits, const bool strict=true) | IRrecv | private
decodeDaikin312(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin312Bits, const bool strict=true) | IRrecv | private
decodeDaikin64(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDaikin64Bits, const bool strict=true) | IRrecv | private
decodeDelonghiAc(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDelonghiAcBits, const bool strict=true) | IRrecv | private
decodeDenon(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDenonBits, const bool strict=true) | IRrecv | private
decodeDISH(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDishBits, const bool strict=true) | IRrecv | private
decodeDoshisha(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kDoshishaBits, const bool strict=true) | IRrecv | private
decodeEcoclim(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kEcoclimBits, const bool strict=true) | IRrecv | private
decodeElectraAC(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kElectraAcBits, const bool strict=true) | IRrecv | private
decodeElitescreens(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kEliteScreensBits, const bool strict=true) | IRrecv | private
decodeEpson(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kEpsonBits, const bool strict=true) | IRrecv | private
decodeFujitsuAC(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kFujitsuAcBits, const bool strict=false) | IRrecv | private
decodeGICable(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kGicableBits, const bool strict=true) | IRrecv | private
decodeGoodweather(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kGoodweatherBits, const bool strict=true) | IRrecv | private
decodeGorenje(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kGorenjeBits, const bool strict=true) | IRrecv | private
decodeGree(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kGreeBits, const bool strict=true) | IRrecv | private
decodeHaierAC(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHaierACBits, const bool strict=true) | IRrecv | private
decodeHaierAC160(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHaierAC160Bits, const bool strict=true) | IRrecv | private
decodeHaierAC176(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHaierAC176Bits, const bool strict=true) | IRrecv | private
decodeHaierACYRW02(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHaierACYRW02Bits, const bool strict=true) | IRrecv | private
decodeHash(decode_results *results) | IRrecv | private
decodeHitachiAC(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHitachiAcBits, const bool strict=true, const bool MSBfirst=true) | IRrecv | private
decodeHitachiAC1(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHitachiAc1Bits, const bool strict=true) | IRrecv | private
decodeHitachiAc296(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHitachiAc296Bits, const bool strict=true) | IRrecv | private
decodeHitachiAc3(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHitachiAc3Bits, const bool strict=true) | IRrecv | private
decodeHitachiAc424(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kHitachiAc424Bits, const bool strict=true) | IRrecv | private
decodeInax(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kInaxBits, const bool strict=true) | IRrecv | private
decodeJVC(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kJvcBits, const bool strict=true) | IRrecv | private
decodeKelon(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kKelonBits, const bool strict=true) | IRrecv | private
decodeKelon168(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kKelon168Bits, const bool strict=true) | IRrecv | private
decodeKelvinator(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kKelvinatorBits, const bool strict=true) | IRrecv | private
decodeLasertag(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kLasertagBits, const bool strict=true) | IRrecv | private
decodeLegoPf(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kLegoPfBits, const bool strict=true) | IRrecv | private
decodeLG(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kLgBits, const bool strict=false) | IRrecv | private
decodeLutron(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kLutronBits, const bool strict=true) | IRrecv | private
decodeMagiQuest(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMagiquestBits, const bool strict=true) | IRrecv | private
decodeMetz(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMetzBits, const bool strict=true) | IRrecv | private
decodeMidea(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMideaBits, const bool strict=true) | IRrecv | private
decodeMidea24(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMidea24Bits, const bool strict=true) | IRrecv | private
decodeMilestag2(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMilesTag2ShotBits, const bool strict=true) | IRrecv | private
decodeMirage(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMirageBits, const bool strict=true) | IRrecv | private
decodeMitsubishi(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMitsubishiBits, const bool strict=true) | IRrecv | private
decodeMitsubishi112(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMitsubishi112Bits, const bool strict=true) | IRrecv | private
decodeMitsubishi136(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMitsubishi136Bits, const bool strict=true) | IRrecv | private
decodeMitsubishi2(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMitsubishiBits, const bool strict=true) | IRrecv | private
decodeMitsubishiAC(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMitsubishiACBits, const bool strict=false) | IRrecv | private
decodeMitsubishiHeavy(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMitsubishiHeavy152Bits, const bool strict=true) | IRrecv | private
decodeMultibrackets(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kMultibracketsBits, const bool strict=true) | IRrecv | private
decodeMWM(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=24, const bool strict=true) | IRrecv | private
decodeNEC(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kNECBits, const bool strict=true) | IRrecv | private
decodeNeoclima(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kNeoclimaBits, const bool strict=true) | IRrecv | private
decodeNikai(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kNikaiBits, const bool strict=true) | IRrecv | private
decodePanasonic(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kPanasonicBits, const bool strict=false, const uint32_t manufacturer=kPanasonicManufacturer) | IRrecv | private
decodePanasonicAC(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kPanasonicAcBits, const bool strict=true) | IRrecv | private
decodePanasonicAC32(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kPanasonicAc32Bits, const bool strict=true) | IRrecv | private
decodePioneer(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kPioneerBits, const bool strict=true) | IRrecv | private
decodeRC5(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kRC5XBits, const bool strict=true) | IRrecv | private
decodeRC6(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kRC6Mode0Bits, const bool strict=false) | IRrecv | private
decodeRCMM(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kRCMMBits, const bool strict=false) | IRrecv | private
decodeRhoss(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kRhossBits, const bool strict=true) | IRrecv | private
decodeSAMSUNG(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSamsungBits, const bool strict=true) | IRrecv | private
decodeSamsung36(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSamsung36Bits, const bool strict=true) | IRrecv | private
decodeSamsungAC(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSamsungAcBits, const bool strict=true) | IRrecv | private
decodeSanyoAc(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSanyoAcBits, const bool strict=true) | IRrecv | private
decodeSanyoAc152(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSanyoAc152Bits, const bool strict=true) | IRrecv | private
decodeSanyoAc88(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSanyoAc88Bits, const bool strict=true) | IRrecv | private
decodeSanyoLC7461(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSanyoLC7461Bits, const bool strict=true) | IRrecv | private
decodeSharp(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSharpBits, const bool strict=true, const bool expansion=true) | IRrecv | private
decodeSharpAc(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSharpAcBits, const bool strict=true) | IRrecv | private
decodeSony(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSonyMinBits, const bool strict=false) | IRrecv | private
decodeSymphony(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kSymphonyBits, const bool strict=true) | IRrecv | private
decodeTcl96Ac(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTcl96AcBits, const bool strict=true) | IRrecv | private
decodeTechnibelAc(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTechnibelAcBits, const bool strict=true) | IRrecv | private
decodeTeco(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTecoBits, const bool strict=false) | IRrecv | private
decodeTeknopoint(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTeknopointBits, const bool strict=true) | IRrecv | private
decodeToshibaAC(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kToshibaACBits, const bool strict=true) | IRrecv | private
decodeToto(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTotoBits, const bool strict=true) | IRrecv | private
decodeTranscold(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTranscoldBits, const bool strict=true) | IRrecv | private
decodeTrotec(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTrotecBits, const bool strict=true) | IRrecv | private
decodeTrotec3550(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTrotecBits, const bool strict=true) | IRrecv | private
decodeTruma(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kTrumaBits, const bool strict=true) | IRrecv | private
decodeVestelAc(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kVestelAcBits, const bool strict=true) | IRrecv | private
decodeVoltas(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kVoltasBits, const bool strict=true) | IRrecv | private
decodeWhirlpoolAC(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kWhirlpoolAcBits, const bool strict=true) | IRrecv | private
decodeWhynter(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kWhynterBits, const bool strict=true) | IRrecv | private
decodeWowwee(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kWowweeBits, const bool strict=true) | IRrecv | private
decodeXmp(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kXmpBits, const bool strict=true) | IRrecv | private
decodeYork(decode_results *results, uint16_t kStartOffset, const uint16_t kYorkBits, const bool strict=true) | IRrecv | private
decodeZepeal(decode_results *results, uint16_t offset=kStartOffset, const uint16_t nbits=kZepealBits, const bool strict=true) | IRrecv | private
disableIRIn(void) | IRrecv |
enableIRIn(const bool pullup=false) | IRrecv |
getBufSize(void) | IRrecv |
getRClevel(decode_results *results, uint16_t *offset, uint16_t *used, uint16_t bitTime, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const uint16_t delta=0, const uint8_t maxwidth=3) | IRrecv | private
getTolerance(void) | IRrecv |
irparams_save | IRrecv | private
IRrecv(const uint16_t recvpin, const uint16_t bufsize=kRawBuf, const uint8_t timeout=kTimeoutMs, const bool save_buffer=false, const uint8_t timer_num=kDefaultESP32Timer) | IRrecv | explicit
IRrecv(const uint16_t recvpin, const uint16_t bufsize=kRawBuf, const uint8_t timeout=kTimeoutMs, const bool save_buffer=false) | IRrecv | explicit
match(const uint32_t measured, const uint32_t desired, const uint8_t tolerance=kUseDefTol, const uint16_t delta=0) | IRrecv |
matchAtLeast(const uint32_t measured, const uint32_t desired, const uint8_t tolerance=kUseDefTol, const uint16_t delta=0) | IRrecv | private
matchBytes(volatile uint16_t *data_ptr, uint8_t *result_ptr, const uint16_t remaining, const uint16_t nbytes, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true, const bool expectlastspace=true) | IRrecv | private
matchData(volatile uint16_t *data_ptr, const uint16_t nbits, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true, const bool expectlastspace=true) | IRrecv | private
matchGeneric(volatile uint16_t *data_ptr, uint64_t *result_ptr, const uint16_t remaining, const uint16_t nbits, const uint16_t hdrmark, const uint32_t hdrspace, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint16_t footermark, const uint32_t footerspace, const bool atleast=false, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true) | IRrecv | private
matchGeneric(volatile uint16_t *data_ptr, uint8_t *result_ptr, const uint16_t remaining, const uint16_t nbits, const uint16_t hdrmark, const uint32_t hdrspace, const uint16_t onemark, const uint32_t onespace, const uint16_t zeromark, const uint32_t zerospace, const uint16_t footermark, const uint32_t footerspace, const bool atleast=false, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true) | IRrecv | private
matchGenericConstBitTime(volatile uint16_t *data_ptr, uint64_t *result_ptr, const uint16_t remaining, const uint16_t nbits, const uint16_t hdrmark, const uint32_t hdrspace, const uint16_t one, const uint32_t zero, const uint16_t footermark, const uint32_t footerspace, const bool atleast=false, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true) | IRrecv | private
matchManchester(volatile const uint16_t *data_ptr, uint64_t *result_ptr, const uint16_t remaining, const uint16_t nbits, const uint16_t hdrmark, const uint32_t hdrspace, const uint16_t clock_period, const uint16_t footermark, const uint32_t footerspace, const bool atleast=false, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true, const bool GEThomas=true) | IRrecv | private
matchManchesterData(volatile const uint16_t *data_ptr, uint64_t *result_ptr, const uint16_t remaining, const uint16_t nbits, const uint16_t half_period, const uint16_t starting_balance=0, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess, const bool MSBfirst=true, const bool GEThomas=true) | IRrecv | private
matchMark(const uint32_t measured, const uint32_t desired, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess) | IRrecv |
matchMarkRange(const uint32_t measured, const uint32_t desired, const uint16_t range=100, const int16_t excess=kMarkExcess) | IRrecv |
matchSpace(const uint32_t measured, const uint32_t desired, const uint8_t tolerance=kUseDefTol, const int16_t excess=kMarkExcess) | IRrecv |
matchSpaceRange(const uint32_t measured, const uint32_t desired, const uint16_t range=100, const int16_t excess=kMarkExcess) | IRrecv |
pause(void) | IRrecv |
resume(void) | IRrecv |
setTolerance(const uint8_t percent=kTolerance) | IRrecv |
setUnknownThreshold(const uint16_t length) | IRrecv |
ticksHigh(const uint32_t usecs, const uint8_t tolerance=kUseDefTol, const uint16_t delta=0) | IRrecv | private
ticksLow(const uint32_t usecs, const uint8_t tolerance=kUseDefTol, const uint16_t delta=0) | IRrecv | private
~IRrecv(void) | IRrecv |