IRremoteESP8266

Classes | Variables
ir_Trotec.h File Reference

Support for Trotec protocols. More...

Go to the source code of this file.

## Classes
union | TrotecProtocol
| Native representation of a Trotec A/C message. More...
union | Trotec3550Protocol
| Native representation of a Trotec 3550 A/C message. More...
class | IRTrotecESP
| Class for handling detailed Trotec A/C messages. More...
class | IRTrotec3550
| Class for handling detailed Trotec 3550 A/C messages. More...

## Variables
const uint8_t | kTrotecIntro1 = 0x12
const uint8_t | kTrotecIntro2 = 0x34
const uint8_t | kTrotecAuto = 0
const uint8_t | kTrotecCool = 1
const uint8_t | kTrotecDry = 2
const uint8_t | kTrotecFan = 3
const uint8_t | kTrotecFanLow = 1
const uint8_t | kTrotecFanMed = 2
const uint8_t | kTrotecFanHigh = 3
const uint8_t | kTrotecMinTemp = 18
const uint8_t | kTrotecDefTemp = 25
const uint8_t | kTrotecMaxTemp = 32
const uint8_t | kTrotecMaxTimer = 23
const uint8_t | kTrotec3550MinTempC = 16
const uint8_t | kTrotec3550MaxTempC = 30
const uint8_t | kTrotec3550MinTempF = 59
const uint8_t | kTrotec3550MaxTempF = 86

## Detailed Description

Support for Trotec protocols.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/pull/279
  https://github.com/crankyoldgit/IRremoteESP8266/issues/1176

## Variable Documentation

## ◆ kTrotec3550MaxTempC

const uint8_t kTrotec3550MaxTempC = 30

## ◆ kTrotec3550MaxTempF

const uint8_t kTrotec3550MaxTempF = 86

## ◆ kTrotec3550MinTempC

const uint8_t kTrotec3550MinTempC = 16

## ◆ kTrotec3550MinTempF

const uint8_t kTrotec3550MinTempF = 59

## ◆ kTrotecAuto

const uint8_t kTrotecAuto = 0

## ◆ kTrotecCool

const uint8_t kTrotecCool = 1

## ◆ kTrotecDefTemp

const uint8_t kTrotecDefTemp = 25

## ◆ kTrotecDry

const uint8_t kTrotecDry = 2

## ◆ kTrotecFan

const uint8_t kTrotecFan = 3

## ◆ kTrotecFanHigh

const uint8_t kTrotecFanHigh = 3

## ◆ kTrotecFanLow

const uint8_t kTrotecFanLow = 1

## ◆ kTrotecFanMed

const uint8_t kTrotecFanMed = 2

## ◆ kTrotecIntro1

const uint8_t kTrotecIntro1 = 0x12

## ◆ kTrotecIntro2

const uint8_t kTrotecIntro2 = 0x34

## ◆ kTrotecMaxTemp

const uint8_t kTrotecMaxTemp = 32

## ◆ kTrotecMaxTimer

const uint8_t kTrotecMaxTimer = 23

## ◆ kTrotecMinTemp

const uint8_t kTrotecMinTemp = 18