IRremoteESP8266

Public Attributes | List of all members
HitachiAC264Protocol Union Reference

Native representation of a Hitachi 164-bit A/C message. More...

`#include <ir_Hitachi.h>`

## Public Attributes
uint8_t | raw [kHitachiAc264StateLength]
| The state in native code. More...
struct {
uint8_t pad0 [11]
uint8_t Button:8
uint8_t __pad0__:8
uint8_t __pad1__:2
uint8_t Temp:6
uint8_t __pad2__:8
uint8_t pad1 [10]
uint8_t Mode:4
uint8_t Fan:4
uint8_t __pad3__:8
uint8_t __pad4__:4
uint8_t Power:1
uint8_t __pad5__:3
uint8_t __pad6__:8
uint8_t pad2 [4]
}; |

## Detailed Description

Native representation of a Hitachi 164-bit A/C message.

## Member Data Documentation

## ◆ @67

struct { ... }

## ◆ __pad0__

uint8_t HitachiAC264Protocol::__pad0__

## ◆ __pad1__

uint8_t HitachiAC264Protocol::__pad1__

## ◆ __pad2__

uint8_t HitachiAC264Protocol::__pad2__

## ◆ __pad3__

uint8_t HitachiAC264Protocol::__pad3__

## ◆ __pad4__

uint8_t HitachiAC264Protocol::__pad4__

## ◆ __pad5__

uint8_t HitachiAC264Protocol::__pad5__

## ◆ __pad6__

uint8_t HitachiAC264Protocol::__pad6__

## ◆ Button

uint8_t HitachiAC264Protocol::Button

## ◆ Fan

uint8_t HitachiAC264Protocol::Fan

## ◆ Mode

uint8_t HitachiAC264Protocol::Mode

## ◆ pad0

uint8_t HitachiAC264Protocol::pad0[11]

## ◆ pad1

uint8_t HitachiAC264Protocol::pad1[10]

## ◆ pad2

uint8_t HitachiAC264Protocol::pad2[4]

## ◆ Power

uint8_t HitachiAC264Protocol::Power

## ◆ raw

uint8_t HitachiAC264Protocol::raw[kHitachiAc264StateLength]

The state in native code.

## ◆ Temp

uint8_t HitachiAC264Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Hitachi.h