IRremoteESP8266

IRMideaAC Member List

This is the complete list of members for IRMideaAC, including all inherited members.

_ | IRMideaAC | private
_8CHeatToggle | IRMideaAC | private
_CleanToggle | IRMideaAC | private
_EconoToggle | IRMideaAC | private
_irsend | IRMideaAC | private
_LightToggle | IRMideaAC | private
_Quiet | IRMideaAC | private
_Quiet_prev | IRMideaAC | private
_SwingVStep | IRMideaAC | private
_SwingVToggle | IRMideaAC | private
_TurboToggle | IRMideaAC | private
begin(void) | IRMideaAC |
calcChecksum(const uint64_t state) | IRMideaAC | private static
calibrate(void) | IRMideaAC | inline
checksum(void) | IRMideaAC | private
convertFan(const stdAc::fanspeed_t speed) | IRMideaAC | static
convertMode(const stdAc::opmode_t mode) | IRMideaAC | static
get8CHeatToggle(void) | IRMideaAC |
getCleanToggle(void) | IRMideaAC |
getEconoToggle(void) | IRMideaAC |
getEnableSensorTemp(void) const | IRMideaAC |
getFan(void) const | IRMideaAC |
getLightToggle(void) | IRMideaAC |
getMode(void) const | IRMideaAC |
getOffTimer(void) const | IRMideaAC |
getOnTimer(void) const | IRMideaAC |
getPower(void) const | IRMideaAC |
getQuiet(void) const | IRMideaAC |
getRaw(void) | IRMideaAC |
getSensorTemp(const bool useCelsius=false) const | IRMideaAC |
getSleep(void) const | IRMideaAC |
getSwingVStep(void) | IRMideaAC |
getSwingVToggle(void) | IRMideaAC |
getTemp(const bool useCelsius=false) const | IRMideaAC |
getTurboToggle(void) | IRMideaAC |
getType(void) const | IRMideaAC |
getUseCelsius(void) const | IRMideaAC |
IRMideaAC(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRMideaAC | explicit
is8CHeatToggle(void) const | IRMideaAC |
isCleanToggle(void) const | IRMideaAC |
isEconoToggle(void) const | IRMideaAC |
isLightToggle(void) const | IRMideaAC |
isOffTimerEnabled(void) const | IRMideaAC |
isOnTimerEnabled(void) const | IRMideaAC |
isQuiet(void) const | IRMideaAC |
isSwingVStep(void) const | IRMideaAC |
isSwingVToggle(void) const | IRMideaAC |
isTurboToggle(void) const | IRMideaAC |
off(void) | IRMideaAC |
on(void) | IRMideaAC |
send(const uint16_t repeat=kMideaMinRepeat) | IRMideaAC |
set8CHeatToggle(const bool on) | IRMideaAC |
setCleanToggle(const bool on) | IRMideaAC |
setEconoToggle(const bool on) | IRMideaAC |
setEnableSensorTemp(const bool on) | IRMideaAC |
setFan(const uint8_t fan) | IRMideaAC |
setLightToggle(const bool on) | IRMideaAC |
setMode(const uint8_t mode) | IRMideaAC |
setOffTimer(const uint16_t mins) | IRMideaAC |
setOnTimer(const uint16_t mins) | IRMideaAC |
setPower(const bool on) | IRMideaAC |
setQuiet(const bool on) | IRMideaAC |
setQuiet(const bool on, const bool prev) | IRMideaAC |
setRaw(const uint64_t newState) | IRMideaAC |
setSensorTemp(const uint8_t temp, const bool useCelsius=false) | IRMideaAC |
setSleep(const bool on) | IRMideaAC |
setSwingVStep(const bool on) | IRMideaAC |
setSwingVToggle(const bool on) | IRMideaAC |
setTemp(const uint8_t temp, const bool useCelsius=false) | IRMideaAC |
setTurboToggle(const bool on) | IRMideaAC |
setType(const uint8_t type) | IRMideaAC | private
setUseCelsius(const bool celsius) | IRMideaAC |
stateReset(void) | IRMideaAC |
toCommon(const stdAc::state_t *prev=NULL) | IRMideaAC |
toCommonFanSpeed(const uint8_t speed) | IRMideaAC | static
toCommonMode(const uint8_t mode) | IRMideaAC | static
toString(void) | IRMideaAC |
validChecksum(const uint64_t state) | IRMideaAC | static