IRremoteESP8266

Variables
ir_ClimaButler.cpp File Reference

Support for Clima-Butler protocol. More...

## Variables
const uint16_t | kClimaButlerBitMark = 511
const uint16_t | kClimaButlerHdrMark = kClimaButlerBitMark
const uint16_t | kClimaButlerHdrSpace = 3492
const uint16_t | kClimaButlerOneSpace = 1540
const uint16_t | kClimaButlerZeroSpace = 548
const uint32_t | kClimaButlerGap = kDefaultMessageGap
const uint16_t | kClimaButlerFreq = 38000

## Detailed Description

Support for Clima-Butler protocol.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/1812

## Variable Documentation

## ◆ kClimaButlerBitMark

const uint16_t kClimaButlerBitMark = 511

## ◆ kClimaButlerFreq

const uint16_t kClimaButlerFreq = 38000

## ◆ kClimaButlerGap

const uint32_t kClimaButlerGap = kDefaultMessageGap

## ◆ kClimaButlerHdrMark

const uint16_t kClimaButlerHdrMark = kClimaButlerBitMark

## ◆ kClimaButlerHdrSpace

const uint16_t kClimaButlerHdrSpace = 3492

## ◆ kClimaButlerOneSpace

const uint16_t kClimaButlerOneSpace = 1540

## ◆ kClimaButlerZeroSpace

const uint16_t kClimaButlerZeroSpace = 548