IRremoteESP8266

Variables
ir_Carrier.cpp File Reference

Carrier protocols. More...

## Variables
const uint16_t | kCarrierAcHdrMark = 8532
const uint16_t | kCarrierAcHdrSpace = 4228
const uint16_t | kCarrierAcBitMark = 628
const uint16_t | kCarrierAcOneSpace = 1320
const uint16_t | kCarrierAcZeroSpace = 532
const uint16_t | kCarrierAcGap = 20000
const uint16_t | kCarrierAcFreq = 38
const uint16_t | kCarrierAc40HdrMark = 8402
const uint16_t | kCarrierAc40HdrSpace = 4166
const uint16_t | kCarrierAc40BitMark = 547
const uint16_t | kCarrierAc40OneSpace = 1540
const uint16_t | kCarrierAc40ZeroSpace = 497
const uint32_t | kCarrierAc40Gap = 150000
const uint16_t | kCarrierAc64HdrMark = 8940
const uint16_t | kCarrierAc64HdrSpace = 4556
const uint16_t | kCarrierAc64BitMark = 503
const uint16_t | kCarrierAc64OneSpace = 1736
const uint16_t | kCarrierAc64ZeroSpace = 615
const uint32_t | kCarrierAc64Gap = kDefaultMessageGap
const uint16_t | kCarrierAc84HdrMark = 5850
const uint16_t | kCarrierAc84Zero = 1175
const uint16_t | kCarrierAc84One = 430
const uint16_t | kCarrierAc84HdrSpace = kCarrierAc84Zero
const uint32_t | kCarrierAc84Gap = kDefaultMessageGap
const uint8_t | kCarrierAc84ExtraBits = 4
const uint8_t | kCarrierAc84ExtraTolerance = 5
const uint16_t | kCarrierAc128HdrMark = 4600
const uint16_t | kCarrierAc128HdrSpace = 2600
const uint16_t | kCarrierAc128Hdr2Mark = 9300
const uint16_t | kCarrierAc128Hdr2Space = 5000
const uint16_t | kCarrierAc128BitMark = 340
const uint16_t | kCarrierAc128OneSpace = 1000
const uint16_t | kCarrierAc128ZeroSpace = 400
const uint16_t | kCarrierAc128SectionGap = 20600
const uint16_t | kCarrierAc128InterSpace = 6700
const uint16_t | kCarrierAc128SectionBits = kCarrierAc128Bits / 2

## Detailed Description

Carrier protocols.

See also
  CarrierAc https://github.com/crankyoldgit/IRremoteESP8266/issues/385
  CarrierAc64 https://github.com/crankyoldgit/IRremoteESP8266/issues/1127
  CarrierAc128 https://github.com/crankyoldgit/IRremoteESP8266/issues/1797

## Variable Documentation

## ◆ kCarrierAc128BitMark

const uint16_t kCarrierAc128BitMark = 340

## ◆ kCarrierAc128Hdr2Mark

const uint16_t kCarrierAc128Hdr2Mark = 9300

## ◆ kCarrierAc128Hdr2Space

const uint16_t kCarrierAc128Hdr2Space = 5000

## ◆ kCarrierAc128HdrMark

const uint16_t kCarrierAc128HdrMark = 4600

## ◆ kCarrierAc128HdrSpace

const uint16_t kCarrierAc128HdrSpace = 2600

## ◆ kCarrierAc128InterSpace

const uint16_t kCarrierAc128InterSpace = 6700

## ◆ kCarrierAc128OneSpace

const uint16_t kCarrierAc128OneSpace = 1000

## ◆ kCarrierAc128SectionBits

const uint16_t kCarrierAc128SectionBits = kCarrierAc128Bits / 2

## ◆ kCarrierAc128SectionGap

const uint16_t kCarrierAc128SectionGap = 20600

## ◆ kCarrierAc128ZeroSpace

const uint16_t kCarrierAc128ZeroSpace = 400

## ◆ kCarrierAc40BitMark

const uint16_t kCarrierAc40BitMark = 547

## ◆ kCarrierAc40Gap

const uint32_t kCarrierAc40Gap = 150000

See also
  https://github.com/crankyoldgit/IRremoteESP8266/issues/1190#issuecomment-643380155

## ◆ kCarrierAc40HdrMark

const uint16_t kCarrierAc40HdrMark = 8402

## ◆ kCarrierAc40HdrSpace

const uint16_t kCarrierAc40HdrSpace = 4166

## ◆ kCarrierAc40OneSpace

const uint16_t kCarrierAc40OneSpace = 1540

## ◆ kCarrierAc40ZeroSpace

const uint16_t kCarrierAc40ZeroSpace = 497

## ◆ kCarrierAc64BitMark

const uint16_t kCarrierAc64BitMark = 503

## ◆ kCarrierAc64Gap

const uint32_t kCarrierAc64Gap = kDefaultMessageGap

## ◆ kCarrierAc64HdrMark

const uint16_t kCarrierAc64HdrMark = 8940

## ◆ kCarrierAc64HdrSpace

const uint16_t kCarrierAc64HdrSpace = 4556

## ◆ kCarrierAc64OneSpace

const uint16_t kCarrierAc64OneSpace = 1736

## ◆ kCarrierAc64ZeroSpace

const uint16_t kCarrierAc64ZeroSpace = 615

## ◆ kCarrierAc84ExtraBits

const uint8_t kCarrierAc84ExtraBits = 4

## ◆ kCarrierAc84ExtraTolerance

const uint8_t kCarrierAc84ExtraTolerance = 5

## ◆ kCarrierAc84Gap

const uint32_t kCarrierAc84Gap = kDefaultMessageGap

## ◆ kCarrierAc84HdrMark

const uint16_t kCarrierAc84HdrMark = 5850

## ◆ kCarrierAc84HdrSpace

const uint16_t kCarrierAc84HdrSpace = kCarrierAc84Zero

## ◆ kCarrierAc84One

const uint16_t kCarrierAc84One = 430

## ◆ kCarrierAc84Zero

const uint16_t kCarrierAc84Zero = 1175

## ◆ kCarrierAcBitMark

const uint16_t kCarrierAcBitMark = 628

## ◆ kCarrierAcFreq

const uint16_t kCarrierAcFreq = 38

## ◆ kCarrierAcGap

const uint16_t kCarrierAcGap = 20000

## ◆ kCarrierAcHdrMark

const uint16_t kCarrierAcHdrMark = 8532

## ◆ kCarrierAcHdrSpace

const uint16_t kCarrierAcHdrSpace = 4228

## ◆ kCarrierAcOneSpace

const uint16_t kCarrierAcOneSpace = 1320

## ◆ kCarrierAcZeroSpace

const uint16_t kCarrierAcZeroSpace = 532