IRremoteESP8266

Variables
ir_Kelon.cpp File Reference

Support for Kelon AC protocols. Both sending and decoding should be functional for models of series KELON ON/OFF 9000-12000. All features of the standard remote are implemented. More...

## Variables
const uint16_t | kKelonHdrMark = 9000
const uint16_t | kKelonHdrSpace = 4600
const uint16_t | kKelonBitMark = 560
const uint16_t | kKelonOneSpace = 1680
const uint16_t | kKelonZeroSpace = 600
const uint32_t | kKelonGap = 2 * kDefaultMessageGap
const uint16_t | kKelonFreq = 38000
const uint32_t | kKelon168FooterSpace = 8000
const uint16_t | kKelon168Section1Size = 6
const uint16_t | kKelon168Section2Size = 8
const uint16_t | kKelon168Section3Size = 7

## Detailed Description

Support for Kelon AC protocols. Both sending and decoding should be functional for models of series KELON ON/OFF 9000-12000. All features of the standard remote are implemented.

Note
  Unsupported:
  - Explicit on/off due to AC unit limitations
  - Explicit swing position due to AC unit limitations
  - Fahrenheit.

## Variable Documentation

## ◆ kKelon168FooterSpace

const uint32_t kKelon168FooterSpace = 8000

## ◆ kKelon168Section1Size

const uint16_t kKelon168Section1Size = 6

## ◆ kKelon168Section2Size

const uint16_t kKelon168Section2Size = 8

## ◆ kKelon168Section3Size

const uint16_t kKelon168Section3Size = 7

## ◆ kKelonBitMark

const uint16_t kKelonBitMark = 560

## ◆ kKelonFreq

const uint16_t kKelonFreq = 38000

## ◆ kKelonGap

const uint32_t kKelonGap = 2 * kDefaultMessageGap

## ◆ kKelonHdrMark

const uint16_t kKelonHdrMark = 9000

## ◆ kKelonHdrSpace

const uint16_t kKelonHdrSpace = 4600

## ◆ kKelonOneSpace

const uint16_t kKelonOneSpace = 1680

## ◆ kKelonZeroSpace

const uint16_t kKelonZeroSpace = 600