IRremoteESP8266

Public Attributes | List of all members
Daikin216Protocol Union Reference

Native representation of a Daikin216 A/C message. More...

`#include <ir_Daikin.h>`

## Public Attributes
uint8_t | raw [kDaikin216StateLength]
| The state of the IR remote. More...
struct {
uint8_t pad0 [7]
uint8_t Sum1:8
uint8_t pad1 [5]
uint8_t Power:1
uint8_t __pad0__:3
uint8_t Mode:3
uint8_t __pad1__:1
uint8_t __pad2__:1
uint8_t Temp:6
uint8_t __pad3__:1
uint8_t __pad4__:8
uint8_t SwingV:4
uint8_t Fan:4
uint8_t SwingH:4
uint8_t __pad5__:4
uint8_t pad2 [3]
uint8_t Powerful:1
uint8_t __pad6__:0
uint8_t pad3 [4]
uint8_t Sum2:8
}; |

## Detailed Description

Native representation of a Daikin216 A/C message.

## Member Data Documentation

## ◆ @29

struct { ... }

## ◆ __pad0__

uint8_t Daikin216Protocol::__pad0__

## ◆ __pad1__

uint8_t Daikin216Protocol::__pad1__

## ◆ __pad2__

uint8_t Daikin216Protocol::__pad2__

## ◆ __pad3__

uint8_t Daikin216Protocol::__pad3__

## ◆ __pad4__

uint8_t Daikin216Protocol::__pad4__

## ◆ __pad5__

uint8_t Daikin216Protocol::__pad5__

## ◆ __pad6__

uint8_t Daikin216Protocol::__pad6__

## ◆ Fan

uint8_t Daikin216Protocol::Fan

## ◆ Mode

uint8_t Daikin216Protocol::Mode

## ◆ pad0

uint8_t Daikin216Protocol::pad0[7]

## ◆ pad1

uint8_t Daikin216Protocol::pad1[5]

## ◆ pad2

uint8_t Daikin216Protocol::pad2[3]

## ◆ pad3

uint8_t Daikin216Protocol::pad3[4]

## ◆ Power

uint8_t Daikin216Protocol::Power

## ◆ Powerful

uint8_t Daikin216Protocol::Powerful

## ◆ raw

uint8_t Daikin216Protocol::raw[kDaikin216StateLength]

The state of the IR remote.

## ◆ Sum1

uint8_t Daikin216Protocol::Sum1

## ◆ Sum2

uint8_t Daikin216Protocol::Sum2

## ◆ SwingH

uint8_t Daikin216Protocol::SwingH

## ◆ SwingV

uint8_t Daikin216Protocol::SwingV

## ◆ Temp

uint8_t Daikin216Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Daikin.h