IRremoteESP8266

Public Member Functions | Static Public Member Functions | Private Attributes | List of all members
IRAirwellAc Class Reference

Class for handling detailed Airwell A/C messages. More...

`#include <ir_Airwell.h>`

Collaboration diagram for IRAirwellAc:
[legend]

## Public Member Functions
| IRAirwellAc (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | stateReset ()
| Reset the internals of the object to a known good state. More...
void | send (const uint16_t repeat=kAirwellMinRepeats)
| Send the current internal state as an IR message. More...
int8_t | calibrate (void)
| Run the calibration to calculate uSec timing offsets for this platform. More...
void | begin ()
| Set up hardware to be able to send a message. More...
void | setPowerToggle (const bool on)
| Turn on/off the Power Airwell setting. More...
bool | getPowerToggle () const
| Get the power toggle setting from the internal state. More...
void | setTemp (const uint8_t temp)
| Set the temperature. More...
uint8_t | getTemp () const
| Get the current temperature setting. More...
void | setFan (const uint8_t speed)
| Set the speed of the fan. More...
uint8_t | getFan () const
| Get the current fan speed setting. More...
void | setMode (const uint8_t mode)
| Set the desired operation mode. More...
uint8_t | getMode () const
| Get the current operation mode setting. More...
uint64_t | getRaw () const
| Get the raw state of the object, suitable to be sent with the appropriate IRsend object method. More...
void | setRaw (const uint64_t state)
| Set the raw state of the object. More...
stdAc::state_t | toCommon (const stdAc::state_t *prev=NULL) const
| Convert the current internal state into its stdAc::state_t equivalent. More...
String | toString () const
| Convert the current internal state into a human readable string. More...

## Static Public Member Functions
static uint8_t | convertMode (const stdAc::opmode_t mode)
| Convert a stdAc::opmode_t enum into its native mode. More...
static uint8_t | convertFan (const stdAc::fanspeed_t speed)
| Convert a stdAc::fanspeed_t enum into it's native speed. More...
static stdAc::opmode_t | toCommonMode (const uint8_t mode)
| Convert a native mode into its stdAc equivalent. More...
static stdAc::fanspeed_t | toCommonFanSpeed (const uint8_t speed)
| Convert a native fan speed into its stdAc equivalent. More...

## Private Attributes
IRsend | _irsend
| Instance of the IR send class. More...
AirwellProtocol | _

## Detailed Description

Class for handling detailed Airwell A/C messages.

## Constructor & Destructor Documentation

## ◆ IRAirwellAc()

IRAirwellAc::IRAirwellAc | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |
| explicit

Class constructor.

Parameters

  [in] | pin | GPIO to be used when sending.
  [in] | inverted | Is the output signal to be inverted?
  [in] | use_modulation | Is frequency modulation to be used?

## Member Function Documentation

## ◆ begin()

void IRAirwellAc::begin | ( |  | ) |

Set up hardware to be able to send a message.

## ◆ calibrate()

int8_t IRAirwellAc::calibrate | ( | void |  | ) |
| inline

Run the calibration to calculate uSec timing offsets for this platform.

Returns
  The uSec timing offset needed per modulation of the IR Led.

Note
  This will produce a 65ms IR signal pulse at 38kHz. Only ever needs to be run once per object instantiation, if at all.

## ◆ convertFan()

uint8_t IRAirwellAc::convertFan | ( | const stdAc::fanspeed_t | speed | ) |
| static

Convert a stdAc::fanspeed_t enum into it's native speed.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ convertMode()

uint8_t IRAirwellAc::convertMode | ( | const stdAc::opmode_t | mode | ) |
| static

Convert a stdAc::opmode_t enum into its native mode.

Parameters

  [in] | mode | The enum to be converted.

Returns
  The native equivalent of the enum.

## ◆ getFan()

uint8_t IRAirwellAc::getFan | ( |  | ) | const

Get the current fan speed setting.

Returns
  The current fan speed.

## ◆ getMode()

uint8_t IRAirwellAc::getMode | ( |  | ) | const

Get the current operation mode setting.

Returns
  The current operation mode.

## ◆ getPowerToggle()

bool IRAirwellAc::getPowerToggle | ( |  | ) | const

Get the power toggle setting from the internal state.

Returns
  A boolean indicating the setting.

## ◆ getRaw()

uint64_t IRAirwellAc::getRaw | ( |  | ) | const

Get the raw state of the object, suitable to be sent with the appropriate IRsend object method.

Returns
  A copy of the internal state.

## ◆ getTemp()

uint8_t IRAirwellAc::getTemp | ( |  | ) | const

Get the current temperature setting.

Returns
  Get current setting for temp. in degrees celsius.

## ◆ send()

void IRAirwellAc::send | ( | const uint16_t | repeat = `kAirwellMinRepeats` | ) |

Send the current internal state as an IR message.

Parameters

  [in] | repeat | Nr. of times the message will be repeated.

## ◆ setFan()

void IRAirwellAc::setFan | ( | const uint8_t | speed | ) |

Set the speed of the fan.

Parameters

  [in] | speed | The desired setting.

Note
  The speed is locked to Low when in Dry mode.

## ◆ setMode()

void IRAirwellAc::setMode | ( | const uint8_t | mode | ) |

Set the desired operation mode.

Parameters

  [in] | mode | The desired operation mode.

## ◆ setPowerToggle()

void IRAirwellAc::setPowerToggle | ( | const bool | on | ) |

Turn on/off the Power Airwell setting.

Parameters

  [in] | on | The desired setting state.

## ◆ setRaw()

void IRAirwellAc::setRaw | ( | const uint64_t | state | ) |

Set the raw state of the object.

Parameters

  [in] | state | The raw state from the native IR message.

## ◆ setTemp()

void IRAirwellAc::setTemp | ( | const uint8_t | degrees | ) |

Set the temperature.

Parameters

  [in] | degrees | The temperature in degrees celsius.

## ◆ stateReset()

void IRAirwellAc::stateReset | ( |  | ) |

Reset the internals of the object to a known good state.

## ◆ toCommon()

stdAc::state_t IRAirwellAc::toCommon | ( | const stdAc::state_t * | prev = `NULL` | ) | const

Convert the current internal state into its stdAc::state_t equivalent.

Parameters

  [in] | prev | Ptr to the previous state if required.

Returns
  The stdAc equivalent of the native settings.

## ◆ toCommonFanSpeed()

stdAc::fanspeed_t IRAirwellAc::toCommonFanSpeed | ( | const uint8_t | speed | ) |
| static

Convert a native fan speed into its stdAc equivalent.

Parameters

  [in] | speed | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toCommonMode()

stdAc::opmode_t IRAirwellAc::toCommonMode | ( | const uint8_t | mode | ) |
| static

Convert a native mode into its stdAc equivalent.

Parameters

  [in] | mode | The native setting to be converted.

Returns
  The stdAc equivalent of the native setting.

## ◆ toString()

String IRAirwellAc::toString | ( |  | ) | const

Convert the current internal state into a human readable string.

Returns
  A human readable string.

## Member Data Documentation

## ◆ _

AirwellProtocol IRAirwellAc::_
| private

## ◆ _irsend

IRsend IRAirwellAc::_irsend
| private

Instance of the IR send class.

The documentation for this class was generated from the following files:

- src/ir_Airwell.h
- src/ir_Airwell.cpp