IRremoteESP8266

IRNeoclimaAc Member List

This is the complete list of members for IRNeoclimaAc, including all inherited members.

_ | IRNeoclimaAc | private
_irsend | IRNeoclimaAc | private
begin(void) | IRNeoclimaAc |
calcChecksum(const uint8_t state[], const uint16_t length=kNeoclimaStateLength) | IRNeoclimaAc | static
calibrate(void) | IRNeoclimaAc | inline
checksum(const uint16_t length=kNeoclimaStateLength) | IRNeoclimaAc | private
convertFan(const stdAc::fanspeed_t speed) | IRNeoclimaAc | static
convertMode(const stdAc::opmode_t mode) | IRNeoclimaAc | static
get8CHeat(void) const | IRNeoclimaAc |
getButton(void) const | IRNeoclimaAc |
getEcono(void) const | IRNeoclimaAc |
getEye(void) const | IRNeoclimaAc |
getFan(void) const | IRNeoclimaAc |
getFollow(void) const | IRNeoclimaAc |
getFresh(void) const | IRNeoclimaAc |
getHold(void) const | IRNeoclimaAc |
getIon(void) const | IRNeoclimaAc |
getLight(void) const | IRNeoclimaAc |
getMode(void) const | IRNeoclimaAc |
getPower(void) const | IRNeoclimaAc |
getRaw(void) | IRNeoclimaAc |
getSleep(void) const | IRNeoclimaAc |
getSwingH(void) const | IRNeoclimaAc |
getSwingV(void) const | IRNeoclimaAc |
getTemp(void) const | IRNeoclimaAc |
getTempUnits(void) const | IRNeoclimaAc |
getTurbo(void) const | IRNeoclimaAc |
IRNeoclimaAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRNeoclimaAc | explicit
off(void) | IRNeoclimaAc |
on(void) | IRNeoclimaAc |
send(const uint16_t repeat=kNeoclimaMinRepeat) | IRNeoclimaAc |
set8CHeat(const bool on) | IRNeoclimaAc |
setButton(const uint8_t button) | IRNeoclimaAc |
setEcono(const bool on) | IRNeoclimaAc |
setEye(const bool on) | IRNeoclimaAc |
setFan(const uint8_t speed) | IRNeoclimaAc |
setFresh(const bool on) | IRNeoclimaAc |
setHold(const bool on) | IRNeoclimaAc |
setIon(const bool on) | IRNeoclimaAc |
setLight(const bool on) | IRNeoclimaAc |
setMode(const uint8_t mode) | IRNeoclimaAc |
setPower(const bool on) | IRNeoclimaAc |
setRaw(const uint8_t new_code[], const uint16_t length=kNeoclimaStateLength) | IRNeoclimaAc |
setSleep(const bool on) | IRNeoclimaAc |
setSwingH(const bool on) | IRNeoclimaAc |
setSwingV(const bool on) | IRNeoclimaAc |
setTemp(const uint8_t temp, const bool celsius=true) | IRNeoclimaAc |
setTurbo(const bool on) | IRNeoclimaAc |
stateReset(void) | IRNeoclimaAc |
toCommon(void) const | IRNeoclimaAc |
toCommonFanSpeed(const uint8_t speed) | IRNeoclimaAc | static
toCommonMode(const uint8_t mode) | IRNeoclimaAc | static
toString(void) const | IRNeoclimaAc |
validChecksum(const uint8_t state[], const uint16_t length=kNeoclimaStateLength) | IRNeoclimaAc | static