IRremoteESP8266

Public Attributes | List of all members
Mitsubishi136Protocol Union Reference

Native representation of a Mitsubishi 136-bit A/C message. More...

`#include <ir_Mitsubishi.h>`

## Public Attributes
uint8_t | raw [kMitsubishi136StateLength]
| The state in code form. More...
struct {
uint8_t pad [5]
uint8_t __pad0__:6
uint8_t Power:1
uint8_t __pad1__:1
uint8_t Mode:3
uint8_t __pad2__:1
uint8_t Temp:4
uint8_t __pad3__:1
uint8_t Fan:2
uint8_t __pad4__:1
uint8_t SwingV:4
}; |

## Detailed Description

Native representation of a Mitsubishi 136-bit A/C message.

## Member Data Documentation

## ◆ @88

struct { ... }

## ◆ __pad0__

uint8_t Mitsubishi136Protocol::__pad0__

## ◆ __pad1__

uint8_t Mitsubishi136Protocol::__pad1__

## ◆ __pad2__

uint8_t Mitsubishi136Protocol::__pad2__

## ◆ __pad3__

uint8_t Mitsubishi136Protocol::__pad3__

## ◆ __pad4__

uint8_t Mitsubishi136Protocol::__pad4__

## ◆ Fan

uint8_t Mitsubishi136Protocol::Fan

## ◆ Mode

uint8_t Mitsubishi136Protocol::Mode

## ◆ pad

uint8_t Mitsubishi136Protocol::pad[5]

## ◆ Power

uint8_t Mitsubishi136Protocol::Power

## ◆ raw

uint8_t Mitsubishi136Protocol::raw[kMitsubishi136StateLength]

The state in code form.

## ◆ SwingV

uint8_t Mitsubishi136Protocol::SwingV

## ◆ Temp

uint8_t Mitsubishi136Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Mitsubishi.h