IRremoteESP8266

IRDelonghiAc Member List

This is the complete list of members for IRDelonghiAc, including all inherited members.

_ | IRDelonghiAc | private
_irsend | IRDelonghiAc | private
_saved_temp | IRDelonghiAc | private
_saved_temp_units | IRDelonghiAc | private
begin(void) | IRDelonghiAc |
calcChecksum(const uint64_t state) | IRDelonghiAc | static
calibrate(void) | IRDelonghiAc | inline
checksum(void) | IRDelonghiAc | private
convertFan(const stdAc::fanspeed_t speed) | IRDelonghiAc | static
convertMode(const stdAc::opmode_t mode) | IRDelonghiAc | static
getBoost(void) const | IRDelonghiAc |
getFan(void) const | IRDelonghiAc |
getMode(void) const | IRDelonghiAc |
getOffTimer(void) const | IRDelonghiAc |
getOffTimerEnabled(void) const | IRDelonghiAc |
getOnTimer(void) const | IRDelonghiAc |
getOnTimerEnabled(void) const | IRDelonghiAc |
getPower(void) const | IRDelonghiAc |
getRaw(void) | IRDelonghiAc |
getSleep(void) const | IRDelonghiAc |
getTemp(void) const | IRDelonghiAc |
getTempUnit(void) const | IRDelonghiAc |
IRDelonghiAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRDelonghiAc | explicit
off(void) | IRDelonghiAc |
on(void) | IRDelonghiAc |
send(const uint16_t repeat=kDelonghiAcDefaultRepeat) | IRDelonghiAc |
setBoost(const bool on) | IRDelonghiAc |
setFan(const uint8_t speed) | IRDelonghiAc |
setMode(const uint8_t mode) | IRDelonghiAc |
setOffTimer(const uint16_t nr_of_mins) | IRDelonghiAc |
setOffTimerEnabled(const bool on) | IRDelonghiAc |
setOnTimer(const uint16_t nr_of_mins) | IRDelonghiAc |
setOnTimerEnabled(const bool on) | IRDelonghiAc |
setPower(const bool on) | IRDelonghiAc |
setRaw(const uint64_t state) | IRDelonghiAc |
setSleep(const bool on) | IRDelonghiAc |
setTemp(const uint8_t temp, const bool fahrenheit=false, const bool force=false) | IRDelonghiAc |
setTempUnit(const bool celsius) | IRDelonghiAc |
stateReset(void) | IRDelonghiAc |
toCommon(void) const | IRDelonghiAc |
toCommonFanSpeed(const uint8_t speed) | IRDelonghiAc | static
toCommonMode(const uint8_t mode) | IRDelonghiAc | static
toString(void) const | IRDelonghiAc |
validChecksum(const uint64_t state) | IRDelonghiAc | static