IRremoteESP8266

IRElectraAc Member List

This is the complete list of members for IRElectraAc, including all inherited members.

_ | IRElectraAc | private
_irsend | IRElectraAc | private
begin(void) | IRElectraAc |
calcChecksum(const uint8_t state[], const uint16_t length=kElectraAcStateLength) | IRElectraAc | static
calibrate(void) | IRElectraAc | inline
checksum(const uint16_t length=kElectraAcStateLength) | IRElectraAc | private
convertFan(const stdAc::fanspeed_t speed) | IRElectraAc | static
convertMode(const stdAc::opmode_t mode) | IRElectraAc | static
getClean(void) const | IRElectraAc |
getFan(void) const | IRElectraAc |
getIFeel(void) const | IRElectraAc |
getLightToggle(void) const | IRElectraAc |
getMode(void) const | IRElectraAc |
getPower(void) const | IRElectraAc |
getRaw(void) | IRElectraAc |
getSensorTemp(void) const | IRElectraAc |
getSensorUpdate(void) const | IRElectraAc |
getSwingH(void) const | IRElectraAc |
getSwingV(void) const | IRElectraAc |
getTemp(void) const | IRElectraAc |
getTurbo(void) const | IRElectraAc |
IRElectraAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRElectraAc | explicit
off(void) | IRElectraAc |
on(void) | IRElectraAc |
send(const uint16_t repeat=kElectraAcMinRepeat) | IRElectraAc |
setClean(const bool on) | IRElectraAc |
setFan(const uint8_t speed) | IRElectraAc |
setIFeel(const bool on) | IRElectraAc |
setLightToggle(const bool on) | IRElectraAc |
setMode(const uint8_t mode) | IRElectraAc |
setPower(const bool on) | IRElectraAc |
setRaw(const uint8_t new_code[], const uint16_t length=kElectraAcStateLength) | IRElectraAc |
setSensorTemp(const uint8_t temp) | IRElectraAc |
setSensorUpdate(const bool on) | IRElectraAc |
setSwingH(const bool on) | IRElectraAc |
setSwingV(const bool on) | IRElectraAc |
setTemp(const uint8_t temp) | IRElectraAc |
setTurbo(const bool on) | IRElectraAc |
stateReset(void) | IRElectraAc |
toCommon(void) const | IRElectraAc |
toCommonFanSpeed(const uint8_t speed) | IRElectraAc | static
toCommonMode(const uint8_t mode) | IRElectraAc | static
toString(void) const | IRElectraAc |
validChecksum(const uint8_t state[], const uint16_t length=kElectraAcStateLength) | IRElectraAc | static