IRremoteESP8266

Classes | Namespaces | Enumerations | Variables
IRsend.h File Reference

Go to the source code of this file.

## Classes
struct | stdAc::state_t
| Structure to hold a common A/C state. More...
class | IRsend
| Class for sending all basic IR protocols. More...

## Namespaces
| stdAc
| Enumerators and Structures for the Common A/C API.

## Enumerations
enum | stdAc::opmode_t { stdAc::opmode_t::kOff = -1, stdAc::opmode_t::kAuto = 0, stdAc::opmode_t::kCool = 1, stdAc::opmode_t::kHeat = 2, stdAc::opmode_t::kDry = 3, stdAc::opmode_t::kFan = 4, stdAc::opmode_t::kLastOpmodeEnum = kFan }
| Common A/C settings for A/C operating modes. More...
enum | stdAc::fanspeed_t { stdAc::fanspeed_t::kAuto = 0, stdAc::fanspeed_t::kMin = 1, stdAc::fanspeed_t::kLow = 2, stdAc::fanspeed_t::kMedium = 3, stdAc::fanspeed_t::kHigh = 4, stdAc::fanspeed_t::kMax = 5, stdAc::fanspeed_t::kMediumHigh = 6, stdAc::fanspeed_t::kLastFanspeedEnum = kMediumHigh }
| Common A/C settings for Fan Speeds. More...
enum | stdAc::swingv_t { stdAc::swingv_t::kOff = -1, stdAc::swingv_t::kAuto = 0, stdAc::swingv_t::kHighest = 1, stdAc::swingv_t::kHigh = 2, stdAc::swingv_t::kMiddle = 3, stdAc::swingv_t::kLow = 4, stdAc::swingv_t::kLowest = 5, stdAc::swingv_t::kUpperMiddle = 6, stdAc::swingv_t::kLastSwingvEnum = kUpperMiddle }
| Common A/C settings for Vertical Swing. More...
enum | stdAc::ac_command_t { stdAc::ac_command_t::kControlCommand = 0, stdAc::ac_command_t::kSensorTempReport = 1, stdAc::ac_command_t::kTimerCommand = 2, stdAc::ac_command_t::kConfigCommand = 3, stdAc::ac_command_t::kLastAcCommandEnum = kConfigCommand }
| Tyoe of A/C command (if the remote uses different codes for each) More...
enum | stdAc::swingh_t { stdAc::swingh_t::kOff = -1, stdAc::swingh_t::kAuto = 0, stdAc::swingh_t::kLeftMax = 1, stdAc::swingh_t::kLeft = 2, stdAc::swingh_t::kMiddle = 3, stdAc::swingh_t::kRight = 4, stdAc::swingh_t::kRightMax = 5, stdAc::swingh_t::kWide = 6, stdAc::swingh_t::kLastSwinghEnum = kWide }
| Common A/C settings for Horizontal Swing. More...
enum | fujitsu_ac_remote_model_t { ARRAH2E = 1, ARDB1, ARREB1E, ARJW2, ARRY4, ARREW4E }
| Fujitsu A/C model numbers. More...
enum | gree_ac_remote_model_t { YAW1F = 1, YBOFB, YX1FSF }
| Gree A/C model numbers. More...
enum | haier_ac176_remote_model_t { V9014557_A = 1, V9014557_B }
| HAIER_AC176 A/C model numbers. More...
enum | hitachi_ac1_remote_model_t { R_LT0541_HTA_A = 1, R_LT0541_HTA_B }
| HITACHI_AC1 A/C model numbers. More...
enum | mirage_ac_remote_model_t { KKG9AC1 = 1, KKG29AC1 }
| MIRAGE A/C model numbers. More...
enum | panasonic_ac_remote_model_t { kPanasonicUnknown = 0, kPanasonicLke = 1, kPanasonicNke = 2, kPanasonicDke = 3, kPanasonicJke = 4, kPanasonicCkp = 5, kPanasonicRkr = 6 }
| Panasonic A/C model numbers. More...
enum | sharp_ac_remote_model_t { A907 = 1, A705 = 2, A903 = 3 }
| Sharp A/C model numbers. More...
enum | tcl_ac_remote_model_t { TAC09CHSD = 1, GZ055BE1 = 2 }
| TCL (& Teknopoint) A/C model numbers. More...
enum | voltas_ac_remote_model_t { kVoltasUnknown = 0, kVoltas122LZF = 1 }
| Voltas A/C model numbers. More...
enum | whirlpool_ac_remote_model_t { DG11J13A = 1, DG11J191 }
| Whirlpool A/C model numbers. More...
enum | lg_ac_remote_model_t { GE6711AR2853M = 1, AKB75215403, AKB74955603, AKB73757604, LG6711A20083V }
| LG A/C model numbers. More...
enum | argo_ac_remote_model_t { SAC_WREM2 = 1, SAC_WREM3 }
| Argo A/C model numbers. More...

## Variables
const int8_t | kPeriodOffset = -2
const uint8_t | kDutyDefault = 50
const uint8_t | kDutyMax = 100
const uint16_t | kMaxAccurateUsecDelay = 16383
const uint32_t | kDefaultMessageGap = 100000
const float | kNoTempValue = -100.0
| Placeholder for missing sensor temp value. More...

## Enumeration Type Documentation

## ◆ argo_ac_remote_model_t

enum argo_ac_remote_model_t

Argo A/C model numbers.

Enumerator
SAC_WREM2 |
SAC_WREM3 |

## ◆ fujitsu_ac_remote_model_t

enum fujitsu_ac_remote_model_t

Fujitsu A/C model numbers.

Enumerator
ARRAH2E | (1) AR-RAH2E, AR-RAC1E, AR-RAE1E, AR-RCE1E, AR-RAH2U, AR-REG1U (Default) Warning: Use on incorrect models can cause the A/C to lock up, requring the A/C to be physically powered off to fix. e.g. AR-RAH1U may lock up with a Swing command.
ARDB1 | (2) AR-DB1, AR-DL10 (AR-DL10 swing doesn't work)
ARREB1E | (3) AR-REB1E, AR-RAH1U (Similar to ARRAH2E but no horiz control)
ARJW2 | (4) AR-JW2 (Same as ARDB1 but with horiz control)
ARRY4 | (5) AR-RY4 (Same as AR-RAH2E but with clean & filter)
ARREW4E | (6) Similar to ARRAH2E, but with different temp config.

## ◆ gree_ac_remote_model_t

enum gree_ac_remote_model_t

Gree A/C model numbers.

Enumerator
YAW1F |
YBOFB |
YX1FSF |

## ◆ haier_ac176_remote_model_t

enum haier_ac176_remote_model_t

HAIER_AC176 A/C model numbers.

Enumerator
V9014557_A |
V9014557_B |

## ◆ hitachi_ac1_remote_model_t

enum hitachi_ac1_remote_model_t

HITACHI_AC1 A/C model numbers.

Enumerator
R_LT0541_HTA_A |
R_LT0541_HTA_B |

## ◆ lg_ac_remote_model_t

enum lg_ac_remote_model_t

LG A/C model numbers.

Enumerator
GE6711AR2853M |
AKB75215403 |
AKB74955603 |
AKB73757604 |
LG6711A20083V |

## ◆ mirage_ac_remote_model_t

enum mirage_ac_remote_model_t

MIRAGE A/C model numbers.

Enumerator
KKG9AC1 |
KKG29AC1 |

## ◆ panasonic_ac_remote_model_t

enum panasonic_ac_remote_model_t

Panasonic A/C model numbers.

Enumerator
kPanasonicUnknown |
kPanasonicLke |
kPanasonicNke |
kPanasonicDke |
kPanasonicJke |
kPanasonicCkp |
kPanasonicRkr |

## ◆ sharp_ac_remote_model_t

enum sharp_ac_remote_model_t

Sharp A/C model numbers.

Enumerator
A907 |
A705 |
A903 |

## ◆ tcl_ac_remote_model_t

enum tcl_ac_remote_model_t

TCL (& Teknopoint) A/C model numbers.

Enumerator
TAC09CHSD |
GZ055BE1 |

## ◆ voltas_ac_remote_model_t

enum voltas_ac_remote_model_t

Voltas A/C model numbers.

Enumerator
kVoltasUnknown |
kVoltas122LZF |

## ◆ whirlpool_ac_remote_model_t

enum whirlpool_ac_remote_model_t

Whirlpool A/C model numbers.

Enumerator
DG11J13A |
DG11J191 |

## Variable Documentation

## ◆ kDefaultMessageGap

const uint32_t kDefaultMessageGap = 100000

## ◆ kDutyDefault

const uint8_t kDutyDefault = 50

## ◆ kDutyMax

const uint8_t kDutyMax = 100

## ◆ kMaxAccurateUsecDelay

const uint16_t kMaxAccurateUsecDelay = 16383

## ◆ kNoTempValue

const float kNoTempValue = -100.0

Placeholder for missing sensor temp value.

Note
  Not using "-1" as it may be a valid external temp

## ◆ kPeriodOffset

const int8_t kPeriodOffset = -2