IRremoteESP8266

IRBosch144AC Member List

This is the complete list of members for IRBosch144AC, including all inherited members.

_ | IRBosch144AC | private
_irsend | IRBosch144AC | private
begin() | IRBosch144AC |
calibrate(void) | IRBosch144AC | inline
convertFan(const stdAc::fanspeed_t speed) | IRBosch144AC | static
convertMode(const stdAc::opmode_t mode) | IRBosch144AC | static
getFan(void) const | IRBosch144AC |
getMode(void) const | IRBosch144AC |
getPower(void) const | IRBosch144AC |
getQuiet(void) const | IRBosch144AC |
getRaw(void) | IRBosch144AC |
getTemp(void) const | IRBosch144AC |
getTempRaw(void) const | IRBosch144AC | private
IRBosch144AC(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRBosch144AC | explicit
powerFlag | IRBosch144AC | private
send(const uint16_t repeat=0) | IRBosch144AC |
setCheckSumS3() | IRBosch144AC | private
setFan(const uint16_t speed) | IRBosch144AC |
setInvertBytes() | IRBosch144AC | private
setMode(const uint8_t mode) | IRBosch144AC |
setPower(const bool state) | IRBosch144AC |
setQuiet(const bool on) | IRBosch144AC |
setRaw(const uint8_t new_code[], const uint16_t length=kBosch144StateLength) | IRBosch144AC |
setTemp(const uint8_t temp) | IRBosch144AC |
setTempRaw(const uint8_t code) | IRBosch144AC | private
stateReset(void) | IRBosch144AC |
toCommon(void) const | IRBosch144AC |
toCommonFanSpeed(const uint16_t speed) | IRBosch144AC | static
toCommonMode(const uint8_t mode) | IRBosch144AC | static
toString(void) const | IRBosch144AC |