IRremoteESP8266

IRSanyoAc Member List

This is the complete list of members for IRSanyoAc, including all inherited members.

_ | IRSanyoAc | private
_irsend | IRSanyoAc | private
begin(void) | IRSanyoAc |
calcChecksum(const uint8_t state[], const uint16_t length=kSanyoAcStateLength) | IRSanyoAc | private static
calibrate(void) | IRSanyoAc | inline
checksum(void) | IRSanyoAc | private
convertFan(const stdAc::fanspeed_t speed) | IRSanyoAc | static
convertMode(const stdAc::opmode_t mode) | IRSanyoAc | static
convertSwingV(const stdAc::swingv_t position) | IRSanyoAc | static
getBeep(void) const | IRSanyoAc |
getFan(void) const | IRSanyoAc |
getMode(void) const | IRSanyoAc |
getOffTimer(void) const | IRSanyoAc |
getPower(void) const | IRSanyoAc |
getRaw(void) | IRSanyoAc |
getSensor(void) const | IRSanyoAc |
getSensorTemp(void) const | IRSanyoAc |
getSleep(void) const | IRSanyoAc |
getSwingV(void) const | IRSanyoAc |
getTemp(void) const | IRSanyoAc |
IRSanyoAc(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRSanyoAc | explicit
off(void) | IRSanyoAc |
on(void) | IRSanyoAc |
send(const uint16_t repeat=kNoRepeat) | IRSanyoAc |
setBeep(const bool on) | IRSanyoAc |
setFan(const uint8_t speed) | IRSanyoAc |
setMode(const uint8_t mode) | IRSanyoAc |
setOffTimer(const uint16_t mins) | IRSanyoAc |
setPower(const bool on) | IRSanyoAc |
setRaw(const uint8_t newState[]) | IRSanyoAc |
setSensor(const bool location) | IRSanyoAc |
setSensorTemp(const uint8_t degrees) | IRSanyoAc |
setSleep(const bool on) | IRSanyoAc |
setSwingV(const uint8_t setting) | IRSanyoAc |
setTemp(const uint8_t degrees) | IRSanyoAc |
stateReset(void) | IRSanyoAc |
toCommon(void) const | IRSanyoAc |
toCommonFanSpeed(const uint8_t speed) | IRSanyoAc | static
toCommonMode(const uint8_t mode) | IRSanyoAc | static
toCommonSwingV(const uint8_t setting) | IRSanyoAc | static
toString(void) const | IRSanyoAc |
validChecksum(const uint8_t state[], const uint16_t length=kSanyoAcStateLength) | IRSanyoAc | static