IRremoteESP8266

Public Member Functions | Static Public Member Functions | Public Attributes | Private Member Functions | Static Private Member Functions | Private Attributes | List of all members
IRac Class Reference

A universal/common/generic interface for controling supported A/Cs. More...

`#include <IRac.h>`

Collaboration diagram for IRac:
[legend]

## Public Member Functions
| IRac (const uint16_t pin, const bool inverted=false, const bool use_modulation=true)
| Class constructor. More...
void | markAsSent (void)
| Update the previous state to the current one. More...
bool | sendAc (void)
| Send an A/C message based soley on our internal state. More...
bool | sendAc (const stdAc::state_t desired, const stdAc::state_t *prev=NULL)
| Send A/C message for a given device using state_t structures. More...
bool | sendAc (const decode_type_t vendor, const int16_t model, const bool power, const stdAc::opmode_t mode, const float degrees, const bool celsius, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool light, const bool filter, const bool clean, const bool beep, const int16_t sleep=-1, const int16_t clock=-1)
| Send A/C message for a given device using common A/C settings. More...
stdAc::state_t | getState (void)
| Get the current internal A/C climate state. More...
stdAc::state_t | getStatePrev (void)
| Get the previous internal A/C climate state that should have already been sent to the device. i.e. What the A/C unit should already be set to. More...
bool | hasStateChanged (void)
| Check if the internal state has changed from what was previously sent. More...

## Static Public Member Functions
static bool | isProtocolSupported (const decode_type_t protocol)
| Is the given protocol supported by the IRac class? More...
static void | initState (stdAc::state_t *state, const decode_type_t vendor, const int16_t model, const bool power, const stdAc::opmode_t mode, const float degrees, const bool celsius, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool light, const bool filter, const bool clean, const bool beep, const int16_t sleep, const int16_t clock)
| Initialise the given state with the supplied settings. More...
static void | initState (stdAc::state_t *state)
| Initialise the given state with the supplied settings. More...
static bool | cmpStates (const stdAc::state_t a, const stdAc::state_t b)
| Compare two AirCon states. More...
static bool | strToBool (const char *str, const bool def=false)
| Convert the supplied str into the appropriate boolean value. More...
static int16_t | strToModel (const char *str, const int16_t def=-1)
| Convert the supplied str into the appropriate enum. More...
static stdAc::ac_command_t | strToCommandType (const char *str, const stdAc::ac_command_t def=stdAc::ac_command_t::kControlCommand)
| Convert the supplied str into the appropriate enum. More...
static stdAc::opmode_t | strToOpmode (const char *str, const stdAc::opmode_t def=stdAc::opmode_t::kAuto)
| Convert the supplied str into the appropriate enum. More...
static stdAc::fanspeed_t | strToFanspeed (const char *str, const stdAc::fanspeed_t def=stdAc::fanspeed_t::kAuto)
| Convert the supplied str into the appropriate enum. More...
static stdAc::swingv_t | strToSwingV (const char *str, const stdAc::swingv_t def=stdAc::swingv_t::kOff)
| Convert the supplied str into the appropriate enum. More...
static stdAc::swingh_t | strToSwingH (const char *str, const stdAc::swingh_t def=stdAc::swingh_t::kOff)
| Convert the supplied str into the appropriate enum. More...
static String | boolToString (const bool value)
| Convert the supplied boolean into the appropriate String. More...
static String | commandTypeToString (const stdAc::ac_command_t cmdType)
| Convert the supplied operation mode into the appropriate String. More...
static String | opmodeToString (const stdAc::opmode_t mode, const bool ha=false)
| Convert the supplied operation mode into the appropriate String. More...
static String | fanspeedToString (const stdAc::fanspeed_t speed)
| Convert the supplied fan speed enum into the appropriate String. More...
static String | swingvToString (const stdAc::swingv_t swingv)
| Convert the supplied enum into the appropriate String. More...
static String | swinghToString (const stdAc::swingh_t swingh)
| Convert the supplied enum into the appropriate String. More...

## Public Attributes
stdAc::state_t | next
| The state we want the device to be in after we send. More...

## Private Member Functions
void | airton (IRAirtonAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool light, const bool econo, const bool filter, const int16_t sleep=-1)
| Send an Airton 56-bit A/C message with the supplied settings. More...
void | airwell (IRAirwellAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan)
| Send an Airwell A/C message with the supplied settings. More...
void | amcor (IRAmcorAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan)
| Send an Amcor A/C message with the supplied settings. More...
void | argo (IRArgoAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool iFeel, const bool turbo, const int16_t sleep=-1)
| Send an Argo A/C message with the supplied settings. More...
void | argoWrem3_ACCommand (IRArgoAC_WREM3 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool iFeel, const bool night, const bool econo, const bool turbo, const bool filter, const bool light)
| Send an Argo A/C WREM-3 AC control message with the supplied settings. More...
void | argoWrem3_iFeelReport (IRArgoAC_WREM3 *ac, const float sensorTemp)
| Send an Argo A/C WREM-3 iFeel (room temp) silent (no beep) report. More...
void | argoWrem3_ConfigSet (IRArgoAC_WREM3 *ac, const uint8_t param, const uint8_t value, bool safe=true)
| Send an Argo A/C WREM-3 Config command. More...
void | argoWrem3_SetTimer (IRArgoAC_WREM3 *ac, bool on, const uint16_t currentTime, const uint16_t delayMinutes)
| Send an Argo A/C WREM-3 Delay timer command. More...
void | bosch144 (IRBosch144AC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const bool quiet)
| Send a Bosch144 A/C message with the supplied settings. More...
void | carrier64 (IRCarrierAc64 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const int16_t sleep=-1)
| Send a Carrier 64-bit A/C message with the supplied settings. More...
void | coolix (IRCoolixAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool iFeel, const bool turbo, const bool light, const bool clean, const int16_t sleep=-1)
| Send a Coolix A/C message with the supplied settings. More...
void | corona (IRCoronaAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool econo)
| Send a Corona A/C message with the supplied settings. More...
void | daikin (IRDaikinESP *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool clean)
| Send a Daikin A/C message with the supplied settings. More...
void | daikin128 (IRDaikin128 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet, const bool turbo, const bool light, const bool econo, const int16_t sleep=-1, const int16_t clock=-1)
| Send a Daikin 128-bit A/C message with the supplied settings. More...
void | daikin152 (IRDaikin152 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet, const bool turbo, const bool econo)
| Send a Daikin 152-bit A/C message with the supplied settings. More...
void | daikin160 (IRDaikin160 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv)
| Send a Daikin 160-bit A/C message with the supplied settings. More...
void | daikin176 (IRDaikin176 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingh_t swingh)
| Send a Daikin 176-bit A/C message with the supplied settings. More...
void | daikin2 (IRDaikin2 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool light, const bool econo, const bool filter, const bool clean, const bool beep, const int16_t sleep=-1, const int16_t clock=-1)
| Send a Daikin2 A/C message with the supplied settings. More...
void | daikin216 (IRDaikin216 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo)
| Send a Daikin 216-bit A/C message with the supplied settings. More...
void | daikin64 (IRDaikin64 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet, const bool turbo, const int16_t sleep=-1, const int16_t clock=-1)
| Send a Daikin 64-bit A/C message with the supplied settings. More...
void | delonghiac (IRDelonghiAc *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const bool turbo, const int16_t sleep=-1)
| Send a Delonghi A/C message with the supplied settings. More...
void | ecoclim (IREcoclimAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const int16_t sleep=-1, const int16_t clock=-1)
| Send an EcoClim A/C message with the supplied settings. More...
void | electra (IRElectraAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool iFeel, const bool turbo, const bool lighttoggle, const bool clean)
| Send an Electra A/C message with the supplied settings. More...
void | fujitsu (IRFujitsuAC *ac, const fujitsu_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool filter, const bool clean, const int16_t sleep=-1)
| Send a Fujitsu A/C message with the supplied settings. More...
void | goodweather (IRGoodweatherAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool light, const int16_t sleep=-1)
| Send a Goodweather A/C message with the supplied settings. More...
void | gree (IRGreeAC *ac, const gree_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool iFeel, const bool turbo, const bool econo, const bool light, const bool clean, const int16_t sleep=-1)
| Send a Gree A/C message with the supplied settings. More...
void | haier (IRHaierAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool filter, const int16_t sleep=-1, const int16_t clock=-1)
| Send a Haier A/C message with the supplied settings. More...
void | haier160 (IRHaierAC160 *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool quiet, const bool filter, const bool clean, const bool light, const bool prevlight, const int16_t sleep=-1)
| Send a Haier 160 bit A/C message with the supplied settings. More...
void | haier176 (IRHaierAC176 *ac, const haier_ac176_remote_model_t model, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool quiet, const bool filter, const int16_t sleep=-1)
| Send a Haier 176 bit A/C message with the supplied settings. More...
void | haierYrwo2 (IRHaierACYRW02 *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool quiet, const bool filter, const int16_t sleep=-1)
| Send a Haier YRWO2 A/C message with the supplied settings. More...
void | hitachi (IRHitachiAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh)
| Send a Hitachi A/C message with the supplied settings. More...
void | hitachi1 (IRHitachiAc1 *ac, const hitachi_ac1_remote_model_t model, const bool on, const bool power_toggle, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool swing_toggle, const int16_t sleep=-1)
| Send a Hitachi1 A/C message with the supplied settings. More...
void | hitachi264 (IRHitachiAc264 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan)
| Send a Hitachi 264-bit A/C message with the supplied settings. More...
void | hitachi296 (IRHitachiAc296 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan)
| Send a Hitachi 296-bit A/C message with the supplied settings. More...
void | hitachi344 (IRHitachiAc344 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh)
| Send a Hitachi 344-bit A/C message with the supplied settings. More...
void | hitachi424 (IRHitachiAc424 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv)
| Send a Hitachi 424-bit A/C message with the supplied settings. More...
void | kelon (IRKelonAc *ac, const bool togglePower, const stdAc::opmode_t mode, const int8_t dryGrade, const float degrees, const stdAc::fanspeed_t fan, const bool toggleSwing, const bool superCool, const int16_t sleep)
| Send a Kelon A/C message with the supplied settings. More...
void | kelvinator (IRKelvinatorAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool light, const bool filter, const bool clean)
| Send a Kelvinator A/C message with the supplied settings. More...
void | lg (IRLgAc *ac, const lg_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingv_t swingv_prev, const stdAc::swingh_t swingh, const bool light)
| Send a LG A/C message with the supplied settings. More...
void | midea (IRMideaAC *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool iFeel, const bool quiet, const bool quiet_prev, const bool turbo, const bool econo, const bool light, const bool clean, const int16_t sleep=-1)
| Send a Midea A/C message with the supplied settings. More...
void | mirage (IRMirageAc *ac, const stdAc::state_t state)
| Send a Mirage 120-bit A/C message with the supplied settings. More...
void | mitsubishi (IRMitsubishiAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const int16_t clock=-1)
| Send a Mitsubishi A/C message with the supplied settings. More...
void | mitsubishi112 (IRMitsubishi112 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet)
| Send a Mitsubishi 112-bit A/C message with the supplied settings. More...
void | mitsubishi136 (IRMitsubishi136 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool quiet)
| Send a Mitsubishi 136-bit A/C message with the supplied settings. More...
void | mitsubishiHeavy88 (IRMitsubishiHeavy88Ac *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool econo, const bool clean)
| Send a Mitsubishi Heavy 88-bit A/C message with the supplied settings. More...
void | mitsubishiHeavy152 (IRMitsubishiHeavy152Ac *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool filter, const bool clean, const int16_t sleep=-1)
| Send a Mitsubishi Heavy 152-bit A/C message with the supplied settings. More...
void | neoclima (IRNeoclimaAc *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool econo, const bool light, const bool filter, const int16_t sleep=-1)
| Send a Neoclima A/C message with the supplied settings. More...
void | panasonic (IRPanasonicAc *ac, const panasonic_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool filter, const int16_t clock=-1)
| Send a Panasonic A/C message with the supplied settings. More...
void | panasonic32 (IRPanasonicAc32 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh)
| Send a Panasonic A/C message with the supplied settings. More...
void | rhoss (IRRhossAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swing)
| Send an Rhoss A/C message with the supplied settings. More...
void | samsung (IRSamsungAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool econo, const bool light, const bool filter, const bool clean, const bool beep, const int16_t sleep=-1, const bool prevpower=true, const int16_t prevsleep=-1, const bool forceextended=true)
| Send a Samsung A/C message with the supplied settings. More...
void | sanyo (IRSanyoAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const float sensorTemp, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool iFeel, const bool beep, const int16_t sleep=-1)
| Send a Sanyo A/C message with the supplied settings. More...
void | sanyo88 (IRSanyoAc88 *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool filter, const int16_t sleep=-1, const int16_t clock=-1)
| Send a Sanyo 88-bit A/C message with the supplied settings. More...
void | sharp (IRSharpAc *ac, const sharp_ac_remote_model_t model, const bool on, const bool prev_power, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingv_t swingv_prev, const bool turbo, const bool light, const bool filter, const bool clean)
| Send a Sharp A/C message with the supplied settings. More...
void | tcl112 (IRTcl112Ac *ac, const tcl_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool quiet, const bool turbo, const bool light, const bool econo, const bool filter)
| Send a TCL 112-bit A/C message with the supplied settings. More...
void | technibel (IRTechnibelAc *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const int16_t sleep=-1)
| Send a Technibel A/C message with the supplied settings. More...
void | teco (IRTecoAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool light, const int16_t sleep=-1)
| Send a Teco A/C message with the supplied settings. More...
void | toshiba (IRToshibaAC *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool econo, const bool filter)
| Send a Toshiba A/C message with the supplied settings. More...
void | trotec (IRTrotecESP *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const int16_t sleep=-1)
| Send a Trotec A/C message with the supplied settings. More...
void | trotec3550 (IRTrotec3550 *ac, const bool on, const stdAc::opmode_t mode, const bool celsius, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv)
| Send a Trotec 3550 A/C message with the supplied settings. More...
void | truma (IRTrumaAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const bool quiet)
| Send a Truma A/C message with the supplied settings. More...
void | vestel (IRVestelAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool filter, const int16_t sleep=-1, const int16_t clock=-1, const bool sendNormal=true)
| Send a Vestel A/C message with the supplied settings. More...
void | voltas (IRVoltas *ac, const voltas_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh, const bool turbo, const bool econo, const bool light, const int16_t sleep=-1)
| Send a Voltas A/C message with the supplied settings. More...
void | whirlpool (IRWhirlpoolAc *ac, const whirlpool_ac_remote_model_t model, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const bool turbo, const bool light, const int16_t sleep=-1, const int16_t clock=-1)
| Send a Whirlpool A/C message with the supplied settings. More...
void | transcold (IRTranscoldAc *ac, const bool on, const stdAc::opmode_t mode, const float degrees, const stdAc::fanspeed_t fan, const stdAc::swingv_t swingv, const stdAc::swingh_t swingh)
| Send a Transcold A/C message with the supplied settings. More...

## Static Private Member Functions
static stdAc::state_t | cleanState (const stdAc::state_t state)
| Create a new state base on the provided state that has been suitably fixed. More...
static stdAc::state_t | handleToggles (const stdAc::state_t desired, const stdAc::state_t *prev=NULL)
| Create a new state base on desired & previous states but handle any state changes for options that need to be toggled. More...

## Private Attributes
uint16_t | _pin
| The GPIO to use to transmit messages from. More...
bool | _inverted
| IR LED is lit when GPIO is LOW (true) or HIGH (false)? More...
bool | _modulation
| Is frequency modulation to be used? More...
stdAc::state_t | _prev
| The state we expect the device to currently be in. More...

## Detailed Description

A universal/common/generic interface for controling supported A/Cs.

## Constructor & Destructor Documentation

## ◆ IRac()

IRac::IRac | ( | const uint16_t | pin,
|  | const bool | inverted = `false`,
|  | const bool | use_modulation = `true`
| ) |  |
| explicit

Class constructor.

Parameters

  [in] | pin | Gpio pin to use when transmitting IR messages.
  [in] | inverted | true, gpio output defaults to high. false, to low.
  [in] | use_modulation | true means use frequency modulation. false, don't.

## Member Function Documentation

## ◆ airton()

void IRac::airton | ( | IRAirtonAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | econo,
|  | const bool | filter,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send an Airton 56-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRAirtonAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | econo | Run the device in economical mode.
  [in] | filter | Turn on the (ion/pollen/health/etc) filter mode.
  [in] | sleep | Nr. of minutes for sleep mode.

Note
  -1 is Off, >= 0 is on.

## ◆ airwell()

void IRac::airwell | ( | IRAirwellAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan
| ) |  |
| private

Send an Airwell A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRAirwellAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.

## ◆ amcor()

void IRac::amcor | ( | IRAmcorAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan
| ) |  |
| private

Send an Amcor A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRAmcorAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.

## ◆ argo()

void IRac::argo | ( | IRArgoAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const float | sensorTemp,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | iFeel,
|  | const bool | turbo,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send an Argo A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRArgoAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | sensorTemp | The room (iFeel) temperature sensor reading in degrees Celsius.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | iFeel | Whether to enable iFeel (remote temp) mode on the A/C unit.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | sleep | Nr. of minutes for sleep mode.

Note
  -1 is Off, >= 0 is on.

## ◆ argoWrem3_ACCommand()

void IRac::argoWrem3_ACCommand | ( | IRArgoAC_WREM3 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const float | sensorTemp,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | iFeel,
|  | const bool | night,
|  | const bool | econo,
|  | const bool | turbo,
|  | const bool | filter,
|  | const bool | light
| ) |  |
| private

Send an Argo A/C WREM-3 AC control message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRArgoAC_WREM3 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The set temperature setting in degrees Celsius.
  [in] | sensorTemp | The room (iFeel) temperature sensor reading in degrees Celsius.

Warning
  The `sensorTemp` param is assumed to be in 0..255 range (uint8_t) The overflow is not checked, though.

Note
  The value is rounded to nearest integer, rounding halfway cases away from zero. E.g. 1.5 [C] becomes 2 [C].

Parameters

  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | iFeel | Whether to enable iFeel (remote temp) mode on the A/C unit.
  [in] | night | Enable night mode (raises temp by +1*C after 1h).
  [in] | econo | Enable eco mode (limits power consumed).
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | filter | Enable filter mode
  [in] | light | Enable device display/LEDs

## ◆ argoWrem3_ConfigSet()

void IRac::argoWrem3_ConfigSet | ( | IRArgoAC_WREM3 * | ac,
|  | const uint8_t | param,
|  | const uint8_t | value,
|  | bool | safe = `true`
| ) |  |
| private

Send an Argo A/C WREM-3 Config command.

Parameters

  [in,out] | ac | A Ptr to an IRArgoAC_WREM3 object to use.
  [in] | param | The parameter ID.
  [in] | value | The parameter value.
  [in] | safe | If true, will only allow setting the below parameters in order to avoid accidentally setting a restricted vendor-specific param and breaking the A/C device

Note
  Known parameters (P<xx>, where xx is the `param`) P05 - Temperature Scale (0-Celsius, 1-Fahrenheit) P06 - Transmission channel (0..3) P12 - ECO mode power input limit (30..99, default: 75)

## ◆ argoWrem3_iFeelReport()

void IRac::argoWrem3_iFeelReport | ( | IRArgoAC_WREM3 * | ac,
|  | const float | sensorTemp
| ) |  |
| private

Send an Argo A/C WREM-3 iFeel (room temp) silent (no beep) report.

Parameters

  [in,out] | ac | A Ptr to an IRArgoAC_WREM3 object to use.
  [in] | sensorTemp | The room (iFeel) temperature setting in degrees Celsius.

Warning
  The `sensorTemp` param is assumed to be in 0..255 range (uint8_t) The overflow is not checked, though.

Note
  The value is rounded to nearest integer, rounding halfway cases away from zero. E.g. 1.5 [C] becomes 2 [C].

## ◆ argoWrem3_SetTimer()

void IRac::argoWrem3_SetTimer | ( | IRArgoAC_WREM3 * | ac,
|  | bool | on,
|  | const uint16_t | currentTime,
|  | const uint16_t | delayMinutes
| ) |  |
| private

Send an Argo A/C WREM-3 Delay timer command.

Parameters

  [in,out] | ac | A Ptr to an IRArgoAC_WREM3 object to use.
  [in] | on | Whether the unit is currently on. The timer, upon elapse will toggle this state
  [in] | currentTime | currentTime in minutes, starting from 00:00

Note
  For timer mode, this value is not really used much so can be zero.

Parameters

  [in] | delayMinutes | Number of minutes after which the `on` state should be toggled

Note
  Schedule timers are not exposed via this interface

## ◆ boolToString()

String IRac::boolToString | ( | const bool | value | ) |
| static

Convert the supplied boolean into the appropriate String.

Parameters

  [in] | value | The boolean value to be converted.

Returns
  The equivalent String for the locale.

## ◆ bosch144()

void IRac::bosch144 | ( | IRBosch144AC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const bool | quiet
| ) |  |
| private

Send a Bosch144 A/C message with the supplied settings.

Note
  May result in multiple messages being sent.

Parameters

  [in,out] | ac | A Ptr to an IRBosch144AC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | quiet | Run the device in quiet/silent mode.

Note
  -1 is Off, >= 0 is on.

## ◆ carrier64()

void IRac::carrier64 | ( | IRCarrierAc64 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Carrier 64-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRCarrierAc64 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | sleep | Nr. of minutes for sleep mode.

Note
  -1 is Off, >= 0 is on.

## ◆ cleanState()

stdAc::state_t IRac::cleanState | ( | const stdAc::state_t | state | ) |
| static private

Create a new state base on the provided state that has been suitably fixed.

Note
  This is for use with Home Assistant, which requires mode to be off if the power is off.

Parameters

  [in] | state | The state_t structure describing the desired a/c state.

Returns
  A stdAc::state_t with the needed settings.

## ◆ cmpStates()

bool IRac::cmpStates | ( | const stdAc::state_t | a,
|  | const stdAc::state_t | b
| ) |  |
| static

Compare two AirCon states.

Note
  The comparison excludes the clock.

Parameters

  a | A state_t to be compared.
  b | A state_t to be compared.

Returns
  True if they differ, False if they don't.

## ◆ commandTypeToString()

String IRac::commandTypeToString | ( | const stdAc::ac_command_t | cmdType | ) |
| static

Convert the supplied operation mode into the appropriate String.

Parameters

  [in] | cmdType | The enum to be converted.

Returns
  The equivalent String for the locale.

## ◆ coolix()

void IRac::coolix | ( | IRCoolixAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const float | sensorTemp,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | iFeel,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | clean,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Coolix A/C message with the supplied settings.

Note
  May result in multiple messages being sent.

Parameters

  [in,out] | ac | A Ptr to an IRCoolixAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | sensorTemp | The room (iFeel) temperature sensor reading in degrees Celsius.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | iFeel | Whether to enable iFeel (remote temp) mode on the A/C unit.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | sleep | Nr. of minutes for sleep mode.

Note
  -1 is Off, >= 0 is on.

## ◆ corona()

void IRac::corona | ( | IRCoronaAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | econo
| ) |  |
| private

Send a Corona A/C message with the supplied settings.

Note
  May result in multiple messages being sent.

Parameters

  [in,out] | ac | A Ptr to an IRCoronaAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | econo | Run the device in economical mode.

## ◆ daikin()

void IRac::daikin | ( | IRDaikinESP * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | clean
| ) |  |
| private

Send a Daikin A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikinESP object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc

## ◆ daikin128()

void IRac::daikin128 | ( | IRDaikin128 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | econo,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |
| private

Send a Daikin 128-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin128 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | econo | Run the device in economical mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## ◆ daikin152()

void IRac::daikin152 | ( | IRDaikin152 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo
| ) |  |
| private

Send a Daikin 152-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin152 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.

## ◆ daikin160()

void IRac::daikin160 | ( | IRDaikin160 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv
| ) |  |
| private

Send a Daikin 160-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin160 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.

## ◆ daikin176()

void IRac::daikin176 | ( | IRDaikin176 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingh_t | swingh
| ) |  |
| private

Send a Daikin 176-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin176 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingh | The horizontal swing setting.

## ◆ daikin2()

void IRac::daikin2 | ( | IRDaikin2 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | econo,
|  | const bool | filter,
|  | const bool | clean,
|  | const bool | beep,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |
| private

Send a Daikin2 A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin2 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | econo | Run the device in economical mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | beep | Enable/Disable beeps when receiving IR messages.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## ◆ daikin216()

void IRac::daikin216 | ( | IRDaikin216 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo
| ) |  |
| private

Send a Daikin 216-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin216 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.

## ◆ daikin64()

void IRac::daikin64 | ( | IRDaikin64 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |
| private

Send a Daikin 64-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDaikin64 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## ◆ delonghiac()

void IRac::delonghiac | ( | IRDelonghiAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const bool | turbo,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Delonghi A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRDelonghiAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ ecoclim()

void IRac::ecoclim | ( | IREcoclimAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const float | sensorTemp,
|  | const stdAc::fanspeed_t | fan,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |
| private

Send an EcoClim A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IREcoclimAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | sensorTemp | The room (iFeel) temperature sensor reading in degrees Celsius.
  [in] | fan | The speed setting for the fan.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## ◆ electra()

void IRac::electra | ( | IRElectraAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const float | sensorTemp,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | iFeel,
|  | const bool | turbo,
|  | const bool | lighttoggle,
|  | const bool | clean
| ) |  |
| private

Send an Electra A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRElectraAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | sensorTemp | The room (iFeel) temperature sensor reading in degrees Celsius.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | iFeel | Whether to enable iFeel (remote temp) mode on the A/C unit.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | lighttoggle | Should we toggle the LED/Display?
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc

## ◆ fanspeedToString()

String IRac::fanspeedToString | ( | const stdAc::fanspeed_t | speed | ) |
| static

Convert the supplied fan speed enum into the appropriate String.

Parameters

  [in] | speed | The enum to be converted.

Returns
  The equivalent String for the locale.

## ◆ fujitsu()

void IRac::fujitsu | ( | IRFujitsuAC * | ac,
|  | const fujitsu_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | filter,
|  | const bool | clean,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Fujitsu A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRFujitsuAC object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | sleep | Nr. of minutes for sleep mode. <= 0 is Off, > 0 is on.

## ◆ getState()

stdAc::state_t IRac::getState | ( | void |  | ) |

Get the current internal A/C climate state.

Returns
  A Ptr to a state containing the current (to be sent) settings.

## ◆ getStatePrev()

stdAc::state_t IRac::getStatePrev | ( | void |  | ) |

Get the previous internal A/C climate state that should have already been sent to the device. i.e. What the A/C unit should already be set to.

Returns
  A Ptr to a state containing the previously sent settings.

## ◆ goodweather()

void IRac::goodweather | ( | IRGoodweatherAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | light,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Goodweather A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRGoodweatherAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ gree()

void IRac::gree | ( | IRGreeAC * | ac,
|  | const gree_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | iFeel,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | light,
|  | const bool | clean,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Gree A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRGreeAC object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | iFeel | Whether to enable iFeel (remote temp) mode on the A/C unit.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Toggle the device's economical mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ haier()

void IRac::haier | ( | IRHaierAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | filter,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |
| private

Send a Haier A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRGreeAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## ◆ haier160()

void IRac::haier160 | ( | IRHaierAC160 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | quiet,
|  | const bool | filter,
|  | const bool | clean,
|  | const bool | light,
|  | const bool | prevlight,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Haier 160 bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHaierAC160 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | quiet | Run the device in quiet mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the clean mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | prevlight | Previous LED/Display mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ haier176()

void IRac::haier176 | ( | IRHaierAC176 * | ac,
|  | const haier_ac176_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | turbo,
|  | const bool | quiet,
|  | const bool | filter,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Haier 176 bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHaierAC176 object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | quiet | Run the device in quiet mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ haierYrwo2()

void IRac::haierYrwo2 | ( | IRHaierACYRW02 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | turbo,
|  | const bool | quiet,
|  | const bool | filter,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Haier YRWO2 A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHaierACYRW02 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | quiet | Run the device in quiet mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ handleToggles()

stdAc::state_t IRac::handleToggles | ( | const stdAc::state_t | desired,
|  | const stdAc::state_t * | prev = `NULL`
| ) |  |
| static private

Create a new state base on desired & previous states but handle any state changes for options that need to be toggled.

Parameters

  [in] | desired | The state_t structure describing the desired a/c state.
  [in] | prev | A Ptr to the previous state_t structure.

Returns
  A stdAc::state_t with the needed settings.

## ◆ hasStateChanged()

bool IRac::hasStateChanged | ( | void |  | ) |

Check if the internal state has changed from what was previously sent.

Note
  The comparison excludes the clock.

Returns
  True if it has changed, False if not.

## ◆ hitachi()

void IRac::hitachi | ( | IRHitachiAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh
| ) |  |
| private

Send a Hitachi A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHitachiAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.

## ◆ hitachi1()

void IRac::hitachi1 | ( | IRHitachiAc1 * | ac,
|  | const hitachi_ac1_remote_model_t | model,
|  | const bool | on,
|  | const bool | power_toggle,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | swing_toggle,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Hitachi1 A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHitachiAc1 object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | power_toggle | The power toggle setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | swing_toggle | The swing_toggle setting.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

Note
  The sleep mode used is the "Sleep 2" setting.

## ◆ hitachi264()

void IRac::hitachi264 | ( | IRHitachiAc264 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan
| ) |  |
| private

Send a Hitachi 264-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHitachiAc264 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.

## ◆ hitachi296()

void IRac::hitachi296 | ( | IRHitachiAc296 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan
| ) |  |
| private

Send a Hitachi 296-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHitachiAc296 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.

## ◆ hitachi344()

void IRac::hitachi344 | ( | IRHitachiAc344 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh
| ) |  |
| private

Send a Hitachi 344-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHitachiAc344 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.

## ◆ hitachi424()

void IRac::hitachi424 | ( | IRHitachiAc424 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv
| ) |  |
| private

Send a Hitachi 424-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRHitachiAc424 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.

## ◆ initState() [1/2]

void IRac::initState | ( | stdAc::state_t * | state | ) |
| static

Initialise the given state with the supplied settings.

Parameters

  [out] | state | A Ptr to where the settings will be stored.

Note
  Sets all the parameters to reasonable base/automatic defaults.

## ◆ initState() [2/2]

void IRac::initState | ( | stdAc::state_t * | state,
|  | const decode_type_t | vendor,
|  | const int16_t | model,
|  | const bool | power,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const bool | celsius,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | light,
|  | const bool | filter,
|  | const bool | clean,
|  | const bool | beep,
|  | const int16_t | sleep,
|  | const int16_t | clock
| ) |  |
| static

Initialise the given state with the supplied settings.

Parameters

  [out] | state | A Ptr to where the settings will be stored.
  [in] | vendor | The vendor/protocol type.
  [in] | model | The A/C model if applicable.
  [in] | power | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | beep | Enable/Disable beeps when receiving IR messages.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on. Some devices it is the nr. of mins to run for. Others it may be the time to enter/exit sleep mode. i.e. Time in Nr. of mins since midnight.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## ◆ isProtocolSupported()

bool IRac::isProtocolSupported | ( | const decode_type_t | protocol | ) |
| static

Is the given protocol supported by the IRac class?

Parameters

  [in] | protocol | The vendor/protocol type.

Returns
  true if the protocol is supported by this class, otherwise false.

## ◆ kelon()

void IRac::kelon | ( | IRKelonAc * | ac,
|  | const bool | togglePower,
|  | const stdAc::opmode_t | mode,
|  | const int8_t | dryGrade,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const bool | toggleSwing,
|  | const bool | superCool,
|  | const int16_t | sleep
| ) |  |
| private

Send a Kelon A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRKelonAc object to use.
  [in] | togglePower | Whether to toggle the unit's power
  [in] | mode | The operation mode setting.
  [in] | dryGrade | The dehumidification intensity grade
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | toggleSwing | Whether to toggle the swing setting
  [in] | superCool | Run the device in Super cooling mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on

## ◆ kelvinator()

void IRac::kelvinator | ( | IRKelvinatorAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | filter,
|  | const bool | clean
| ) |  |
| private

Send a Kelvinator A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRKelvinatorAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. XFan, dry filters etc

## ◆ lg()

void IRac::lg | ( | IRLgAc * | ac,
|  | const lg_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingv_t | swingv_prev,
|  | const stdAc::swingh_t | swingh,
|  | const bool | light
| ) |  |
| private

Send a LG A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRLgAc object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingv_prev | The previous vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | light | Turn on the LED/Display mode.

## ◆ markAsSent()

void IRac::markAsSent | ( | void |  | ) |

Update the previous state to the current one.

## ◆ midea()

void IRac::midea | ( | IRMideaAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const float | sensorTemp,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | iFeel,
|  | const bool | quiet,
|  | const bool | quiet_prev,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | light,
|  | const bool | clean,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Midea A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMideaAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | sensorTemp | The room (iFeel) temperature sensor reading in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | iFeel | Whether to enable iFeel (remote temp) mode on the A/C unit.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | quiet_prev | The device's previous quiet/silent mode.
  [in] | turbo | Toggle the device's turbo/powerful mode.
  [in] | econo | Toggle the device's economical mode.
  [in] | light | Toggle the LED/Display mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. XFan, dry filters etc
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

Note
  On Danby A/C units, swingv controls the Ion Filter instead.

## ◆ mirage()

void IRac::mirage | ( | IRMirageAc * | ac,
|  | const stdAc::state_t | state
| ) |  |
| private

Send a Mirage 120-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMitsubishiAC object to use.
  [in] | state | The desired state to send.

## ◆ mitsubishi()

void IRac::mitsubishi | ( | IRMitsubishiAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const int16_t | clock = `-1`
| ) |  |
| private

Send a Mitsubishi A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMitsubishiAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

Note
  Clock can only be set in 10 minute increments. i.e. % 10.

## ◆ mitsubishi112()

void IRac::mitsubishi112 | ( | IRMitsubishi112 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet
| ) |  |
| private

Send a Mitsubishi 112-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMitsubishi112 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.

## ◆ mitsubishi136()

void IRac::mitsubishi136 | ( | IRMitsubishi136 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | quiet
| ) |  |
| private

Send a Mitsubishi 136-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMitsubishi136 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | quiet | Run the device in quiet/silent mode.

## ◆ mitsubishiHeavy152()

void IRac::mitsubishiHeavy152 | ( | IRMitsubishiHeavy152Ac * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | filter,
|  | const bool | clean,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Mitsubishi Heavy 152-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMitsubishiHeavy152Ac object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ mitsubishiHeavy88()

void IRac::mitsubishiHeavy88 | ( | IRMitsubishiHeavy88Ac * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | clean
| ) |  |
| private

Send a Mitsubishi Heavy 88-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRMitsubishiHeavy88Ac object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc

## ◆ neoclima()

void IRac::neoclima | ( | IRNeoclimaAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | light,
|  | const bool | filter,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Neoclima A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRNeoclimaAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ opmodeToString()

String IRac::opmodeToString | ( | const stdAc::opmode_t | mode,
|  | const bool | ha = `false`
| ) |  |
| static

Convert the supplied operation mode into the appropriate String.

Parameters

  [in] | mode | The enum to be converted.
  [in] | ha | A flag to indicate we want GoogleHome/HomeAssistant output.

Returns
  The equivalent String for the locale.

## ◆ panasonic()

void IRac::panasonic | ( | IRPanasonicAc * | ac,
|  | const panasonic_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | filter,
|  | const int16_t | clock = `-1`
| ) |  |
| private

Send a Panasonic A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRPanasonicAc object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## ◆ panasonic32()

void IRac::panasonic32 | ( | IRPanasonicAc32 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh
| ) |  |
| private

Send a Panasonic A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRPanasonicAc32 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.

## ◆ rhoss()

void IRac::rhoss | ( | IRRhossAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swing
| ) |  |
| private

Send an Rhoss A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRRhossAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swing | The swing setting.

## ◆ samsung()

void IRac::samsung | ( | IRSamsungAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | light,
|  | const bool | filter,
|  | const bool | clean,
|  | const bool | beep,
|  | const int16_t | sleep = `-1`,
|  | const bool | prevpower = `true`,
|  | const int16_t | prevsleep = `-1`,
|  | const bool | forceextended = `true`
| ) |  |
| private

Send a Samsung A/C message with the supplied settings.

Note
  Multiple IR messages may be generated & sent.

Parameters

  [in,out] | ac | A Ptr to an IRSamsungAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Toggle the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | beep | Toggle beep setting for receiving IR messages.
  [in] | sleep | Nr. of minutes for sleep mode. <= 0 is Off, > 0 is on.
  [in] | prevpower | The power setting from the previous A/C state.
  [in] | prevsleep | Nr. of minutes for sleep from the previous A/C state.
  [in] | forceextended | Do we force sending the special extended message?

## ◆ sanyo()

void IRac::sanyo | ( | IRSanyoAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const float | sensorTemp,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | iFeel,
|  | const bool | beep,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Sanyo A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRSanyoAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | sensorTemp | The room (iFeel) temperature sensor reading in degrees Celsius.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | iFeel | Whether to enable iFeel (remote temp) mode on the A/C unit.
  [in] | beep | Enable/Disable beeps when receiving IR messages.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ sanyo88()

void IRac::sanyo88 | ( | IRSanyoAc88 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | filter,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |
| private

Send a Sanyo 88-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRSanyoAc88 object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## ◆ sendAc() [1/3]

bool IRac::sendAc | ( | const decode_type_t | vendor,
|  | const int16_t | model,
|  | const bool | power,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const bool | celsius,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | light,
|  | const bool | filter,
|  | const bool | clean,
|  | const bool | beep,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |

Send A/C message for a given device using common A/C settings.

Parameters

  [in] | vendor | The vendor/protocol type.
  [in] | model | The A/C model if applicable.
  [in] | power | The power setting.
  [in] | mode | The operation mode setting.

Note
  Changing mode from "Off" to something else does NOT turn on a device. You need to use `power` for that.

Parameters

  [in] | degrees | The temperature setting in degrees.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | fan | The speed setting for the fan.

Note
  The following are all "if supported" by the underlying A/C classes.

Parameters

  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc
  [in] | beep | Enable/Disable beeps when receiving IR messages.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on. Some devices it is the nr. of mins to run for. Others it may be the time to enter/exit sleep mode. i.e. Time in Nr. of mins since midnight.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

Returns
  True, if accepted/converted/attempted etc. False, if unsupported.

## ◆ sendAc() [2/3]

bool IRac::sendAc | ( | const stdAc::state_t | desired,
|  | const stdAc::state_t * | prev = `NULL`
| ) |  |

Send A/C message for a given device using state_t structures.

Parameters

  [in] | desired | The state_t structure describing the desired new ac state
  [in] | prev | A Ptr to the state_t structure containing the previous state

Note
  Changing mode from "Off" to something else does NOT turn on a device. You need to use `power` for that.

Returns
  True, if accepted/converted/attempted etc. False, if unsupported.

Warning
  : this is ABUSING current common parameters: `clock` and `sleep` as config key and value Hence, value pre-validation is performed (safe-mode) to avoid accidental device misconfiguration

## ◆ sendAc() [3/3]

bool IRac::sendAc | ( | void |  | ) |

Send an A/C message based soley on our internal state.

Returns
  True, if accepted/converted/attempted. False, if unsupported.

## ◆ sharp()

void IRac::sharp | ( | IRSharpAc * | ac,
|  | const sharp_ac_remote_model_t | model,
|  | const bool | on,
|  | const bool | prev_power,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingv_t | swingv_prev,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | filter,
|  | const bool | clean
| ) |  |
| private

Send a Sharp A/C message with the supplied settings.

Note
  Multiple IR messages may be generated & sent.

Parameters

  [in,out] | ac | A Ptr to an IRSharpAc object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | prev_power | The power setting from the previous A/C state.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingv_prev | The previous vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | clean | Turn on the self-cleaning mode. e.g. Mould, dry filters etc

## ◆ strToBool()

bool IRac::strToBool | ( | const char * | str,
|  | const bool | def = `false`
| ) |  |
| static

Convert the supplied str into the appropriate boolean value.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The boolean value to return if no conversion was possible.

Returns
  The equivalent boolean value.

## ◆ strToCommandType()

stdAc::ac_command_t IRac::strToCommandType | ( | const char * | str,
|  | const stdAc::ac_command_t | def = `stdAc::ac_command_t::kControlCommand`
| ) |  |
| static

Convert the supplied str into the appropriate enum.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The enum to return if no conversion was possible.

Returns
  The equivalent enum.

## ◆ strToFanspeed()

stdAc::fanspeed_t IRac::strToFanspeed | ( | const char * | str,
|  | const stdAc::fanspeed_t | def = `stdAc::fanspeed_t::kAuto`
| ) |  |
| static

Convert the supplied str into the appropriate enum.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The enum to return if no conversion was possible.

Returns
  The equivalent enum.

## ◆ strToModel()

int16_t IRac::strToModel | ( | const char * | str,
|  | const int16_t | def = `-1`
| ) |  |
| static

Convert the supplied str into the appropriate enum.

Note
  Assumes str is the model code or an integer >= 1.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The enum to return if no conversion was possible.

Returns
  The equivalent enum.

Note
  After adding a new model you should update modelToStr() too.

## ◆ strToOpmode()

stdAc::opmode_t IRac::strToOpmode | ( | const char * | str,
|  | const stdAc::opmode_t | def = `stdAc::opmode_t::kAuto`
| ) |  |
| static

Convert the supplied str into the appropriate enum.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The enum to return if no conversion was possible.

Returns
  The equivalent enum.

## ◆ strToSwingH()

stdAc::swingh_t IRac::strToSwingH | ( | const char * | str,
|  | const stdAc::swingh_t | def = `stdAc::swingh_t::kOff`
| ) |  |
| static

Convert the supplied str into the appropriate enum.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The enum to return if no conversion was possible.

Returns
  The equivalent enum.

## ◆ strToSwingV()

stdAc::swingv_t IRac::strToSwingV | ( | const char * | str,
|  | const stdAc::swingv_t | def = `stdAc::swingv_t::kOff`
| ) |  |
| static

Convert the supplied str into the appropriate enum.

Parameters

  [in] | str | A Ptr to a C-style string to be converted.
  [in] | def | The enum to return if no conversion was possible.

Returns
  The equivalent enum.

## ◆ swinghToString()

String IRac::swinghToString | ( | const stdAc::swingh_t | swingh | ) |
| static

Convert the supplied enum into the appropriate String.

Parameters

  [in] | swingh | The enum to be converted.

Returns
  The equivalent String for the locale.

## ◆ swingvToString()

String IRac::swingvToString | ( | const stdAc::swingv_t | swingv | ) |
| static

Convert the supplied enum into the appropriate String.

Parameters

  [in] | swingv | The enum to be converted.

Returns
  The equivalent String for the locale.

## ◆ tcl112()

void IRac::tcl112 | ( | IRTcl112Ac * | ac,
|  | const tcl_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | quiet,
|  | const bool | turbo,
|  | const bool | light,
|  | const bool | econo,
|  | const bool | filter
| ) |  |
| private

Send a TCL 112-bit A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRTcl112Ac object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | quiet | Run the device in quiet/silent mode.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | econo | Run the device in economical mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.

## ◆ technibel()

void IRac::technibel | ( | IRTechnibelAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Technibel A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRTechnibelAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ teco()

void IRac::teco | ( | IRTecoAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | light,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Teco A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRTecoAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | light | Turn on the LED/Display mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ toshiba()

void IRac::toshiba | ( | IRToshibaAC * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | filter
| ) |  |
| private

Send a Toshiba A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRToshibaAC object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | filter | Turn on the (Pure/ion/pollen/etc) filter mode.

## ◆ transcold()

void IRac::transcold | ( | IRTranscoldAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh
| ) |  |
| private

Send a Transcold A/C message with the supplied settings.

Note
  May result in multiple messages being sent.

Parameters

  [in,out] | ac | A Ptr to an IRTranscoldAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.

Note
  -1 is Off, >= 0 is on.

## ◆ trotec()

void IRac::trotec | ( | IRTrotecESP * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Trotec A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRTrotecESP object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ trotec3550()

void IRac::trotec3550 | ( | IRTrotec3550 * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const bool | celsius,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv
| ) |  |
| private

Send a Trotec 3550 A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRTrotecESP object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | celsius | Temperature units. True is Celsius, False is Fahrenheit.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.

## ◆ truma()

void IRac::truma | ( | IRTrumaAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const bool | quiet
| ) |  |
| private

Send a Truma A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRTrumaAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | quiet | Run the device quietly if we can.

## ◆ vestel()

void IRac::vestel | ( | IRVestelAc * | ac,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | filter,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`,
|  | const bool | sendNormal = `true`
| ) |  |
| private

Send a Vestel A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRVestelAc object to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | filter | Turn on the (ion/pollen/etc) filter mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.
  [in] | sendNormal | Do we send a Normal settings message at all? i.e In addition to the clock/time/timer message

## ◆ voltas()

void IRac::voltas | ( | IRVoltas * | ac,
|  | const voltas_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const stdAc::swingh_t | swingh,
|  | const bool | turbo,
|  | const bool | econo,
|  | const bool | light,
|  | const int16_t | sleep = `-1`
| ) |  |
| private

Send a Voltas A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRVoltas object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | swingh | The horizontal swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | econo | Run the device in economical mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.

## ◆ whirlpool()

void IRac::whirlpool | ( | IRWhirlpoolAc * | ac,
|  | const whirlpool_ac_remote_model_t | model,
|  | const bool | on,
|  | const stdAc::opmode_t | mode,
|  | const float | degrees,
|  | const stdAc::fanspeed_t | fan,
|  | const stdAc::swingv_t | swingv,
|  | const bool | turbo,
|  | const bool | light,
|  | const int16_t | sleep = `-1`,
|  | const int16_t | clock = `-1`
| ) |  |
| private

Send a Whirlpool A/C message with the supplied settings.

Parameters

  [in,out] | ac | A Ptr to an IRWhirlpoolAc object to use.
  [in] | model | The A/C model to use.
  [in] | on | The power setting.
  [in] | mode | The operation mode setting.
  [in] | degrees | The temperature setting in degrees.
  [in] | fan | The speed setting for the fan.
  [in] | swingv | The vertical swing setting.
  [in] | turbo | Run the device in turbo/powerful mode.
  [in] | light | Turn on the LED/Display mode.
  [in] | sleep | Nr. of minutes for sleep mode. -1 is Off, >= 0 is on.
  [in] | clock | The time in Nr. of mins since midnight. < 0 is ignore.

## Member Data Documentation

## ◆ _inverted

bool IRac::_inverted
| private

IR LED is lit when GPIO is LOW (true) or HIGH (false)?

## ◆ _modulation

bool IRac::_modulation
| private

Is frequency modulation to be used?

## ◆ _pin

uint16_t IRac::_pin
| private

The GPIO to use to transmit messages from.

## ◆ _prev

stdAc::state_t IRac::_prev
| private

The state we expect the device to currently be in.

## ◆ next

stdAc::state_t IRac::next

The state we want the device to be in after we send.

The documentation for this class was generated from the following files:

- src/IRac.h
- src/IRac.cpp