IRremoteESP8266

Variables
ir_NEC.h File Reference

Support for NEC (Renesas) protocols. NEC originally added from https://github.com/shirriff/Arduino-IRremote/. More...

Go to the source code of this file.

## Variables
const uint16_t | kNecTick = 560
const uint16_t | kNecHdrMarkTicks = 16
const uint16_t | kNecHdrMark = kNecHdrMarkTicks * kNecTick
const uint16_t | kNecHdrSpaceTicks = 8
const uint16_t | kNecHdrSpace = kNecHdrSpaceTicks * kNecTick
const uint16_t | kNecBitMarkTicks = 1
const uint16_t | kNecBitMark = kNecBitMarkTicks * kNecTick
const uint16_t | kNecOneSpaceTicks = 3
const uint16_t | kNecOneSpace = kNecOneSpaceTicks * kNecTick
const uint16_t | kNecZeroSpaceTicks = 1
const uint16_t | kNecZeroSpace = kNecZeroSpaceTicks * kNecTick
const uint16_t | kNecRptSpaceTicks = 4
const uint16_t | kNecRptSpace = kNecRptSpaceTicks * kNecTick
const uint16_t | kNecRptLength = 4
const uint16_t | kNecMinCommandLengthTicks = 193
const uint32_t | kNecMinCommandLength = kNecMinCommandLengthTicks * kNecTick
const uint32_t | kNecMinGap
const uint16_t | kNecMinGapTicks
const uint32_t | kAlokaPower = 0xFF609F
const uint32_t | kAlokaLedWhite = 0xFF906F
const uint32_t | kAlokaLedGreen = 0xFF9867
const uint32_t | kAlokaLedBlue = 0xFFD827
const uint32_t | kAlokaLedPinkRed = 0xFF8877
const uint32_t | kAlokaLedRed = 0xFFA857
const uint32_t | kAlokaLedLightGreen = 0xFFE817
const uint32_t | kAlokaLedMidBlue = 0xFF48B7
const uint32_t | kAlokaLedPink = 0xFF6897
const uint32_t | kAlokaLedOrange = 0xFFB24D
const uint32_t | kAlokaLedYellow = 0xFF00FF
const uint32_t | kAlokaNightFade = 0xFF50AF
const uint32_t | kAlokaNightTimer = 0xFF7887
const uint32_t | kAlokaLedRainbow = 0xFF708F
const uint32_t | kAlokaLedTreeGrow = 0xFF58A7

## Detailed Description

Support for NEC (Renesas) protocols. NEC originally added from https://github.com/shirriff/Arduino-IRremote/.

See also
  http://www.sbprojects.net/knowledge/ir/nec.php

## Variable Documentation

## ◆ kAlokaLedBlue

const uint32_t kAlokaLedBlue = 0xFFD827

## ◆ kAlokaLedGreen

const uint32_t kAlokaLedGreen = 0xFF9867

## ◆ kAlokaLedLightGreen

const uint32_t kAlokaLedLightGreen = 0xFFE817

## ◆ kAlokaLedMidBlue

const uint32_t kAlokaLedMidBlue = 0xFF48B7

## ◆ kAlokaLedOrange

const uint32_t kAlokaLedOrange = 0xFFB24D

## ◆ kAlokaLedPink

const uint32_t kAlokaLedPink = 0xFF6897

## ◆ kAlokaLedPinkRed

const uint32_t kAlokaLedPinkRed = 0xFF8877

## ◆ kAlokaLedRainbow

const uint32_t kAlokaLedRainbow = 0xFF708F

## ◆ kAlokaLedRed

const uint32_t kAlokaLedRed = 0xFFA857

## ◆ kAlokaLedTreeGrow

const uint32_t kAlokaLedTreeGrow = 0xFF58A7

## ◆ kAlokaLedWhite

const uint32_t kAlokaLedWhite = 0xFF906F

## ◆ kAlokaLedYellow

const uint32_t kAlokaLedYellow = 0xFF00FF

## ◆ kAlokaNightFade

const uint32_t kAlokaNightFade = 0xFF50AF

## ◆ kAlokaNightTimer

const uint32_t kAlokaNightTimer = 0xFF7887

## ◆ kAlokaPower

const uint32_t kAlokaPower = 0xFF609F

## ◆ kNecBitMark

const uint16_t kNecBitMark = kNecBitMarkTicks * kNecTick

## ◆ kNecBitMarkTicks

const uint16_t kNecBitMarkTicks = 1

## ◆ kNecHdrMark

const uint16_t kNecHdrMark = kNecHdrMarkTicks * kNecTick

## ◆ kNecHdrMarkTicks

const uint16_t kNecHdrMarkTicks = 16

## ◆ kNecHdrSpace

const uint16_t kNecHdrSpace = kNecHdrSpaceTicks * kNecTick

## ◆ kNecHdrSpaceTicks

const uint16_t kNecHdrSpaceTicks = 8

## ◆ kNecMinCommandLength

const uint32_t kNecMinCommandLength = kNecMinCommandLengthTicks * kNecTick

## ◆ kNecMinCommandLengthTicks

const uint16_t kNecMinCommandLengthTicks = 193

## ◆ kNecMinGap

const uint32_t kNecMinGap

Initial value:
=
kNecMinCommandLength -
(kNecHdrMark + kNecHdrSpace + kNECBits * (kNecBitMark + kNecOneSpace) +
kNecBitMark)

## ◆ kNecMinGapTicks

const uint16_t kNecMinGapTicks

Initial value:
=
kNecMinCommandLengthTicks -
(kNecHdrMarkTicks + kNecHdrSpaceTicks +
kNECBits * (kNecBitMarkTicks + kNecOneSpaceTicks) + kNecBitMarkTicks)

## ◆ kNecOneSpace

const uint16_t kNecOneSpace = kNecOneSpaceTicks * kNecTick

## ◆ kNecOneSpaceTicks

const uint16_t kNecOneSpaceTicks = 3

## ◆ kNecRptLength

const uint16_t kNecRptLength = 4

## ◆ kNecRptSpace

const uint16_t kNecRptSpace = kNecRptSpaceTicks * kNecTick

## ◆ kNecRptSpaceTicks

const uint16_t kNecRptSpaceTicks = 4

## ◆ kNecTick

const uint16_t kNecTick = 560

## ◆ kNecZeroSpace

const uint16_t kNecZeroSpace = kNecZeroSpaceTicks * kNecTick

## ◆ kNecZeroSpaceTicks

const uint16_t kNecZeroSpaceTicks = 1

kNecBitMarkTicks
const uint16_t kNecBitMarkTicks
Definition: ir_NEC.h:32
kNecHdrSpace
const uint16_t kNecHdrSpace
Definition: ir_NEC.h:31
kNecBitMark
const uint16_t kNecBitMark
Definition: ir_NEC.h:33
kNecMinCommandLength
const uint32_t kNecMinCommandLength
Definition: ir_NEC.h:42
kNecOneSpace
const uint16_t kNecOneSpace
Definition: ir_NEC.h:35
kNecMinCommandLengthTicks
const uint16_t kNecMinCommandLengthTicks
Definition: ir_NEC.h:41
kNecOneSpaceTicks
const uint16_t kNecOneSpaceTicks
Definition: ir_NEC.h:34
kNecHdrMarkTicks
const uint16_t kNecHdrMarkTicks
Definition: ir_NEC.h:28
kNECBits
const uint16_t kNECBits
Definition: IRremoteESP8266.h:1332
kNecHdrMark
const uint16_t kNecHdrMark
Definition: ir_NEC.h:29
kNecHdrSpaceTicks
const uint16_t kNecHdrSpaceTicks
Definition: ir_NEC.h:30