IRremoteESP8266

IRDaikin176 Member List

This is the complete list of members for IRDaikin176, including all inherited members.

_ | IRDaikin176 | private
_irsend | IRDaikin176 | private
_saved_temp | IRDaikin176 | private
begin(void) | IRDaikin176 |
calibrate(void) | IRDaikin176 | inline
checksum(void) | IRDaikin176 | private
convertFan(const stdAc::fanspeed_t speed) | IRDaikin176 | static
convertMode(const stdAc::opmode_t mode) | IRDaikin176 | static
convertSwingH(const stdAc::swingh_t position) | IRDaikin176 | static
getFan(void) const | IRDaikin176 |
getId(void) const | IRDaikin176 |
getMode(void) const | IRDaikin176 |
getPower(void) const | IRDaikin176 |
getRaw(void) | IRDaikin176 |
getSwingHorizontal(void) const | IRDaikin176 |
getTemp(void) const | IRDaikin176 |
IRDaikin176(const uint16_t pin, const bool inverted=false, const bool use_modulation=true) | IRDaikin176 | explicit
off(void) | IRDaikin176 |
on(void) | IRDaikin176 |
send(const uint16_t repeat=kDaikin176DefaultRepeat) | IRDaikin176 |
setFan(const uint8_t fan) | IRDaikin176 |
setId(const uint8_t num) | IRDaikin176 |
setMode(const uint8_t mode) | IRDaikin176 |
setPower(const bool on) | IRDaikin176 |
setRaw(const uint8_t new_code[]) | IRDaikin176 |
setSwingHorizontal(const uint8_t position) | IRDaikin176 |
setTemp(const uint8_t temp) | IRDaikin176 |
stateReset(void) | IRDaikin176 | private
toCommon(void) const | IRDaikin176 |
toCommonFanSpeed(const uint8_t speed) | IRDaikin176 | static
toCommonMode(const uint8_t mode) | IRDaikin176 | static
toCommonSwingH(const uint8_t setting) | IRDaikin176 | static
toString(void) const | IRDaikin176 |
validChecksum(uint8_t state[], const uint16_t length=kDaikin176StateLength) | IRDaikin176 | static