IRremoteESP8266

Public Attributes | List of all members
TranscoldProtocol Union Reference

Native representation of a Transcold A/C message. More...

`#include <ir_Transcold.h>`

## Public Attributes
uint32_t | raw
| The state of the IR remote in IR code form. More...
struct {
uint8_t __pad0__:8
uint8_t Temp:4
uint8_t Mode:4
uint8_t Fan:4
uint8_t __pad1__:4
uint8_t __pad2__:8
}; |

## Detailed Description

Native representation of a Transcold A/C message.

## Member Data Documentation

## ◆ @120

struct { ... }

## ◆ __pad0__

uint8_t TranscoldProtocol::__pad0__

## ◆ __pad1__

uint8_t TranscoldProtocol::__pad1__

## ◆ __pad2__

uint8_t TranscoldProtocol::__pad2__

## ◆ Fan

uint8_t TranscoldProtocol::Fan

## ◆ Mode

uint8_t TranscoldProtocol::Mode

## ◆ raw

uint32_t TranscoldProtocol::raw

The state of the IR remote in IR code form.

## ◆ Temp

uint8_t TranscoldProtocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Transcold.h