IRremoteESP8266

Classes | Variables
ir_Corona.h File Reference

Go to the source code of this file.

## Classes
struct | CoronaSection
| Native representation of a section of a Corona A/C message. More...
union | CoronaProtocol
| Native representation of a Corona A/C message. More...
class | IRCoronaAc
| Class for handling detailed Corona A/C messages. More...

## Variables
const uint8_t | kCoronaAcSections = 3
const uint8_t | kCoronaAcSectionBytes = 7
const uint8_t | kCoronaAcSectionHeader0 = 0x28
const uint8_t | kCoronaAcSectionHeader1 = 0x61
const uint8_t | kCoronaAcSectionLabelBase = 0x0D
const uint8_t | kCoronaAcSectionData0Base = 0x10
const uint8_t | kCoronaAcFanAuto = 0b00
const uint8_t | kCoronaAcFanLow = 0b01
const uint8_t | kCoronaAcFanMedium = 0b10
const uint8_t | kCoronaAcFanHigh = 0b11
const uint8_t | kCoronaAcMinTemp = 17
const uint8_t | kCoronaAcMaxTemp = 30
const uint8_t | kCoronaAcModeHeat = 0b00
const uint8_t | kCoronaAcModeDry = 0b01
const uint8_t | kCoronaAcModeCool = 0b10
const uint8_t | kCoronaAcModeFan = 0b11
const uint8_t | kCoronaAcSettingsSection = 0
const uint8_t | kCoronaAcOnTimerSection = 1
const uint8_t | kCoronaAcOffTimerSection = 2
const uint16_t | kCoronaAcTimerMax = 12 * 60
const uint16_t | kCoronaAcTimerOff = 0xffff
const uint16_t | kCoronaAcTimerUnitsPerMin = 30

## Variable Documentation

## ◆ kCoronaAcFanAuto

const uint8_t kCoronaAcFanAuto = 0b00

## ◆ kCoronaAcFanHigh

const uint8_t kCoronaAcFanHigh = 0b11

## ◆ kCoronaAcFanLow

const uint8_t kCoronaAcFanLow = 0b01

## ◆ kCoronaAcFanMedium

const uint8_t kCoronaAcFanMedium = 0b10

## ◆ kCoronaAcMaxTemp

const uint8_t kCoronaAcMaxTemp = 30

## ◆ kCoronaAcMinTemp

const uint8_t kCoronaAcMinTemp = 17

## ◆ kCoronaAcModeCool

const uint8_t kCoronaAcModeCool = 0b10

## ◆ kCoronaAcModeDry

const uint8_t kCoronaAcModeDry = 0b01

## ◆ kCoronaAcModeFan

const uint8_t kCoronaAcModeFan = 0b11

## ◆ kCoronaAcModeHeat

const uint8_t kCoronaAcModeHeat = 0b00

## ◆ kCoronaAcOffTimerSection

const uint8_t kCoronaAcOffTimerSection = 2

## ◆ kCoronaAcOnTimerSection

const uint8_t kCoronaAcOnTimerSection = 1

## ◆ kCoronaAcSectionBytes

const uint8_t kCoronaAcSectionBytes = 7

## ◆ kCoronaAcSectionData0Base

const uint8_t kCoronaAcSectionData0Base = 0x10

## ◆ kCoronaAcSectionHeader0

const uint8_t kCoronaAcSectionHeader0 = 0x28

## ◆ kCoronaAcSectionHeader1

const uint8_t kCoronaAcSectionHeader1 = 0x61

## ◆ kCoronaAcSectionLabelBase

const uint8_t kCoronaAcSectionLabelBase = 0x0D

## ◆ kCoronaAcSections

const uint8_t kCoronaAcSections = 3

## ◆ kCoronaAcSettingsSection

const uint8_t kCoronaAcSettingsSection = 0

## ◆ kCoronaAcTimerMax

const uint16_t kCoronaAcTimerMax = 12 * 60

## ◆ kCoronaAcTimerOff

const uint16_t kCoronaAcTimerOff = 0xffff

## ◆ kCoronaAcTimerUnitsPerMin

const uint16_t kCoronaAcTimerUnitsPerMin = 30