IRremoteESP8266

Public Attributes | List of all members
TrumaProtocol Union Reference

Native representation of a Truma A/C message. More...

`#include <ir_Truma.h>`

## Public Attributes
uint64_t | raw
| Remote state in IR code form. More...
struct {
uint8_t __pad0__:8
uint8_t Mode:2
uint8_t PowerOff:1
uint8_t Fan:3
uint8_t __pad1__:2
uint8_t Temp:5
| Temp in DegC minus 10(DEC). More...
uint8_t __pad2__:3
uint8_t __pad3__:8
uint8_t __pad4__:8
uint8_t __pad5__:8
uint8_t Sum:8
| Checksum value. More...
}; |

## Detailed Description

Native representation of a Truma A/C message.

## Member Data Documentation

## ◆ @126

struct { ... }

## ◆ __pad0__

uint8_t TrumaProtocol::__pad0__

## ◆ __pad1__

uint8_t TrumaProtocol::__pad1__

## ◆ __pad2__

uint8_t TrumaProtocol::__pad2__

## ◆ __pad3__

uint8_t TrumaProtocol::__pad3__

## ◆ __pad4__

uint8_t TrumaProtocol::__pad4__

## ◆ __pad5__

uint8_t TrumaProtocol::__pad5__

## ◆ Fan

uint8_t TrumaProtocol::Fan

## ◆ Mode

uint8_t TrumaProtocol::Mode

## ◆ PowerOff

uint8_t TrumaProtocol::PowerOff

## ◆ raw

uint64_t TrumaProtocol::raw

Remote state in IR code form.

## ◆ Sum

uint8_t TrumaProtocol::Sum

Checksum value.

## ◆ Temp

uint8_t TrumaProtocol::Temp

Temp in DegC minus 10(DEC).

The documentation for this union was generated from the following file:

- src/ir_Truma.h