IRremoteESP8266

Variables
ir_Bose.cpp File Reference

Support for Bose protocols. More...

## Variables
const uint16_t | kBoseHdrMark = 1100
const uint16_t | kBoseHdrSpace = 1350
const uint16_t | kBoseBitMark = 555
const uint16_t | kBoseOneSpace = 1435
const uint16_t | kBoseZeroSpace = 500
const uint32_t | kBoseGap = kDefaultMessageGap
const uint16_t | kBoseFreq = 38

## Detailed Description

Support for Bose protocols.

Note
  Currently only tested against Bose TV Speaker.

See also
  https://github.com/crankyoldgit/IRremoteESP8266/pull/1579

## Variable Documentation

## ◆ kBoseBitMark

const uint16_t kBoseBitMark = 555

## ◆ kBoseFreq

const uint16_t kBoseFreq = 38

## ◆ kBoseGap

const uint32_t kBoseGap = kDefaultMessageGap

## ◆ kBoseHdrMark

const uint16_t kBoseHdrMark = 1100

## ◆ kBoseHdrSpace

const uint16_t kBoseHdrSpace = 1350

## ◆ kBoseOneSpace

const uint16_t kBoseOneSpace = 1435

## ◆ kBoseZeroSpace

const uint16_t kBoseZeroSpace = 500