IRremoteESP8266

Public Attributes | List of all members
Daikin64Protocol Union Reference

Native representation of a Daikin64 A/C message. More...

`#include <ir_Daikin.h>`

## Public Attributes
uint64_t | raw
| The state of the IR remote. More...
struct {
uint8_t __pad0__:8
uint8_t Mode:4
uint8_t Fan:4
uint8_t ClockMins:8
uint8_t ClockHours:8
uint8_t OnHours:6
uint8_t OnHalfHour:1
uint8_t OnTimer:1
uint8_t OffHours:6
uint8_t OffHalfHour:1
uint8_t OffTimer:1
uint8_t Temp:8
uint8_t SwingV:1
uint8_t Sleep:1
uint8_t __pad1__:1
uint8_t Power:1
uint8_t Sum:4
}; |

## Detailed Description

Native representation of a Daikin64 A/C message.

## Member Data Documentation

## ◆ @39

struct { ... }

## ◆ __pad0__

uint8_t Daikin64Protocol::__pad0__

## ◆ __pad1__

uint8_t Daikin64Protocol::__pad1__

## ◆ ClockHours

uint8_t Daikin64Protocol::ClockHours

## ◆ ClockMins

uint8_t Daikin64Protocol::ClockMins

## ◆ Fan

uint8_t Daikin64Protocol::Fan

## ◆ Mode

uint8_t Daikin64Protocol::Mode

## ◆ OffHalfHour

uint8_t Daikin64Protocol::OffHalfHour

## ◆ OffHours

uint8_t Daikin64Protocol::OffHours

## ◆ OffTimer

uint8_t Daikin64Protocol::OffTimer

## ◆ OnHalfHour

uint8_t Daikin64Protocol::OnHalfHour

## ◆ OnHours

uint8_t Daikin64Protocol::OnHours

## ◆ OnTimer

uint8_t Daikin64Protocol::OnTimer

## ◆ Power

uint8_t Daikin64Protocol::Power

## ◆ raw

uint64_t Daikin64Protocol::raw

The state of the IR remote.

## ◆ Sleep

uint8_t Daikin64Protocol::Sleep

## ◆ Sum

uint8_t Daikin64Protocol::Sum

## ◆ SwingV

uint8_t Daikin64Protocol::SwingV

## ◆ Temp

uint8_t Daikin64Protocol::Temp

The documentation for this union was generated from the following file:

- src/ir_Daikin.h