IRremoteESP8266

Public Attributes | List of all members
YorkProtocol Union Reference

Native representation of a York A/C message. More...

`#include <ir_York.h>`

## Public Attributes
uint8_t | raw [kYorkStateLength]
| The state of the IR remote. More...
struct {
uint8_t preamble [6]
uint8_t Key1:4
uint8_t Key2:4
uint8_t Fan:4
uint8_t Power:1
uint8_t __pad0__:3
uint8_t Mode:4
uint8_t __pad1__:4
uint8_t __pad2__:2
uint8_t Temp:6
uint8_t OffTimer:8
uint8_t OnTimer:8
uint8_t __pad3__:8
uint8_t SwingV:1
uint8_t __pad4__:7
uint8_t __pad5__:8
uint8_t Chk1:8
uint8_t Chk2:8
}; |

## Detailed Description

Native representation of a York A/C message.

## Member Data Documentation

## ◆ @136

struct { ... }

## ◆ __pad0__

uint8_t YorkProtocol::__pad0__

## ◆ __pad1__

uint8_t YorkProtocol::__pad1__

## ◆ __pad2__

uint8_t YorkProtocol::__pad2__

## ◆ __pad3__

uint8_t YorkProtocol::__pad3__

## ◆ __pad4__

uint8_t YorkProtocol::__pad4__

## ◆ __pad5__

uint8_t YorkProtocol::__pad5__

## ◆ Chk1

uint8_t YorkProtocol::Chk1

## ◆ Chk2

uint8_t YorkProtocol::Chk2

## ◆ Fan

uint8_t YorkProtocol::Fan

## ◆ Key1

uint8_t YorkProtocol::Key1

## ◆ Key2

uint8_t YorkProtocol::Key2

## ◆ Mode

uint8_t YorkProtocol::Mode

## ◆ OffTimer

uint8_t YorkProtocol::OffTimer

## ◆ OnTimer

uint8_t YorkProtocol::OnTimer

## ◆ Power

uint8_t YorkProtocol::Power

## ◆ preamble

uint8_t YorkProtocol::preamble[6]

## ◆ raw

uint8_t YorkProtocol::raw[kYorkStateLength]

The state of the IR remote.

## ◆ SwingV

uint8_t YorkProtocol::SwingV

## ◆ Temp

uint8_t YorkProtocol::Temp

The documentation for this union was generated from the following file:

- src/ir_York.h